Next: Nios II Features, Previous: MIPS Features, Up: Standard Target Features

#### G.4.5 M68K Features

`‘``org.gnu.gdb.m68k.core``’`
`‘``org.gnu.gdb.coldfire.core``’`
`‘``org.gnu.gdb.fido.core``’`
  One of those features must be always present. The feature that is present determines which flavor of m68k is used. The feature that is present should contain registers ‘`d0`’ through ‘`d7`’, ‘`a0`’ through ‘`a5`’, ‘`fp`’, ‘`sp`’, ‘`ps`’ and ‘`pc`’.
`‘``org.gnu.gdb.coldfire.fp``’`
  This feature is optional. If present, it should contain registers ‘`fp0`’ through ‘`fp7`’, ‘`fpcontrol`’, ‘`fpstatus`’ and ‘`fpiaddr`’.