Version|0.2
Log Level|4
Debug Print|Y
Available Target List|mobile|wearable
Selected Target|mobile
Default Feature List|2|3|103
Total Overhead Range|1000000|3000000|7000000|15000000
Options Selected Feature List|5002:0
Selected Preferences|2001
mobile|Protocol Version|4.0
mobile|Available Template List|1|2|3|4|5|6|7|8|9|10|11
mobile|Selected Template|1
mobile|Available Feature List|1|1000|4|5|6|7|8|9|100|101|1001|301|200|201|202|203|204|206
mobile|Available FlatFeature List|101|102|103|201|202|203|301|302|401|501|502|601|602|603|701|801|802
mobile|Selected Feature List|1|5|1000:1000|100|101|1001:10
mobile|Selected FlatFeature List|
mobile|Available Chart List|CPU Usage|Core Usage|Core Frequency|System Memory|Process Memory|Heap Allocation|Screenshot|UI Event|Disk IO|Network IO|Peripheral Status|Power Estimation
wearable|Protocol Version|3.0
wearable|Available Template List|1|2|3|4|5|6|7|8|9|10|11
wearable|Selected Template|1
wearable|Available Feature List|1|1000|4|5|6|7|8|9|100|101|1001|301|200|201|202|203|204|206
wearable|Available FlatFeature List|101|102|103|201|202|203|301|302|401|501|502|601|602|603|701|801|802
wearable|Selected Feature List|1|5|1000:1000|100|101|1001:10
wearable|Selected FlatFeature List|
wearable|Available Chart List|CPU Usage|Core Usage|Core Frequency|System Memory|Process Memory|Heap Allocation|Screenshot|UI Event|Disk IO|Network IO|Peripheral Status|Power Estimation
tv|Protocol Version|3.0
tv|Available Template List|1|2|3|4|5|6|7|8|10
tv|Selected Template|1
tv|Available Feature List|1|1000|4|5|6|7|100|101|1001|102|200|201|202|203
tv|Available FlatFeature List|101|102|103|201|202|203|301|302|401|501|502|601|602|603|701|801|802
tv|Selected Feature List|1|5|1000:1000|100|101|1001:10
tv|Available Chart List|CPU|CPU core|CPU frequency|Heap allocation|Process Size|Memory|Screenshot|Disk IO|Network IO
