class Elm.Atspi_Bridge (Eo.Base)
{
   eo_prefix: elm_obj_atspi_bridge;
   methods {
      @property connected {
         get {
            [[Indicate if connection with AT-SPI2 bus has been established.

              \@internal
              \@if MOBILE \@since_tizen 3.0
              \@elseif WEARABLE \@since_tizen 3.0
              \@endif
            ]]
            values {
               ret: bool;
            }
         }
      }
      @property root {
         get {
            [[Get root object of accessible object hierarchy

              \@internal
            ]]
            values {
               ret: Eo*;
            }
         }
      }
   }
   implements {
      Eo.Base.constructor;
      Eo.Base.destructor;
   }
   events {
      connected;
      disconnected;
   }
}
