Next: ARM ACLE Intrinsics, Previous: ARM iWMMXt Built-in Functions, Up: Target Builtins

#### 6.57.6 ARM NEON Intrinsics

These built-in intrinsics for the ARM Advanced SIMD extension are available when the `-mfpu=neon` switch is used:

##### 6.57.6.1 Addition

- uint32x2_t vadd_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vadd.i32` d0`,` d0`,` d0

- uint16x4_t vadd_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vadd.i16` d0`,` d0`,` d0

- uint8x8_t vadd_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vadd.i8` d0`,` d0`,` d0

- int32x2_t vadd_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vadd.i32` d0`,` d0`,` d0

- int16x4_t vadd_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vadd.i16` d0`,` d0`,` d0

- int8x8_t vadd_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vadd.i8` d0`,` d0`,` d0

- float32x2_t vadd_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vadd.f32` d0`,` d0`,` d0

- uint64x1_t vadd_u64 (uint64x1_t, uint64x1_t)

- int64x1_t vadd_s64 (int64x1_t, int64x1_t)

- uint32x4_t vaddq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vadd.i32` q0`,` q0`,` q0

- uint16x8_t vaddq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vadd.i16` q0`,` q0`,` q0

- uint8x16_t vaddq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vadd.i8` q0`,` q0`,` q0

- int32x4_t vaddq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vadd.i32` q0`,` q0`,` q0

- int16x8_t vaddq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vadd.i16` q0`,` q0`,` q0

- int8x16_t vaddq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vadd.i8` q0`,` q0`,` q0

- uint64x2_t vaddq_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vadd.i64` q0`,` q0`,` q0

- int64x2_t vaddq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vadd.i64` q0`,` q0`,` q0

- float32x4_t vaddq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vadd.f32` q0`,` q0`,` q0

- uint64x2_t vaddl_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vaddl.u32` q0`,` d0`,` d0

- uint32x4_t vaddl_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vaddl.u16` q0`,` d0`,` d0

- uint16x8_t vaddl_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vaddl.u8` q0`,` d0`,` d0

- int64x2_t vaddl_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vaddl.s32` q0`,` d0`,` d0

- int32x4_t vaddl_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vaddl.s16` q0`,` d0`,` d0

- int16x8_t vaddl_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vaddl.s8` q0`,` d0`,` d0

- uint64x2_t vaddw_u32 (uint64x2_t, uint32x2_t)
  Form of expected instruction(s): `vaddw.u32` q0`,` q0`,` d0

- uint32x4_t vaddw_u16 (uint32x4_t, uint16x4_t)
  Form of expected instruction(s): `vaddw.u16` q0`,` q0`,` d0

- uint16x8_t vaddw_u8 (uint16x8_t, uint8x8_t)
  Form of expected instruction(s): `vaddw.u8` q0`,` q0`,` d0

- int64x2_t vaddw_s32 (int64x2_t, int32x2_t)
  Form of expected instruction(s): `vaddw.s32` q0`,` q0`,` d0

- int32x4_t vaddw_s16 (int32x4_t, int16x4_t)
  Form of expected instruction(s): `vaddw.s16` q0`,` q0`,` d0

- int16x8_t vaddw_s8 (int16x8_t, int8x8_t)
  Form of expected instruction(s): `vaddw.s8` q0`,` q0`,` d0

- uint32x2_t vhadd_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vhadd.u32` d0`,` d0`,` d0

- uint16x4_t vhadd_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vhadd.u16` d0`,` d0`,` d0

- uint8x8_t vhadd_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vhadd.u8` d0`,` d0`,` d0

- int32x2_t vhadd_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vhadd.s32` d0`,` d0`,` d0

- int16x4_t vhadd_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vhadd.s16` d0`,` d0`,` d0

- int8x8_t vhadd_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vhadd.s8` d0`,` d0`,` d0

- uint32x4_t vhaddq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vhadd.u32` q0`,` q0`,` q0

- uint16x8_t vhaddq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vhadd.u16` q0`,` q0`,` q0

- uint8x16_t vhaddq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vhadd.u8` q0`,` q0`,` q0

- int32x4_t vhaddq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vhadd.s32` q0`,` q0`,` q0

- int16x8_t vhaddq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vhadd.s16` q0`,` q0`,` q0

- int8x16_t vhaddq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vhadd.s8` q0`,` q0`,` q0

- uint32x2_t vrhadd_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vrhadd.u32` d0`,` d0`,` d0

- uint16x4_t vrhadd_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vrhadd.u16` d0`,` d0`,` d0

- uint8x8_t vrhadd_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vrhadd.u8` d0`,` d0`,` d0

- int32x2_t vrhadd_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vrhadd.s32` d0`,` d0`,` d0

- int16x4_t vrhadd_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vrhadd.s16` d0`,` d0`,` d0

- int8x8_t vrhadd_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vrhadd.s8` d0`,` d0`,` d0

- uint32x4_t vrhaddq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vrhadd.u32` q0`,` q0`,` q0

- uint16x8_t vrhaddq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vrhadd.u16` q0`,` q0`,` q0

- uint8x16_t vrhaddq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vrhadd.u8` q0`,` q0`,` q0

- int32x4_t vrhaddq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vrhadd.s32` q0`,` q0`,` q0

- int16x8_t vrhaddq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vrhadd.s16` q0`,` q0`,` q0

- int8x16_t vrhaddq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vrhadd.s8` q0`,` q0`,` q0

- uint32x2_t vqadd_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vqadd.u32` d0`,` d0`,` d0

- uint16x4_t vqadd_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vqadd.u16` d0`,` d0`,` d0

- uint8x8_t vqadd_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vqadd.u8` d0`,` d0`,` d0

- int32x2_t vqadd_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vqadd.s32` d0`,` d0`,` d0

- int16x4_t vqadd_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vqadd.s16` d0`,` d0`,` d0

- int8x8_t vqadd_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vqadd.s8` d0`,` d0`,` d0

- uint64x1_t vqadd_u64 (uint64x1_t, uint64x1_t)
  Form of expected instruction(s): `vqadd.u64` d0`,` d0`,` d0

- int64x1_t vqadd_s64 (int64x1_t, int64x1_t)
  Form of expected instruction(s): `vqadd.s64` d0`,` d0`,` d0

- uint32x4_t vqaddq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vqadd.u32` q0`,` q0`,` q0

- uint16x8_t vqaddq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vqadd.u16` q0`,` q0`,` q0

- uint8x16_t vqaddq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vqadd.u8` q0`,` q0`,` q0

- int32x4_t vqaddq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vqadd.s32` q0`,` q0`,` q0

- int16x8_t vqaddq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vqadd.s16` q0`,` q0`,` q0

- int8x16_t vqaddq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vqadd.s8` q0`,` q0`,` q0

- uint64x2_t vqaddq_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vqadd.u64` q0`,` q0`,` q0

- int64x2_t vqaddq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vqadd.s64` q0`,` q0`,` q0

- uint32x2_t vaddhn_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vaddhn.i64` d0`,` q0`,` q0

- uint16x4_t vaddhn_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vaddhn.i32` d0`,` q0`,` q0

- uint8x8_t vaddhn_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vaddhn.i16` d0`,` q0`,` q0

- int32x2_t vaddhn_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vaddhn.i64` d0`,` q0`,` q0

- int16x4_t vaddhn_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vaddhn.i32` d0`,` q0`,` q0

- int8x8_t vaddhn_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vaddhn.i16` d0`,` q0`,` q0

- uint32x2_t vraddhn_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vraddhn.i64` d0`,` q0`,` q0

- uint16x4_t vraddhn_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vraddhn.i32` d0`,` q0`,` q0

- uint8x8_t vraddhn_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vraddhn.i16` d0`,` q0`,` q0

- int32x2_t vraddhn_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vraddhn.i64` d0`,` q0`,` q0

- int16x4_t vraddhn_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vraddhn.i32` d0`,` q0`,` q0

- int8x8_t vraddhn_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vraddhn.i16` d0`,` q0`,` q0

##### 6.57.6.2 Multiplication

- uint32x2_t vmul_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vmul.i32` d0`,` d0`,` d0

- uint16x4_t vmul_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vmul.i16` d0`,` d0`,` d0

- uint8x8_t vmul_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vmul.i8` d0`,` d0`,` d0

- int32x2_t vmul_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vmul.i32` d0`,` d0`,` d0

- int16x4_t vmul_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vmul.i16` d0`,` d0`,` d0

- int8x8_t vmul_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vmul.i8` d0`,` d0`,` d0

- float32x2_t vmul_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vmul.f32` d0`,` d0`,` d0

- poly8x8_t vmul_p8 (poly8x8_t, poly8x8_t)
  Form of expected instruction(s): `vmul.p8` d0`,` d0`,` d0

- uint32x4_t vmulq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vmul.i32` q0`,` q0`,` q0

- uint16x8_t vmulq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vmul.i16` q0`,` q0`,` q0

- uint8x16_t vmulq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vmul.i8` q0`,` q0`,` q0

- int32x4_t vmulq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vmul.i32` q0`,` q0`,` q0

- int16x8_t vmulq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vmul.i16` q0`,` q0`,` q0

- int8x16_t vmulq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vmul.i8` q0`,` q0`,` q0

- float32x4_t vmulq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vmul.f32` q0`,` q0`,` q0

- poly8x16_t vmulq_p8 (poly8x16_t, poly8x16_t)
  Form of expected instruction(s): `vmul.p8` q0`,` q0`,` q0

- int32x2_t vqdmulh_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vqdmulh.s32` d0`,` d0`,` d0

- int16x4_t vqdmulh_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vqdmulh.s16` d0`,` d0`,` d0

- int32x4_t vqdmulhq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vqdmulh.s32` q0`,` q0`,` q0

- int16x8_t vqdmulhq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vqdmulh.s16` q0`,` q0`,` q0

- int32x2_t vqrdmulh_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vqrdmulh.s32` d0`,` d0`,` d0

- int16x4_t vqrdmulh_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vqrdmulh.s16` d0`,` d0`,` d0

- int32x4_t vqrdmulhq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vqrdmulh.s32` q0`,` q0`,` q0

- int16x8_t vqrdmulhq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vqrdmulh.s16` q0`,` q0`,` q0

- uint64x2_t vmull_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vmull.u32` q0`,` d0`,` d0

- uint32x4_t vmull_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vmull.u16` q0`,` d0`,` d0

- uint16x8_t vmull_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vmull.u8` q0`,` d0`,` d0

- int64x2_t vmull_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vmull.s32` q0`,` d0`,` d0

- int32x4_t vmull_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vmull.s16` q0`,` d0`,` d0

- int16x8_t vmull_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vmull.s8` q0`,` d0`,` d0

- poly16x8_t vmull_p8 (poly8x8_t, poly8x8_t)
  Form of expected instruction(s): `vmull.p8` q0`,` d0`,` d0

- int64x2_t vqdmull_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vqdmull.s32` q0`,` d0`,` d0

- int32x4_t vqdmull_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vqdmull.s16` q0`,` d0`,` d0

##### 6.57.6.3 Multiply-accumulate

- uint32x2_t vmla_u32 (uint32x2_t, uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vmla.i32` d0`,` d0`,` d0

- uint16x4_t vmla_u16 (uint16x4_t, uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vmla.i16` d0`,` d0`,` d0

- uint8x8_t vmla_u8 (uint8x8_t, uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vmla.i8` d0`,` d0`,` d0

- int32x2_t vmla_s32 (int32x2_t, int32x2_t, int32x2_t)
  Form of expected instruction(s): `vmla.i32` d0`,` d0`,` d0

- int16x4_t vmla_s16 (int16x4_t, int16x4_t, int16x4_t)
  Form of expected instruction(s): `vmla.i16` d0`,` d0`,` d0

- int8x8_t vmla_s8 (int8x8_t, int8x8_t, int8x8_t)
  Form of expected instruction(s): `vmla.i8` d0`,` d0`,` d0

- float32x2_t vmla_f32 (float32x2_t, float32x2_t, float32x2_t)
  Form of expected instruction(s): `vmla.f32` d0`,` d0`,` d0

- uint32x4_t vmlaq_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vmla.i32` q0`,` q0`,` q0

- uint16x8_t vmlaq_u16 (uint16x8_t, uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vmla.i16` q0`,` q0`,` q0

- uint8x16_t vmlaq_u8 (uint8x16_t, uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vmla.i8` q0`,` q0`,` q0

- int32x4_t vmlaq_s32 (int32x4_t, int32x4_t, int32x4_t)
  Form of expected instruction(s): `vmla.i32` q0`,` q0`,` q0

- int16x8_t vmlaq_s16 (int16x8_t, int16x8_t, int16x8_t)
  Form of expected instruction(s): `vmla.i16` q0`,` q0`,` q0

- int8x16_t vmlaq_s8 (int8x16_t, int8x16_t, int8x16_t)
  Form of expected instruction(s): `vmla.i8` q0`,` q0`,` q0

- float32x4_t vmlaq_f32 (float32x4_t, float32x4_t, float32x4_t)
  Form of expected instruction(s): `vmla.f32` q0`,` q0`,` q0

- uint64x2_t vmlal_u32 (uint64x2_t, uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vmlal.u32` q0`,` d0`,` d0

- uint32x4_t vmlal_u16 (uint32x4_t, uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vmlal.u16` q0`,` d0`,` d0

- uint16x8_t vmlal_u8 (uint16x8_t, uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vmlal.u8` q0`,` d0`,` d0

- int64x2_t vmlal_s32 (int64x2_t, int32x2_t, int32x2_t)
  Form of expected instruction(s): `vmlal.s32` q0`,` d0`,` d0

- int32x4_t vmlal_s16 (int32x4_t, int16x4_t, int16x4_t)
  Form of expected instruction(s): `vmlal.s16` q0`,` d0`,` d0

- int16x8_t vmlal_s8 (int16x8_t, int8x8_t, int8x8_t)
  Form of expected instruction(s): `vmlal.s8` q0`,` d0`,` d0

- int64x2_t vqdmlal_s32 (int64x2_t, int32x2_t, int32x2_t)
  Form of expected instruction(s): `vqdmlal.s32` q0`,` d0`,` d0

- int32x4_t vqdmlal_s16 (int32x4_t, int16x4_t, int16x4_t)
  Form of expected instruction(s): `vqdmlal.s16` q0`,` d0`,` d0

##### 6.57.6.4 Multiply-subtract

- uint32x2_t vmls_u32 (uint32x2_t, uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vmls.i32` d0`,` d0`,` d0

- uint16x4_t vmls_u16 (uint16x4_t, uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vmls.i16` d0`,` d0`,` d0

- uint8x8_t vmls_u8 (uint8x8_t, uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vmls.i8` d0`,` d0`,` d0

- int32x2_t vmls_s32 (int32x2_t, int32x2_t, int32x2_t)
  Form of expected instruction(s): `vmls.i32` d0`,` d0`,` d0

- int16x4_t vmls_s16 (int16x4_t, int16x4_t, int16x4_t)
  Form of expected instruction(s): `vmls.i16` d0`,` d0`,` d0

- int8x8_t vmls_s8 (int8x8_t, int8x8_t, int8x8_t)
  Form of expected instruction(s): `vmls.i8` d0`,` d0`,` d0

- float32x2_t vmls_f32 (float32x2_t, float32x2_t, float32x2_t)
  Form of expected instruction(s): `vmls.f32` d0`,` d0`,` d0

- uint32x4_t vmlsq_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vmls.i32` q0`,` q0`,` q0

- uint16x8_t vmlsq_u16 (uint16x8_t, uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vmls.i16` q0`,` q0`,` q0

- uint8x16_t vmlsq_u8 (uint8x16_t, uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vmls.i8` q0`,` q0`,` q0

- int32x4_t vmlsq_s32 (int32x4_t, int32x4_t, int32x4_t)
  Form of expected instruction(s): `vmls.i32` q0`,` q0`,` q0

- int16x8_t vmlsq_s16 (int16x8_t, int16x8_t, int16x8_t)
  Form of expected instruction(s): `vmls.i16` q0`,` q0`,` q0

- int8x16_t vmlsq_s8 (int8x16_t, int8x16_t, int8x16_t)
  Form of expected instruction(s): `vmls.i8` q0`,` q0`,` q0

- float32x4_t vmlsq_f32 (float32x4_t, float32x4_t, float32x4_t)
  Form of expected instruction(s): `vmls.f32` q0`,` q0`,` q0

- uint64x2_t vmlsl_u32 (uint64x2_t, uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vmlsl.u32` q0`,` d0`,` d0

- uint32x4_t vmlsl_u16 (uint32x4_t, uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vmlsl.u16` q0`,` d0`,` d0

- uint16x8_t vmlsl_u8 (uint16x8_t, uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vmlsl.u8` q0`,` d0`,` d0

- int64x2_t vmlsl_s32 (int64x2_t, int32x2_t, int32x2_t)
  Form of expected instruction(s): `vmlsl.s32` q0`,` d0`,` d0

- int32x4_t vmlsl_s16 (int32x4_t, int16x4_t, int16x4_t)
  Form of expected instruction(s): `vmlsl.s16` q0`,` d0`,` d0

- int16x8_t vmlsl_s8 (int16x8_t, int8x8_t, int8x8_t)
  Form of expected instruction(s): `vmlsl.s8` q0`,` d0`,` d0

- int64x2_t vqdmlsl_s32 (int64x2_t, int32x2_t, int32x2_t)
  Form of expected instruction(s): `vqdmlsl.s32` q0`,` d0`,` d0

- int32x4_t vqdmlsl_s16 (int32x4_t, int16x4_t, int16x4_t)
  Form of expected instruction(s): `vqdmlsl.s16` q0`,` d0`,` d0

##### 6.57.6.5 Fused-multiply-accumulate

- float32x2_t vfma_f32 (float32x2_t, float32x2_t, float32x2_t)
  Form of expected instruction(s): `vfma.f32` d0`,` d0`,` d0

- float32x4_t vfmaq_f32 (float32x4_t, float32x4_t, float32x4_t)
  Form of expected instruction(s): `vfma.f32` q0`,` q0`,` q0

##### 6.57.6.6 Fused-multiply-subtract

- float32x2_t vfms_f32 (float32x2_t, float32x2_t, float32x2_t)
  Form of expected instruction(s): `vfms.f32` d0`,` d0`,` d0

- float32x4_t vfmsq_f32 (float32x4_t, float32x4_t, float32x4_t)
  Form of expected instruction(s): `vfms.f32` q0`,` q0`,` q0

##### 6.57.6.7 Round to integral (to nearest, ties to even)

- float32x2_t vrndn_f32 (float32x2_t)
  Form of expected instruction(s): `vrintn.f32` d0`,` d0

- float32x4_t vrndqn_f32 (float32x4_t)
  Form of expected instruction(s): `vrintn.f32` q0`,` q0

##### 6.57.6.8 Round to integral (to nearest, ties away from zero)

- float32x2_t vrnda_f32 (float32x2_t)
  Form of expected instruction(s): `vrinta.f32` d0`,` d0

- float32x4_t vrndqa_f32 (float32x4_t)
  Form of expected instruction(s): `vrinta.f32` q0`,` q0

##### 6.57.6.9 Round to integral (towards +Inf)

- float32x2_t vrndp_f32 (float32x2_t)
  Form of expected instruction(s): `vrintp.f32` d0`,` d0

- float32x4_t vrndqp_f32 (float32x4_t)
  Form of expected instruction(s): `vrintp.f32` q0`,` q0

##### 6.57.6.10 Round to integral (towards -Inf)

- float32x2_t vrndm_f32 (float32x2_t)
  Form of expected instruction(s): `vrintm.f32` d0`,` d0

- float32x4_t vrndqm_f32 (float32x4_t)
  Form of expected instruction(s): `vrintm.f32` q0`,` q0

##### 6.57.6.11 Round to integral (towards 0)

- float32x2_t vrnd_f32 (float32x2_t)
  Form of expected instruction(s): `vrintz.f32` d0`,` d0

- float32x4_t vrndq_f32 (float32x4_t)
  Form of expected instruction(s): `vrintz.f32` q0`,` q0

##### 6.57.6.12 Subtraction

- uint32x2_t vsub_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vsub.i32` d0`,` d0`,` d0

- uint16x4_t vsub_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vsub.i16` d0`,` d0`,` d0

- uint8x8_t vsub_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vsub.i8` d0`,` d0`,` d0

- int32x2_t vsub_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vsub.i32` d0`,` d0`,` d0

- int16x4_t vsub_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vsub.i16` d0`,` d0`,` d0

- int8x8_t vsub_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vsub.i8` d0`,` d0`,` d0

- float32x2_t vsub_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vsub.f32` d0`,` d0`,` d0

- uint64x1_t vsub_u64 (uint64x1_t, uint64x1_t)

- int64x1_t vsub_s64 (int64x1_t, int64x1_t)

- uint32x4_t vsubq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vsub.i32` q0`,` q0`,` q0

- uint16x8_t vsubq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vsub.i16` q0`,` q0`,` q0

- uint8x16_t vsubq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vsub.i8` q0`,` q0`,` q0

- int32x4_t vsubq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vsub.i32` q0`,` q0`,` q0

- int16x8_t vsubq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vsub.i16` q0`,` q0`,` q0

- int8x16_t vsubq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vsub.i8` q0`,` q0`,` q0

- uint64x2_t vsubq_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vsub.i64` q0`,` q0`,` q0

- int64x2_t vsubq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vsub.i64` q0`,` q0`,` q0

- float32x4_t vsubq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vsub.f32` q0`,` q0`,` q0

- uint64x2_t vsubl_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vsubl.u32` q0`,` d0`,` d0

- uint32x4_t vsubl_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vsubl.u16` q0`,` d0`,` d0

- uint16x8_t vsubl_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vsubl.u8` q0`,` d0`,` d0

- int64x2_t vsubl_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vsubl.s32` q0`,` d0`,` d0

- int32x4_t vsubl_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vsubl.s16` q0`,` d0`,` d0

- int16x8_t vsubl_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vsubl.s8` q0`,` d0`,` d0

- uint64x2_t vsubw_u32 (uint64x2_t, uint32x2_t)
  Form of expected instruction(s): `vsubw.u32` q0`,` q0`,` d0

- uint32x4_t vsubw_u16 (uint32x4_t, uint16x4_t)
  Form of expected instruction(s): `vsubw.u16` q0`,` q0`,` d0

- uint16x8_t vsubw_u8 (uint16x8_t, uint8x8_t)
  Form of expected instruction(s): `vsubw.u8` q0`,` q0`,` d0

- int64x2_t vsubw_s32 (int64x2_t, int32x2_t)
  Form of expected instruction(s): `vsubw.s32` q0`,` q0`,` d0

- int32x4_t vsubw_s16 (int32x4_t, int16x4_t)
  Form of expected instruction(s): `vsubw.s16` q0`,` q0`,` d0

- int16x8_t vsubw_s8 (int16x8_t, int8x8_t)
  Form of expected instruction(s): `vsubw.s8` q0`,` q0`,` d0

- uint32x2_t vhsub_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vhsub.u32` d0`,` d0`,` d0

- uint16x4_t vhsub_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vhsub.u16` d0`,` d0`,` d0

- uint8x8_t vhsub_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vhsub.u8` d0`,` d0`,` d0

- int32x2_t vhsub_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vhsub.s32` d0`,` d0`,` d0

- int16x4_t vhsub_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vhsub.s16` d0`,` d0`,` d0

- int8x8_t vhsub_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vhsub.s8` d0`,` d0`,` d0

- uint32x4_t vhsubq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vhsub.u32` q0`,` q0`,` q0

- uint16x8_t vhsubq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vhsub.u16` q0`,` q0`,` q0

- uint8x16_t vhsubq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vhsub.u8` q0`,` q0`,` q0

- int32x4_t vhsubq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vhsub.s32` q0`,` q0`,` q0

- int16x8_t vhsubq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vhsub.s16` q0`,` q0`,` q0

- int8x16_t vhsubq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vhsub.s8` q0`,` q0`,` q0

- uint32x2_t vqsub_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vqsub.u32` d0`,` d0`,` d0

- uint16x4_t vqsub_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vqsub.u16` d0`,` d0`,` d0

- uint8x8_t vqsub_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vqsub.u8` d0`,` d0`,` d0

- int32x2_t vqsub_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vqsub.s32` d0`,` d0`,` d0

- int16x4_t vqsub_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vqsub.s16` d0`,` d0`,` d0

- int8x8_t vqsub_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vqsub.s8` d0`,` d0`,` d0

- uint64x1_t vqsub_u64 (uint64x1_t, uint64x1_t)
  Form of expected instruction(s): `vqsub.u64` d0`,` d0`,` d0

- int64x1_t vqsub_s64 (int64x1_t, int64x1_t)
  Form of expected instruction(s): `vqsub.s64` d0`,` d0`,` d0

- uint32x4_t vqsubq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vqsub.u32` q0`,` q0`,` q0

- uint16x8_t vqsubq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vqsub.u16` q0`,` q0`,` q0

- uint8x16_t vqsubq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vqsub.u8` q0`,` q0`,` q0

- int32x4_t vqsubq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vqsub.s32` q0`,` q0`,` q0

- int16x8_t vqsubq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vqsub.s16` q0`,` q0`,` q0

- int8x16_t vqsubq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vqsub.s8` q0`,` q0`,` q0

- uint64x2_t vqsubq_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vqsub.u64` q0`,` q0`,` q0

- int64x2_t vqsubq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vqsub.s64` q0`,` q0`,` q0

- uint32x2_t vsubhn_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vsubhn.i64` d0`,` q0`,` q0

- uint16x4_t vsubhn_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vsubhn.i32` d0`,` q0`,` q0

- uint8x8_t vsubhn_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vsubhn.i16` d0`,` q0`,` q0

- int32x2_t vsubhn_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vsubhn.i64` d0`,` q0`,` q0

- int16x4_t vsubhn_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vsubhn.i32` d0`,` q0`,` q0

- int8x8_t vsubhn_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vsubhn.i16` d0`,` q0`,` q0

- uint32x2_t vrsubhn_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vrsubhn.i64` d0`,` q0`,` q0

- uint16x4_t vrsubhn_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vrsubhn.i32` d0`,` q0`,` q0

- uint8x8_t vrsubhn_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vrsubhn.i16` d0`,` q0`,` q0

- int32x2_t vrsubhn_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vrsubhn.i64` d0`,` q0`,` q0

- int16x4_t vrsubhn_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vrsubhn.i32` d0`,` q0`,` q0

- int8x8_t vrsubhn_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vrsubhn.i16` d0`,` q0`,` q0

##### 6.57.6.13 Comparison (equal-to)

- uint32x2_t vceq_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vceq.i32` d0`,` d0`,` d0

- uint16x4_t vceq_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vceq.i16` d0`,` d0`,` d0

- uint8x8_t vceq_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vceq.i8` d0`,` d0`,` d0

- uint32x2_t vceq_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vceq.i32` d0`,` d0`,` d0

- uint16x4_t vceq_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vceq.i16` d0`,` d0`,` d0

- uint8x8_t vceq_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vceq.i8` d0`,` d0`,` d0

- uint32x2_t vceq_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vceq.f32` d0`,` d0`,` d0

- uint8x8_t vceq_p8 (poly8x8_t, poly8x8_t)
  Form of expected instruction(s): `vceq.i8` d0`,` d0`,` d0

- uint32x4_t vceqq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vceq.i32` q0`,` q0`,` q0

- uint16x8_t vceqq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vceq.i16` q0`,` q0`,` q0

- uint8x16_t vceqq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vceq.i8` q0`,` q0`,` q0

- uint32x4_t vceqq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vceq.i32` q0`,` q0`,` q0

- uint16x8_t vceqq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vceq.i16` q0`,` q0`,` q0

- uint8x16_t vceqq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vceq.i8` q0`,` q0`,` q0

- uint32x4_t vceqq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vceq.f32` q0`,` q0`,` q0

- uint8x16_t vceqq_p8 (poly8x16_t, poly8x16_t)
  Form of expected instruction(s): `vceq.i8` q0`,` q0`,` q0

##### 6.57.6.14 Comparison (greater-than-or-equal-to)

- uint32x2_t vcge_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vcge.s32` d0`,` d0`,` d0

- uint16x4_t vcge_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vcge.s16` d0`,` d0`,` d0

- uint8x8_t vcge_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vcge.s8` d0`,` d0`,` d0

- uint32x2_t vcge_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vcge.f32` d0`,` d0`,` d0

- uint32x2_t vcge_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vcge.u32` d0`,` d0`,` d0

- uint16x4_t vcge_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vcge.u16` d0`,` d0`,` d0

- uint8x8_t vcge_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vcge.u8` d0`,` d0`,` d0

- uint32x4_t vcgeq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vcge.s32` q0`,` q0`,` q0

- uint16x8_t vcgeq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vcge.s16` q0`,` q0`,` q0

- uint8x16_t vcgeq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vcge.s8` q0`,` q0`,` q0

- uint32x4_t vcgeq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vcge.f32` q0`,` q0`,` q0

- uint32x4_t vcgeq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vcge.u32` q0`,` q0`,` q0

- uint16x8_t vcgeq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vcge.u16` q0`,` q0`,` q0

- uint8x16_t vcgeq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vcge.u8` q0`,` q0`,` q0

##### 6.57.6.15 Comparison (less-than-or-equal-to)

- uint32x2_t vcle_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vcge.s32` d0`,` d0`,` d0

- uint16x4_t vcle_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vcge.s16` d0`,` d0`,` d0

- uint8x8_t vcle_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vcge.s8` d0`,` d0`,` d0

- uint32x2_t vcle_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vcge.f32` d0`,` d0`,` d0

- uint32x2_t vcle_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vcge.u32` d0`,` d0`,` d0

- uint16x4_t vcle_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vcge.u16` d0`,` d0`,` d0

- uint8x8_t vcle_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vcge.u8` d0`,` d0`,` d0

- uint32x4_t vcleq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vcge.s32` q0`,` q0`,` q0

- uint16x8_t vcleq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vcge.s16` q0`,` q0`,` q0

- uint8x16_t vcleq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vcge.s8` q0`,` q0`,` q0

- uint32x4_t vcleq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vcge.f32` q0`,` q0`,` q0

- uint32x4_t vcleq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vcge.u32` q0`,` q0`,` q0

- uint16x8_t vcleq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vcge.u16` q0`,` q0`,` q0

- uint8x16_t vcleq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vcge.u8` q0`,` q0`,` q0

##### 6.57.6.16 Comparison (greater-than)

- uint32x2_t vcgt_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vcgt.s32` d0`,` d0`,` d0

- uint16x4_t vcgt_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vcgt.s16` d0`,` d0`,` d0

- uint8x8_t vcgt_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vcgt.s8` d0`,` d0`,` d0

- uint32x2_t vcgt_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vcgt.f32` d0`,` d0`,` d0

- uint32x2_t vcgt_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vcgt.u32` d0`,` d0`,` d0

- uint16x4_t vcgt_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vcgt.u16` d0`,` d0`,` d0

- uint8x8_t vcgt_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vcgt.u8` d0`,` d0`,` d0

- uint32x4_t vcgtq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vcgt.s32` q0`,` q0`,` q0

- uint16x8_t vcgtq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vcgt.s16` q0`,` q0`,` q0

- uint8x16_t vcgtq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vcgt.s8` q0`,` q0`,` q0

- uint32x4_t vcgtq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vcgt.f32` q0`,` q0`,` q0

- uint32x4_t vcgtq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vcgt.u32` q0`,` q0`,` q0

- uint16x8_t vcgtq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vcgt.u16` q0`,` q0`,` q0

- uint8x16_t vcgtq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vcgt.u8` q0`,` q0`,` q0

##### 6.57.6.17 Comparison (less-than)

- uint32x2_t vclt_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vcgt.s32` d0`,` d0`,` d0

- uint16x4_t vclt_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vcgt.s16` d0`,` d0`,` d0

- uint8x8_t vclt_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vcgt.s8` d0`,` d0`,` d0

- uint32x2_t vclt_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vcgt.f32` d0`,` d0`,` d0

- uint32x2_t vclt_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vcgt.u32` d0`,` d0`,` d0

- uint16x4_t vclt_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vcgt.u16` d0`,` d0`,` d0

- uint8x8_t vclt_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vcgt.u8` d0`,` d0`,` d0

- uint32x4_t vcltq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vcgt.s32` q0`,` q0`,` q0

- uint16x8_t vcltq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vcgt.s16` q0`,` q0`,` q0

- uint8x16_t vcltq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vcgt.s8` q0`,` q0`,` q0

- uint32x4_t vcltq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vcgt.f32` q0`,` q0`,` q0

- uint32x4_t vcltq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vcgt.u32` q0`,` q0`,` q0

- uint16x8_t vcltq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vcgt.u16` q0`,` q0`,` q0

- uint8x16_t vcltq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vcgt.u8` q0`,` q0`,` q0

##### 6.57.6.18 Comparison (absolute greater-than-or-equal-to)

- uint32x2_t vcage_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vacge.f32` d0`,` d0`,` d0

- uint32x4_t vcageq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vacge.f32` q0`,` q0`,` q0

##### 6.57.6.19 Comparison (absolute less-than-or-equal-to)

- uint32x2_t vcale_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vacge.f32` d0`,` d0`,` d0

- uint32x4_t vcaleq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vacge.f32` q0`,` q0`,` q0

##### 6.57.6.20 Comparison (absolute greater-than)

- uint32x2_t vcagt_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vacgt.f32` d0`,` d0`,` d0

- uint32x4_t vcagtq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vacgt.f32` q0`,` q0`,` q0

##### 6.57.6.21 Comparison (absolute less-than)

- uint32x2_t vcalt_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vacgt.f32` d0`,` d0`,` d0

- uint32x4_t vcaltq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vacgt.f32` q0`,` q0`,` q0

##### 6.57.6.22 Test bits

- uint32x2_t vtst_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vtst.32` d0`,` d0`,` d0

- uint16x4_t vtst_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vtst.16` d0`,` d0`,` d0

- uint8x8_t vtst_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vtst.8` d0`,` d0`,` d0

- uint32x2_t vtst_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vtst.32` d0`,` d0`,` d0

- uint16x4_t vtst_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vtst.16` d0`,` d0`,` d0

- uint8x8_t vtst_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vtst.8` d0`,` d0`,` d0

- uint8x8_t vtst_p8 (poly8x8_t, poly8x8_t)
  Form of expected instruction(s): `vtst.8` d0`,` d0`,` d0

- uint32x4_t vtstq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vtst.32` q0`,` q0`,` q0

- uint16x8_t vtstq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vtst.16` q0`,` q0`,` q0

- uint8x16_t vtstq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vtst.8` q0`,` q0`,` q0

- uint32x4_t vtstq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vtst.32` q0`,` q0`,` q0

- uint16x8_t vtstq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vtst.16` q0`,` q0`,` q0

- uint8x16_t vtstq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vtst.8` q0`,` q0`,` q0

- uint8x16_t vtstq_p8 (poly8x16_t, poly8x16_t)
  Form of expected instruction(s): `vtst.8` q0`,` q0`,` q0

##### 6.57.6.23 Absolute difference

- uint32x2_t vabd_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vabd.u32` d0`,` d0`,` d0

- uint16x4_t vabd_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vabd.u16` d0`,` d0`,` d0

- uint8x8_t vabd_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vabd.u8` d0`,` d0`,` d0

- int32x2_t vabd_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vabd.s32` d0`,` d0`,` d0

- int16x4_t vabd_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vabd.s16` d0`,` d0`,` d0

- int8x8_t vabd_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vabd.s8` d0`,` d0`,` d0

- float32x2_t vabd_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vabd.f32` d0`,` d0`,` d0

- uint32x4_t vabdq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vabd.u32` q0`,` q0`,` q0

- uint16x8_t vabdq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vabd.u16` q0`,` q0`,` q0

- uint8x16_t vabdq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vabd.u8` q0`,` q0`,` q0

- int32x4_t vabdq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vabd.s32` q0`,` q0`,` q0

- int16x8_t vabdq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vabd.s16` q0`,` q0`,` q0

- int8x16_t vabdq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vabd.s8` q0`,` q0`,` q0

- float32x4_t vabdq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vabd.f32` q0`,` q0`,` q0

- uint64x2_t vabdl_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vabdl.u32` q0`,` d0`,` d0

- uint32x4_t vabdl_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vabdl.u16` q0`,` d0`,` d0

- uint16x8_t vabdl_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vabdl.u8` q0`,` d0`,` d0

- int64x2_t vabdl_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vabdl.s32` q0`,` d0`,` d0

- int32x4_t vabdl_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vabdl.s16` q0`,` d0`,` d0

- int16x8_t vabdl_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vabdl.s8` q0`,` d0`,` d0

##### 6.57.6.24 Absolute difference and accumulate

- uint32x2_t vaba_u32 (uint32x2_t, uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vaba.u32` d0`,` d0`,` d0

- uint16x4_t vaba_u16 (uint16x4_t, uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vaba.u16` d0`,` d0`,` d0

- uint8x8_t vaba_u8 (uint8x8_t, uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vaba.u8` d0`,` d0`,` d0

- int32x2_t vaba_s32 (int32x2_t, int32x2_t, int32x2_t)
  Form of expected instruction(s): `vaba.s32` d0`,` d0`,` d0

- int16x4_t vaba_s16 (int16x4_t, int16x4_t, int16x4_t)
  Form of expected instruction(s): `vaba.s16` d0`,` d0`,` d0

- int8x8_t vaba_s8 (int8x8_t, int8x8_t, int8x8_t)
  Form of expected instruction(s): `vaba.s8` d0`,` d0`,` d0

- uint32x4_t vabaq_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vaba.u32` q0`,` q0`,` q0

- uint16x8_t vabaq_u16 (uint16x8_t, uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vaba.u16` q0`,` q0`,` q0

- uint8x16_t vabaq_u8 (uint8x16_t, uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vaba.u8` q0`,` q0`,` q0

- int32x4_t vabaq_s32 (int32x4_t, int32x4_t, int32x4_t)
  Form of expected instruction(s): `vaba.s32` q0`,` q0`,` q0

- int16x8_t vabaq_s16 (int16x8_t, int16x8_t, int16x8_t)
  Form of expected instruction(s): `vaba.s16` q0`,` q0`,` q0

- int8x16_t vabaq_s8 (int8x16_t, int8x16_t, int8x16_t)
  Form of expected instruction(s): `vaba.s8` q0`,` q0`,` q0

- uint64x2_t vabal_u32 (uint64x2_t, uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vabal.u32` q0`,` d0`,` d0

- uint32x4_t vabal_u16 (uint32x4_t, uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vabal.u16` q0`,` d0`,` d0

- uint16x8_t vabal_u8 (uint16x8_t, uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vabal.u8` q0`,` d0`,` d0

- int64x2_t vabal_s32 (int64x2_t, int32x2_t, int32x2_t)
  Form of expected instruction(s): `vabal.s32` q0`,` d0`,` d0

- int32x4_t vabal_s16 (int32x4_t, int16x4_t, int16x4_t)
  Form of expected instruction(s): `vabal.s16` q0`,` d0`,` d0

- int16x8_t vabal_s8 (int16x8_t, int8x8_t, int8x8_t)
  Form of expected instruction(s): `vabal.s8` q0`,` d0`,` d0

##### 6.57.6.25 Maximum

- uint32x2_t vmax_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vmax.u32` d0`,` d0`,` d0

- uint16x4_t vmax_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vmax.u16` d0`,` d0`,` d0

- uint8x8_t vmax_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vmax.u8` d0`,` d0`,` d0

- int32x2_t vmax_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vmax.s32` d0`,` d0`,` d0

- int16x4_t vmax_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vmax.s16` d0`,` d0`,` d0

- int8x8_t vmax_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vmax.s8` d0`,` d0`,` d0

- float32x2_t vmax_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vmax.f32` d0`,` d0`,` d0

- uint32x4_t vmaxq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vmax.u32` q0`,` q0`,` q0

- uint16x8_t vmaxq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vmax.u16` q0`,` q0`,` q0

- uint8x16_t vmaxq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vmax.u8` q0`,` q0`,` q0

- int32x4_t vmaxq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vmax.s32` q0`,` q0`,` q0

- int16x8_t vmaxq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vmax.s16` q0`,` q0`,` q0

- int8x16_t vmaxq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vmax.s8` q0`,` q0`,` q0

- float32x4_t vmaxq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vmax.f32` q0`,` q0`,` q0

##### 6.57.6.26 Minimum

- uint32x2_t vmin_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vmin.u32` d0`,` d0`,` d0

- uint16x4_t vmin_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vmin.u16` d0`,` d0`,` d0

- uint8x8_t vmin_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vmin.u8` d0`,` d0`,` d0

- int32x2_t vmin_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vmin.s32` d0`,` d0`,` d0

- int16x4_t vmin_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vmin.s16` d0`,` d0`,` d0

- int8x8_t vmin_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vmin.s8` d0`,` d0`,` d0

- float32x2_t vmin_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vmin.f32` d0`,` d0`,` d0

- uint32x4_t vminq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vmin.u32` q0`,` q0`,` q0

- uint16x8_t vminq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vmin.u16` q0`,` q0`,` q0

- uint8x16_t vminq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vmin.u8` q0`,` q0`,` q0

- int32x4_t vminq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vmin.s32` q0`,` q0`,` q0

- int16x8_t vminq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vmin.s16` q0`,` q0`,` q0

- int8x16_t vminq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vmin.s8` q0`,` q0`,` q0

- float32x4_t vminq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vmin.f32` q0`,` q0`,` q0

##### 6.57.6.27 Pairwise add

- uint32x2_t vpadd_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vpadd.i32` d0`,` d0`,` d0

- uint16x4_t vpadd_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vpadd.i16` d0`,` d0`,` d0

- uint8x8_t vpadd_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vpadd.i8` d0`,` d0`,` d0

- int32x2_t vpadd_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vpadd.i32` d0`,` d0`,` d0

- int16x4_t vpadd_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vpadd.i16` d0`,` d0`,` d0

- int8x8_t vpadd_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vpadd.i8` d0`,` d0`,` d0

- float32x2_t vpadd_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vpadd.f32` d0`,` d0`,` d0

- uint64x1_t vpaddl_u32 (uint32x2_t)
  Form of expected instruction(s): `vpaddl.u32` d0`,` d0

- uint32x2_t vpaddl_u16 (uint16x4_t)
  Form of expected instruction(s): `vpaddl.u16` d0`,` d0

- uint16x4_t vpaddl_u8 (uint8x8_t)
  Form of expected instruction(s): `vpaddl.u8` d0`,` d0

- int64x1_t vpaddl_s32 (int32x2_t)
  Form of expected instruction(s): `vpaddl.s32` d0`,` d0

- int32x2_t vpaddl_s16 (int16x4_t)
  Form of expected instruction(s): `vpaddl.s16` d0`,` d0

- int16x4_t vpaddl_s8 (int8x8_t)
  Form of expected instruction(s): `vpaddl.s8` d0`,` d0

- uint64x2_t vpaddlq_u32 (uint32x4_t)
  Form of expected instruction(s): `vpaddl.u32` q0`,` q0

- uint32x4_t vpaddlq_u16 (uint16x8_t)
  Form of expected instruction(s): `vpaddl.u16` q0`,` q0

- uint16x8_t vpaddlq_u8 (uint8x16_t)
  Form of expected instruction(s): `vpaddl.u8` q0`,` q0

- int64x2_t vpaddlq_s32 (int32x4_t)
  Form of expected instruction(s): `vpaddl.s32` q0`,` q0

- int32x4_t vpaddlq_s16 (int16x8_t)
  Form of expected instruction(s): `vpaddl.s16` q0`,` q0

- int16x8_t vpaddlq_s8 (int8x16_t)
  Form of expected instruction(s): `vpaddl.s8` q0`,` q0

##### 6.57.6.28 Pairwise add, single_opcode widen and accumulate

- uint64x1_t vpadal_u32 (uint64x1_t, uint32x2_t)
  Form of expected instruction(s): `vpadal.u32` d0`,` d0

- uint32x2_t vpadal_u16 (uint32x2_t, uint16x4_t)
  Form of expected instruction(s): `vpadal.u16` d0`,` d0

- uint16x4_t vpadal_u8 (uint16x4_t, uint8x8_t)
  Form of expected instruction(s): `vpadal.u8` d0`,` d0

- int64x1_t vpadal_s32 (int64x1_t, int32x2_t)
  Form of expected instruction(s): `vpadal.s32` d0`,` d0

- int32x2_t vpadal_s16 (int32x2_t, int16x4_t)
  Form of expected instruction(s): `vpadal.s16` d0`,` d0

- int16x4_t vpadal_s8 (int16x4_t, int8x8_t)
  Form of expected instruction(s): `vpadal.s8` d0`,` d0

- uint64x2_t vpadalq_u32 (uint64x2_t, uint32x4_t)
  Form of expected instruction(s): `vpadal.u32` q0`,` q0

- uint32x4_t vpadalq_u16 (uint32x4_t, uint16x8_t)
  Form of expected instruction(s): `vpadal.u16` q0`,` q0

- uint16x8_t vpadalq_u8 (uint16x8_t, uint8x16_t)
  Form of expected instruction(s): `vpadal.u8` q0`,` q0

- int64x2_t vpadalq_s32 (int64x2_t, int32x4_t)
  Form of expected instruction(s): `vpadal.s32` q0`,` q0

- int32x4_t vpadalq_s16 (int32x4_t, int16x8_t)
  Form of expected instruction(s): `vpadal.s16` q0`,` q0

- int16x8_t vpadalq_s8 (int16x8_t, int8x16_t)
  Form of expected instruction(s): `vpadal.s8` q0`,` q0

##### 6.57.6.29 Folding maximum

- uint32x2_t vpmax_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vpmax.u32` d0`,` d0`,` d0

- uint16x4_t vpmax_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vpmax.u16` d0`,` d0`,` d0

- uint8x8_t vpmax_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vpmax.u8` d0`,` d0`,` d0

- int32x2_t vpmax_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vpmax.s32` d0`,` d0`,` d0

- int16x4_t vpmax_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vpmax.s16` d0`,` d0`,` d0

- int8x8_t vpmax_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vpmax.s8` d0`,` d0`,` d0

- float32x2_t vpmax_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vpmax.f32` d0`,` d0`,` d0

##### 6.57.6.30 Folding minimum

- uint32x2_t vpmin_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vpmin.u32` d0`,` d0`,` d0

- uint16x4_t vpmin_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vpmin.u16` d0`,` d0`,` d0

- uint8x8_t vpmin_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vpmin.u8` d0`,` d0`,` d0

- int32x2_t vpmin_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vpmin.s32` d0`,` d0`,` d0

- int16x4_t vpmin_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vpmin.s16` d0`,` d0`,` d0

- int8x8_t vpmin_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vpmin.s8` d0`,` d0`,` d0

- float32x2_t vpmin_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vpmin.f32` d0`,` d0`,` d0

##### 6.57.6.31 Reciprocal step

- float32x2_t vrecps_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vrecps.f32` d0`,` d0`,` d0

- float32x4_t vrecpsq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vrecps.f32` q0`,` q0`,` q0

- float32x2_t vrsqrts_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vrsqrts.f32` d0`,` d0`,` d0

- float32x4_t vrsqrtsq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vrsqrts.f32` q0`,` q0`,` q0

##### 6.57.6.32 Vector shift left

- uint32x2_t vshl_u32 (uint32x2_t, int32x2_t)
  Form of expected instruction(s): `vshl.u32` d0`,` d0`,` d0

- uint16x4_t vshl_u16 (uint16x4_t, int16x4_t)
  Form of expected instruction(s): `vshl.u16` d0`,` d0`,` d0

- uint8x8_t vshl_u8 (uint8x8_t, int8x8_t)
  Form of expected instruction(s): `vshl.u8` d0`,` d0`,` d0

- int32x2_t vshl_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vshl.s32` d0`,` d0`,` d0

- int16x4_t vshl_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vshl.s16` d0`,` d0`,` d0

- int8x8_t vshl_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vshl.s8` d0`,` d0`,` d0

- uint64x1_t vshl_u64 (uint64x1_t, int64x1_t)
  Form of expected instruction(s): `vshl.u64` d0`,` d0`,` d0

- int64x1_t vshl_s64 (int64x1_t, int64x1_t)
  Form of expected instruction(s): `vshl.s64` d0`,` d0`,` d0

- uint32x4_t vshlq_u32 (uint32x4_t, int32x4_t)
  Form of expected instruction(s): `vshl.u32` q0`,` q0`,` q0

- uint16x8_t vshlq_u16 (uint16x8_t, int16x8_t)
  Form of expected instruction(s): `vshl.u16` q0`,` q0`,` q0

- uint8x16_t vshlq_u8 (uint8x16_t, int8x16_t)
  Form of expected instruction(s): `vshl.u8` q0`,` q0`,` q0

- int32x4_t vshlq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vshl.s32` q0`,` q0`,` q0

- int16x8_t vshlq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vshl.s16` q0`,` q0`,` q0

- int8x16_t vshlq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vshl.s8` q0`,` q0`,` q0

- uint64x2_t vshlq_u64 (uint64x2_t, int64x2_t)
  Form of expected instruction(s): `vshl.u64` q0`,` q0`,` q0

- int64x2_t vshlq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vshl.s64` q0`,` q0`,` q0

- uint32x2_t vrshl_u32 (uint32x2_t, int32x2_t)
  Form of expected instruction(s): `vrshl.u32` d0`,` d0`,` d0

- uint16x4_t vrshl_u16 (uint16x4_t, int16x4_t)
  Form of expected instruction(s): `vrshl.u16` d0`,` d0`,` d0

- uint8x8_t vrshl_u8 (uint8x8_t, int8x8_t)
  Form of expected instruction(s): `vrshl.u8` d0`,` d0`,` d0

- int32x2_t vrshl_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vrshl.s32` d0`,` d0`,` d0

- int16x4_t vrshl_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vrshl.s16` d0`,` d0`,` d0

- int8x8_t vrshl_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vrshl.s8` d0`,` d0`,` d0

- uint64x1_t vrshl_u64 (uint64x1_t, int64x1_t)
  Form of expected instruction(s): `vrshl.u64` d0`,` d0`,` d0

- int64x1_t vrshl_s64 (int64x1_t, int64x1_t)
  Form of expected instruction(s): `vrshl.s64` d0`,` d0`,` d0

- uint32x4_t vrshlq_u32 (uint32x4_t, int32x4_t)
  Form of expected instruction(s): `vrshl.u32` q0`,` q0`,` q0

- uint16x8_t vrshlq_u16 (uint16x8_t, int16x8_t)
  Form of expected instruction(s): `vrshl.u16` q0`,` q0`,` q0

- uint8x16_t vrshlq_u8 (uint8x16_t, int8x16_t)
  Form of expected instruction(s): `vrshl.u8` q0`,` q0`,` q0

- int32x4_t vrshlq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vrshl.s32` q0`,` q0`,` q0

- int16x8_t vrshlq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vrshl.s16` q0`,` q0`,` q0

- int8x16_t vrshlq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vrshl.s8` q0`,` q0`,` q0

- uint64x2_t vrshlq_u64 (uint64x2_t, int64x2_t)
  Form of expected instruction(s): `vrshl.u64` q0`,` q0`,` q0

- int64x2_t vrshlq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vrshl.s64` q0`,` q0`,` q0

- uint32x2_t vqshl_u32 (uint32x2_t, int32x2_t)
  Form of expected instruction(s): `vqshl.u32` d0`,` d0`,` d0

- uint16x4_t vqshl_u16 (uint16x4_t, int16x4_t)
  Form of expected instruction(s): `vqshl.u16` d0`,` d0`,` d0

- uint8x8_t vqshl_u8 (uint8x8_t, int8x8_t)
  Form of expected instruction(s): `vqshl.u8` d0`,` d0`,` d0

- int32x2_t vqshl_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vqshl.s32` d0`,` d0`,` d0

- int16x4_t vqshl_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vqshl.s16` d0`,` d0`,` d0

- int8x8_t vqshl_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vqshl.s8` d0`,` d0`,` d0

- uint64x1_t vqshl_u64 (uint64x1_t, int64x1_t)
  Form of expected instruction(s): `vqshl.u64` d0`,` d0`,` d0

- int64x1_t vqshl_s64 (int64x1_t, int64x1_t)
  Form of expected instruction(s): `vqshl.s64` d0`,` d0`,` d0

- uint32x4_t vqshlq_u32 (uint32x4_t, int32x4_t)
  Form of expected instruction(s): `vqshl.u32` q0`,` q0`,` q0

- uint16x8_t vqshlq_u16 (uint16x8_t, int16x8_t)
  Form of expected instruction(s): `vqshl.u16` q0`,` q0`,` q0

- uint8x16_t vqshlq_u8 (uint8x16_t, int8x16_t)
  Form of expected instruction(s): `vqshl.u8` q0`,` q0`,` q0

- int32x4_t vqshlq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vqshl.s32` q0`,` q0`,` q0

- int16x8_t vqshlq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vqshl.s16` q0`,` q0`,` q0

- int8x16_t vqshlq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vqshl.s8` q0`,` q0`,` q0

- uint64x2_t vqshlq_u64 (uint64x2_t, int64x2_t)
  Form of expected instruction(s): `vqshl.u64` q0`,` q0`,` q0

- int64x2_t vqshlq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vqshl.s64` q0`,` q0`,` q0

- uint32x2_t vqrshl_u32 (uint32x2_t, int32x2_t)
  Form of expected instruction(s): `vqrshl.u32` d0`,` d0`,` d0

- uint16x4_t vqrshl_u16 (uint16x4_t, int16x4_t)
  Form of expected instruction(s): `vqrshl.u16` d0`,` d0`,` d0

- uint8x8_t vqrshl_u8 (uint8x8_t, int8x8_t)
  Form of expected instruction(s): `vqrshl.u8` d0`,` d0`,` d0

- int32x2_t vqrshl_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vqrshl.s32` d0`,` d0`,` d0

- int16x4_t vqrshl_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vqrshl.s16` d0`,` d0`,` d0

- int8x8_t vqrshl_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vqrshl.s8` d0`,` d0`,` d0

- uint64x1_t vqrshl_u64 (uint64x1_t, int64x1_t)
  Form of expected instruction(s): `vqrshl.u64` d0`,` d0`,` d0

- int64x1_t vqrshl_s64 (int64x1_t, int64x1_t)
  Form of expected instruction(s): `vqrshl.s64` d0`,` d0`,` d0

- uint32x4_t vqrshlq_u32 (uint32x4_t, int32x4_t)
  Form of expected instruction(s): `vqrshl.u32` q0`,` q0`,` q0

- uint16x8_t vqrshlq_u16 (uint16x8_t, int16x8_t)
  Form of expected instruction(s): `vqrshl.u16` q0`,` q0`,` q0

- uint8x16_t vqrshlq_u8 (uint8x16_t, int8x16_t)
  Form of expected instruction(s): `vqrshl.u8` q0`,` q0`,` q0

- int32x4_t vqrshlq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vqrshl.s32` q0`,` q0`,` q0

- int16x8_t vqrshlq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vqrshl.s16` q0`,` q0`,` q0

- int8x16_t vqrshlq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vqrshl.s8` q0`,` q0`,` q0

- uint64x2_t vqrshlq_u64 (uint64x2_t, int64x2_t)
  Form of expected instruction(s): `vqrshl.u64` q0`,` q0`,` q0

- int64x2_t vqrshlq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vqrshl.s64` q0`,` q0`,` q0

##### 6.57.6.33 Vector shift left by constant

- uint32x2_t vshl_n_u32 (uint32x2_t, const int)
  Form of expected instruction(s): `vshl.i32` d0`,` d0`, #`0

- uint16x4_t vshl_n_u16 (uint16x4_t, const int)
  Form of expected instruction(s): `vshl.i16` d0`,` d0`, #`0

- uint8x8_t vshl_n_u8 (uint8x8_t, const int)
  Form of expected instruction(s): `vshl.i8` d0`,` d0`, #`0

- int32x2_t vshl_n_s32 (int32x2_t, const int)
  Form of expected instruction(s): `vshl.i32` d0`,` d0`, #`0

- int16x4_t vshl_n_s16 (int16x4_t, const int)
  Form of expected instruction(s): `vshl.i16` d0`,` d0`, #`0

- int8x8_t vshl_n_s8 (int8x8_t, const int)
  Form of expected instruction(s): `vshl.i8` d0`,` d0`, #`0

- uint64x1_t vshl_n_u64 (uint64x1_t, const int)
  Form of expected instruction(s): `vshl.i64` d0`,` d0`, #`0

- int64x1_t vshl_n_s64 (int64x1_t, const int)
  Form of expected instruction(s): `vshl.i64` d0`,` d0`, #`0

- uint32x4_t vshlq_n_u32 (uint32x4_t, const int)
  Form of expected instruction(s): `vshl.i32` q0`,` q0`, #`0

- uint16x8_t vshlq_n_u16 (uint16x8_t, const int)
  Form of expected instruction(s): `vshl.i16` q0`,` q0`, #`0

- uint8x16_t vshlq_n_u8 (uint8x16_t, const int)
  Form of expected instruction(s): `vshl.i8` q0`,` q0`, #`0

- int32x4_t vshlq_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vshl.i32` q0`,` q0`, #`0

- int16x8_t vshlq_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vshl.i16` q0`,` q0`, #`0

- int8x16_t vshlq_n_s8 (int8x16_t, const int)
  Form of expected instruction(s): `vshl.i8` q0`,` q0`, #`0

- uint64x2_t vshlq_n_u64 (uint64x2_t, const int)
  Form of expected instruction(s): `vshl.i64` q0`,` q0`, #`0

- int64x2_t vshlq_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vshl.i64` q0`,` q0`, #`0

- uint32x2_t vqshl_n_u32 (uint32x2_t, const int)
  Form of expected instruction(s): `vqshl.u32` d0`,` d0`, #`0

- uint16x4_t vqshl_n_u16 (uint16x4_t, const int)
  Form of expected instruction(s): `vqshl.u16` d0`,` d0`, #`0

- uint8x8_t vqshl_n_u8 (uint8x8_t, const int)
  Form of expected instruction(s): `vqshl.u8` d0`,` d0`, #`0

- int32x2_t vqshl_n_s32 (int32x2_t, const int)
  Form of expected instruction(s): `vqshl.s32` d0`,` d0`, #`0

- int16x4_t vqshl_n_s16 (int16x4_t, const int)
  Form of expected instruction(s): `vqshl.s16` d0`,` d0`, #`0

- int8x8_t vqshl_n_s8 (int8x8_t, const int)
  Form of expected instruction(s): `vqshl.s8` d0`,` d0`, #`0

- uint64x1_t vqshl_n_u64 (uint64x1_t, const int)
  Form of expected instruction(s): `vqshl.u64` d0`,` d0`, #`0

- int64x1_t vqshl_n_s64 (int64x1_t, const int)
  Form of expected instruction(s): `vqshl.s64` d0`,` d0`, #`0

- uint32x4_t vqshlq_n_u32 (uint32x4_t, const int)
  Form of expected instruction(s): `vqshl.u32` q0`,` q0`, #`0

- uint16x8_t vqshlq_n_u16 (uint16x8_t, const int)
  Form of expected instruction(s): `vqshl.u16` q0`,` q0`, #`0

- uint8x16_t vqshlq_n_u8 (uint8x16_t, const int)
  Form of expected instruction(s): `vqshl.u8` q0`,` q0`, #`0

- int32x4_t vqshlq_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vqshl.s32` q0`,` q0`, #`0

- int16x8_t vqshlq_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vqshl.s16` q0`,` q0`, #`0

- int8x16_t vqshlq_n_s8 (int8x16_t, const int)
  Form of expected instruction(s): `vqshl.s8` q0`,` q0`, #`0

- uint64x2_t vqshlq_n_u64 (uint64x2_t, const int)
  Form of expected instruction(s): `vqshl.u64` q0`,` q0`, #`0

- int64x2_t vqshlq_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vqshl.s64` q0`,` q0`, #`0

- uint64x1_t vqshlu_n_s64 (int64x1_t, const int)
  Form of expected instruction(s): `vqshlu.s64` d0`,` d0`, #`0

- uint32x2_t vqshlu_n_s32 (int32x2_t, const int)
  Form of expected instruction(s): `vqshlu.s32` d0`,` d0`, #`0

- uint16x4_t vqshlu_n_s16 (int16x4_t, const int)
  Form of expected instruction(s): `vqshlu.s16` d0`,` d0`, #`0

- uint8x8_t vqshlu_n_s8 (int8x8_t, const int)
  Form of expected instruction(s): `vqshlu.s8` d0`,` d0`, #`0

- uint64x2_t vqshluq_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vqshlu.s64` q0`,` q0`, #`0

- uint32x4_t vqshluq_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vqshlu.s32` q0`,` q0`, #`0

- uint16x8_t vqshluq_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vqshlu.s16` q0`,` q0`, #`0

- uint8x16_t vqshluq_n_s8 (int8x16_t, const int)
  Form of expected instruction(s): `vqshlu.s8` q0`,` q0`, #`0

- uint64x2_t vshll_n_u32 (uint32x2_t, const int)
  Form of expected instruction(s): `vshll.u32` q0`,` d0`, #`0

- uint32x4_t vshll_n_u16 (uint16x4_t, const int)
  Form of expected instruction(s): `vshll.u16` q0`,` d0`, #`0

- uint16x8_t vshll_n_u8 (uint8x8_t, const int)
  Form of expected instruction(s): `vshll.u8` q0`,` d0`, #`0

- int64x2_t vshll_n_s32 (int32x2_t, const int)
  Form of expected instruction(s): `vshll.s32` q0`,` d0`, #`0

- int32x4_t vshll_n_s16 (int16x4_t, const int)
  Form of expected instruction(s): `vshll.s16` q0`,` d0`, #`0

- int16x8_t vshll_n_s8 (int8x8_t, const int)
  Form of expected instruction(s): `vshll.s8` q0`,` d0`, #`0

##### 6.57.6.34 Vector shift right by constant

- uint32x2_t vshr_n_u32 (uint32x2_t, const int)
  Form of expected instruction(s): `vshr.u32` d0`,` d0`, #`0

- uint16x4_t vshr_n_u16 (uint16x4_t, const int)
  Form of expected instruction(s): `vshr.u16` d0`,` d0`, #`0

- uint8x8_t vshr_n_u8 (uint8x8_t, const int)
  Form of expected instruction(s): `vshr.u8` d0`,` d0`, #`0

- int32x2_t vshr_n_s32 (int32x2_t, const int)
  Form of expected instruction(s): `vshr.s32` d0`,` d0`, #`0

- int16x4_t vshr_n_s16 (int16x4_t, const int)
  Form of expected instruction(s): `vshr.s16` d0`,` d0`, #`0

- int8x8_t vshr_n_s8 (int8x8_t, const int)
  Form of expected instruction(s): `vshr.s8` d0`,` d0`, #`0

- uint64x1_t vshr_n_u64 (uint64x1_t, const int)
  Form of expected instruction(s): `vshr.u64` d0`,` d0`, #`0

- int64x1_t vshr_n_s64 (int64x1_t, const int)
  Form of expected instruction(s): `vshr.s64` d0`,` d0`, #`0

- uint32x4_t vshrq_n_u32 (uint32x4_t, const int)
  Form of expected instruction(s): `vshr.u32` q0`,` q0`, #`0

- uint16x8_t vshrq_n_u16 (uint16x8_t, const int)
  Form of expected instruction(s): `vshr.u16` q0`,` q0`, #`0

- uint8x16_t vshrq_n_u8 (uint8x16_t, const int)
  Form of expected instruction(s): `vshr.u8` q0`,` q0`, #`0

- int32x4_t vshrq_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vshr.s32` q0`,` q0`, #`0

- int16x8_t vshrq_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vshr.s16` q0`,` q0`, #`0

- int8x16_t vshrq_n_s8 (int8x16_t, const int)
  Form of expected instruction(s): `vshr.s8` q0`,` q0`, #`0

- uint64x2_t vshrq_n_u64 (uint64x2_t, const int)
  Form of expected instruction(s): `vshr.u64` q0`,` q0`, #`0

- int64x2_t vshrq_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vshr.s64` q0`,` q0`, #`0

- uint32x2_t vrshr_n_u32 (uint32x2_t, const int)
  Form of expected instruction(s): `vrshr.u32` d0`,` d0`, #`0

- uint16x4_t vrshr_n_u16 (uint16x4_t, const int)
  Form of expected instruction(s): `vrshr.u16` d0`,` d0`, #`0

- uint8x8_t vrshr_n_u8 (uint8x8_t, const int)
  Form of expected instruction(s): `vrshr.u8` d0`,` d0`, #`0

- int32x2_t vrshr_n_s32 (int32x2_t, const int)
  Form of expected instruction(s): `vrshr.s32` d0`,` d0`, #`0

- int16x4_t vrshr_n_s16 (int16x4_t, const int)
  Form of expected instruction(s): `vrshr.s16` d0`,` d0`, #`0

- int8x8_t vrshr_n_s8 (int8x8_t, const int)
  Form of expected instruction(s): `vrshr.s8` d0`,` d0`, #`0

- uint64x1_t vrshr_n_u64 (uint64x1_t, const int)
  Form of expected instruction(s): `vrshr.u64` d0`,` d0`, #`0

- int64x1_t vrshr_n_s64 (int64x1_t, const int)
  Form of expected instruction(s): `vrshr.s64` d0`,` d0`, #`0

- uint32x4_t vrshrq_n_u32 (uint32x4_t, const int)
  Form of expected instruction(s): `vrshr.u32` q0`,` q0`, #`0

- uint16x8_t vrshrq_n_u16 (uint16x8_t, const int)
  Form of expected instruction(s): `vrshr.u16` q0`,` q0`, #`0

- uint8x16_t vrshrq_n_u8 (uint8x16_t, const int)
  Form of expected instruction(s): `vrshr.u8` q0`,` q0`, #`0

- int32x4_t vrshrq_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vrshr.s32` q0`,` q0`, #`0

- int16x8_t vrshrq_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vrshr.s16` q0`,` q0`, #`0

- int8x16_t vrshrq_n_s8 (int8x16_t, const int)
  Form of expected instruction(s): `vrshr.s8` q0`,` q0`, #`0

- uint64x2_t vrshrq_n_u64 (uint64x2_t, const int)
  Form of expected instruction(s): `vrshr.u64` q0`,` q0`, #`0

- int64x2_t vrshrq_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vrshr.s64` q0`,` q0`, #`0

- uint32x2_t vshrn_n_u64 (uint64x2_t, const int)
  Form of expected instruction(s): `vshrn.i64` d0`,` q0`, #`0

- uint16x4_t vshrn_n_u32 (uint32x4_t, const int)
  Form of expected instruction(s): `vshrn.i32` d0`,` q0`, #`0

- uint8x8_t vshrn_n_u16 (uint16x8_t, const int)
  Form of expected instruction(s): `vshrn.i16` d0`,` q0`, #`0

- int32x2_t vshrn_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vshrn.i64` d0`,` q0`, #`0

- int16x4_t vshrn_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vshrn.i32` d0`,` q0`, #`0

- int8x8_t vshrn_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vshrn.i16` d0`,` q0`, #`0

- uint32x2_t vrshrn_n_u64 (uint64x2_t, const int)
  Form of expected instruction(s): `vrshrn.i64` d0`,` q0`, #`0

- uint16x4_t vrshrn_n_u32 (uint32x4_t, const int)
  Form of expected instruction(s): `vrshrn.i32` d0`,` q0`, #`0

- uint8x8_t vrshrn_n_u16 (uint16x8_t, const int)
  Form of expected instruction(s): `vrshrn.i16` d0`,` q0`, #`0

- int32x2_t vrshrn_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vrshrn.i64` d0`,` q0`, #`0

- int16x4_t vrshrn_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vrshrn.i32` d0`,` q0`, #`0

- int8x8_t vrshrn_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vrshrn.i16` d0`,` q0`, #`0

- uint32x2_t vqshrn_n_u64 (uint64x2_t, const int)
  Form of expected instruction(s): `vqshrn.u64` d0`,` q0`, #`0

- uint16x4_t vqshrn_n_u32 (uint32x4_t, const int)
  Form of expected instruction(s): `vqshrn.u32` d0`,` q0`, #`0

- uint8x8_t vqshrn_n_u16 (uint16x8_t, const int)
  Form of expected instruction(s): `vqshrn.u16` d0`,` q0`, #`0

- int32x2_t vqshrn_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vqshrn.s64` d0`,` q0`, #`0

- int16x4_t vqshrn_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vqshrn.s32` d0`,` q0`, #`0

- int8x8_t vqshrn_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vqshrn.s16` d0`,` q0`, #`0

- uint32x2_t vqrshrn_n_u64 (uint64x2_t, const int)
  Form of expected instruction(s): `vqrshrn.u64` d0`,` q0`, #`0

- uint16x4_t vqrshrn_n_u32 (uint32x4_t, const int)
  Form of expected instruction(s): `vqrshrn.u32` d0`,` q0`, #`0

- uint8x8_t vqrshrn_n_u16 (uint16x8_t, const int)
  Form of expected instruction(s): `vqrshrn.u16` d0`,` q0`, #`0

- int32x2_t vqrshrn_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vqrshrn.s64` d0`,` q0`, #`0

- int16x4_t vqrshrn_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vqrshrn.s32` d0`,` q0`, #`0

- int8x8_t vqrshrn_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vqrshrn.s16` d0`,` q0`, #`0

- uint32x2_t vqshrun_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vqshrun.s64` d0`,` q0`, #`0

- uint16x4_t vqshrun_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vqshrun.s32` d0`,` q0`, #`0

- uint8x8_t vqshrun_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vqshrun.s16` d0`,` q0`, #`0

- uint32x2_t vqrshrun_n_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vqrshrun.s64` d0`,` q0`, #`0

- uint16x4_t vqrshrun_n_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vqrshrun.s32` d0`,` q0`, #`0

- uint8x8_t vqrshrun_n_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vqrshrun.s16` d0`,` q0`, #`0

##### 6.57.6.35 Vector shift right by constant and accumulate

- uint32x2_t vsra_n_u32 (uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vsra.u32` d0`,` d0`, #`0

- uint16x4_t vsra_n_u16 (uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vsra.u16` d0`,` d0`, #`0

- uint8x8_t vsra_n_u8 (uint8x8_t, uint8x8_t, const int)
  Form of expected instruction(s): `vsra.u8` d0`,` d0`, #`0

- int32x2_t vsra_n_s32 (int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vsra.s32` d0`,` d0`, #`0

- int16x4_t vsra_n_s16 (int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vsra.s16` d0`,` d0`, #`0

- int8x8_t vsra_n_s8 (int8x8_t, int8x8_t, const int)
  Form of expected instruction(s): `vsra.s8` d0`,` d0`, #`0

- uint64x1_t vsra_n_u64 (uint64x1_t, uint64x1_t, const int)
  Form of expected instruction(s): `vsra.u64` d0`,` d0`, #`0

- int64x1_t vsra_n_s64 (int64x1_t, int64x1_t, const int)
  Form of expected instruction(s): `vsra.s64` d0`,` d0`, #`0

- uint32x4_t vsraq_n_u32 (uint32x4_t, uint32x4_t, const int)
  Form of expected instruction(s): `vsra.u32` q0`,` q0`, #`0

- uint16x8_t vsraq_n_u16 (uint16x8_t, uint16x8_t, const int)
  Form of expected instruction(s): `vsra.u16` q0`,` q0`, #`0

- uint8x16_t vsraq_n_u8 (uint8x16_t, uint8x16_t, const int)
  Form of expected instruction(s): `vsra.u8` q0`,` q0`, #`0

- int32x4_t vsraq_n_s32 (int32x4_t, int32x4_t, const int)
  Form of expected instruction(s): `vsra.s32` q0`,` q0`, #`0

- int16x8_t vsraq_n_s16 (int16x8_t, int16x8_t, const int)
  Form of expected instruction(s): `vsra.s16` q0`,` q0`, #`0

- int8x16_t vsraq_n_s8 (int8x16_t, int8x16_t, const int)
  Form of expected instruction(s): `vsra.s8` q0`,` q0`, #`0

- uint64x2_t vsraq_n_u64 (uint64x2_t, uint64x2_t, const int)
  Form of expected instruction(s): `vsra.u64` q0`,` q0`, #`0

- int64x2_t vsraq_n_s64 (int64x2_t, int64x2_t, const int)
  Form of expected instruction(s): `vsra.s64` q0`,` q0`, #`0

- uint32x2_t vrsra_n_u32 (uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vrsra.u32` d0`,` d0`, #`0

- uint16x4_t vrsra_n_u16 (uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vrsra.u16` d0`,` d0`, #`0

- uint8x8_t vrsra_n_u8 (uint8x8_t, uint8x8_t, const int)
  Form of expected instruction(s): `vrsra.u8` d0`,` d0`, #`0

- int32x2_t vrsra_n_s32 (int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vrsra.s32` d0`,` d0`, #`0

- int16x4_t vrsra_n_s16 (int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vrsra.s16` d0`,` d0`, #`0

- int8x8_t vrsra_n_s8 (int8x8_t, int8x8_t, const int)
  Form of expected instruction(s): `vrsra.s8` d0`,` d0`, #`0

- uint64x1_t vrsra_n_u64 (uint64x1_t, uint64x1_t, const int)
  Form of expected instruction(s): `vrsra.u64` d0`,` d0`, #`0

- int64x1_t vrsra_n_s64 (int64x1_t, int64x1_t, const int)
  Form of expected instruction(s): `vrsra.s64` d0`,` d0`, #`0

- uint32x4_t vrsraq_n_u32 (uint32x4_t, uint32x4_t, const int)
  Form of expected instruction(s): `vrsra.u32` q0`,` q0`, #`0

- uint16x8_t vrsraq_n_u16 (uint16x8_t, uint16x8_t, const int)
  Form of expected instruction(s): `vrsra.u16` q0`,` q0`, #`0

- uint8x16_t vrsraq_n_u8 (uint8x16_t, uint8x16_t, const int)
  Form of expected instruction(s): `vrsra.u8` q0`,` q0`, #`0

- int32x4_t vrsraq_n_s32 (int32x4_t, int32x4_t, const int)
  Form of expected instruction(s): `vrsra.s32` q0`,` q0`, #`0

- int16x8_t vrsraq_n_s16 (int16x8_t, int16x8_t, const int)
  Form of expected instruction(s): `vrsra.s16` q0`,` q0`, #`0

- int8x16_t vrsraq_n_s8 (int8x16_t, int8x16_t, const int)
  Form of expected instruction(s): `vrsra.s8` q0`,` q0`, #`0

- uint64x2_t vrsraq_n_u64 (uint64x2_t, uint64x2_t, const int)
  Form of expected instruction(s): `vrsra.u64` q0`,` q0`, #`0

- int64x2_t vrsraq_n_s64 (int64x2_t, int64x2_t, const int)
  Form of expected instruction(s): `vrsra.s64` q0`,` q0`, #`0

##### 6.57.6.36 Vector shift right and insert

- poly64x1_t vsri_n_p64 (poly64x1_t, poly64x1_t, const int)
  Form of expected instruction(s): `vsri.64` d0`,` d0`, #`0

- uint32x2_t vsri_n_u32 (uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vsri.32` d0`,` d0`, #`0

- uint16x4_t vsri_n_u16 (uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vsri.16` d0`,` d0`, #`0

- uint8x8_t vsri_n_u8 (uint8x8_t, uint8x8_t, const int)
  Form of expected instruction(s): `vsri.8` d0`,` d0`, #`0

- int32x2_t vsri_n_s32 (int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vsri.32` d0`,` d0`, #`0

- int16x4_t vsri_n_s16 (int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vsri.16` d0`,` d0`, #`0

- int8x8_t vsri_n_s8 (int8x8_t, int8x8_t, const int)
  Form of expected instruction(s): `vsri.8` d0`,` d0`, #`0

- uint64x1_t vsri_n_u64 (uint64x1_t, uint64x1_t, const int)
  Form of expected instruction(s): `vsri.64` d0`,` d0`, #`0

- int64x1_t vsri_n_s64 (int64x1_t, int64x1_t, const int)
  Form of expected instruction(s): `vsri.64` d0`,` d0`, #`0

- poly16x4_t vsri_n_p16 (poly16x4_t, poly16x4_t, const int)
  Form of expected instruction(s): `vsri.16` d0`,` d0`, #`0

- poly8x8_t vsri_n_p8 (poly8x8_t, poly8x8_t, const int)
  Form of expected instruction(s): `vsri.8` d0`,` d0`, #`0

- poly64x2_t vsriq_n_p64 (poly64x2_t, poly64x2_t, const int)
  Form of expected instruction(s): `vsri.64` q0`,` q0`, #`0

- uint32x4_t vsriq_n_u32 (uint32x4_t, uint32x4_t, const int)
  Form of expected instruction(s): `vsri.32` q0`,` q0`, #`0

- uint16x8_t vsriq_n_u16 (uint16x8_t, uint16x8_t, const int)
  Form of expected instruction(s): `vsri.16` q0`,` q0`, #`0

- uint8x16_t vsriq_n_u8 (uint8x16_t, uint8x16_t, const int)
  Form of expected instruction(s): `vsri.8` q0`,` q0`, #`0

- int32x4_t vsriq_n_s32 (int32x4_t, int32x4_t, const int)
  Form of expected instruction(s): `vsri.32` q0`,` q0`, #`0

- int16x8_t vsriq_n_s16 (int16x8_t, int16x8_t, const int)
  Form of expected instruction(s): `vsri.16` q0`,` q0`, #`0

- int8x16_t vsriq_n_s8 (int8x16_t, int8x16_t, const int)
  Form of expected instruction(s): `vsri.8` q0`,` q0`, #`0

- uint64x2_t vsriq_n_u64 (uint64x2_t, uint64x2_t, const int)
  Form of expected instruction(s): `vsri.64` q0`,` q0`, #`0

- int64x2_t vsriq_n_s64 (int64x2_t, int64x2_t, const int)
  Form of expected instruction(s): `vsri.64` q0`,` q0`, #`0

- poly16x8_t vsriq_n_p16 (poly16x8_t, poly16x8_t, const int)
  Form of expected instruction(s): `vsri.16` q0`,` q0`, #`0

- poly8x16_t vsriq_n_p8 (poly8x16_t, poly8x16_t, const int)
  Form of expected instruction(s): `vsri.8` q0`,` q0`, #`0

##### 6.57.6.37 Vector shift left and insert

- poly64x1_t vsli_n_p64 (poly64x1_t, poly64x1_t, const int)
  Form of expected instruction(s): `vsli.64` d0`,` d0`, #`0

- uint32x2_t vsli_n_u32 (uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vsli.32` d0`,` d0`, #`0

- uint16x4_t vsli_n_u16 (uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vsli.16` d0`,` d0`, #`0

- uint8x8_t vsli_n_u8 (uint8x8_t, uint8x8_t, const int)
  Form of expected instruction(s): `vsli.8` d0`,` d0`, #`0

- int32x2_t vsli_n_s32 (int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vsli.32` d0`,` d0`, #`0

- int16x4_t vsli_n_s16 (int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vsli.16` d0`,` d0`, #`0

- int8x8_t vsli_n_s8 (int8x8_t, int8x8_t, const int)
  Form of expected instruction(s): `vsli.8` d0`,` d0`, #`0

- uint64x1_t vsli_n_u64 (uint64x1_t, uint64x1_t, const int)
  Form of expected instruction(s): `vsli.64` d0`,` d0`, #`0

- int64x1_t vsli_n_s64 (int64x1_t, int64x1_t, const int)
  Form of expected instruction(s): `vsli.64` d0`,` d0`, #`0

- poly16x4_t vsli_n_p16 (poly16x4_t, poly16x4_t, const int)
  Form of expected instruction(s): `vsli.16` d0`,` d0`, #`0

- poly8x8_t vsli_n_p8 (poly8x8_t, poly8x8_t, const int)
  Form of expected instruction(s): `vsli.8` d0`,` d0`, #`0

- poly64x2_t vsliq_n_p64 (poly64x2_t, poly64x2_t, const int)
  Form of expected instruction(s): `vsli.64` q0`,` q0`, #`0

- uint32x4_t vsliq_n_u32 (uint32x4_t, uint32x4_t, const int)
  Form of expected instruction(s): `vsli.32` q0`,` q0`, #`0

- uint16x8_t vsliq_n_u16 (uint16x8_t, uint16x8_t, const int)
  Form of expected instruction(s): `vsli.16` q0`,` q0`, #`0

- uint8x16_t vsliq_n_u8 (uint8x16_t, uint8x16_t, const int)
  Form of expected instruction(s): `vsli.8` q0`,` q0`, #`0

- int32x4_t vsliq_n_s32 (int32x4_t, int32x4_t, const int)
  Form of expected instruction(s): `vsli.32` q0`,` q0`, #`0

- int16x8_t vsliq_n_s16 (int16x8_t, int16x8_t, const int)
  Form of expected instruction(s): `vsli.16` q0`,` q0`, #`0

- int8x16_t vsliq_n_s8 (int8x16_t, int8x16_t, const int)
  Form of expected instruction(s): `vsli.8` q0`,` q0`, #`0

- uint64x2_t vsliq_n_u64 (uint64x2_t, uint64x2_t, const int)
  Form of expected instruction(s): `vsli.64` q0`,` q0`, #`0

- int64x2_t vsliq_n_s64 (int64x2_t, int64x2_t, const int)
  Form of expected instruction(s): `vsli.64` q0`,` q0`, #`0

- poly16x8_t vsliq_n_p16 (poly16x8_t, poly16x8_t, const int)
  Form of expected instruction(s): `vsli.16` q0`,` q0`, #`0

- poly8x16_t vsliq_n_p8 (poly8x16_t, poly8x16_t, const int)
  Form of expected instruction(s): `vsli.8` q0`,` q0`, #`0

##### 6.57.6.38 Absolute value

- float32x2_t vabs_f32 (float32x2_t)
  Form of expected instruction(s): `vabs.f32` d0`,` d0

- int32x2_t vabs_s32 (int32x2_t)
  Form of expected instruction(s): `vabs.s32` d0`,` d0

- int16x4_t vabs_s16 (int16x4_t)
  Form of expected instruction(s): `vabs.s16` d0`,` d0

- int8x8_t vabs_s8 (int8x8_t)
  Form of expected instruction(s): `vabs.s8` d0`,` d0

- float32x4_t vabsq_f32 (float32x4_t)
  Form of expected instruction(s): `vabs.f32` q0`,` q0

- int32x4_t vabsq_s32 (int32x4_t)
  Form of expected instruction(s): `vabs.s32` q0`,` q0

- int16x8_t vabsq_s16 (int16x8_t)
  Form of expected instruction(s): `vabs.s16` q0`,` q0

- int8x16_t vabsq_s8 (int8x16_t)
  Form of expected instruction(s): `vabs.s8` q0`,` q0

- int32x2_t vqabs_s32 (int32x2_t)
  Form of expected instruction(s): `vqabs.s32` d0`,` d0

- int16x4_t vqabs_s16 (int16x4_t)
  Form of expected instruction(s): `vqabs.s16` d0`,` d0

- int8x8_t vqabs_s8 (int8x8_t)
  Form of expected instruction(s): `vqabs.s8` d0`,` d0

- int32x4_t vqabsq_s32 (int32x4_t)
  Form of expected instruction(s): `vqabs.s32` q0`,` q0

- int16x8_t vqabsq_s16 (int16x8_t)
  Form of expected instruction(s): `vqabs.s16` q0`,` q0

- int8x16_t vqabsq_s8 (int8x16_t)
  Form of expected instruction(s): `vqabs.s8` q0`,` q0

##### 6.57.6.39 Negation

- float32x2_t vneg_f32 (float32x2_t)
  Form of expected instruction(s): `vneg.f32` d0`,` d0

- int32x2_t vneg_s32 (int32x2_t)
  Form of expected instruction(s): `vneg.s32` d0`,` d0

- int16x4_t vneg_s16 (int16x4_t)
  Form of expected instruction(s): `vneg.s16` d0`,` d0

- int8x8_t vneg_s8 (int8x8_t)
  Form of expected instruction(s): `vneg.s8` d0`,` d0

- float32x4_t vnegq_f32 (float32x4_t)
  Form of expected instruction(s): `vneg.f32` q0`,` q0

- int32x4_t vnegq_s32 (int32x4_t)
  Form of expected instruction(s): `vneg.s32` q0`,` q0

- int16x8_t vnegq_s16 (int16x8_t)
  Form of expected instruction(s): `vneg.s16` q0`,` q0

- int8x16_t vnegq_s8 (int8x16_t)
  Form of expected instruction(s): `vneg.s8` q0`,` q0

- int32x2_t vqneg_s32 (int32x2_t)
  Form of expected instruction(s): `vqneg.s32` d0`,` d0

- int16x4_t vqneg_s16 (int16x4_t)
  Form of expected instruction(s): `vqneg.s16` d0`,` d0

- int8x8_t vqneg_s8 (int8x8_t)
  Form of expected instruction(s): `vqneg.s8` d0`,` d0

- int32x4_t vqnegq_s32 (int32x4_t)
  Form of expected instruction(s): `vqneg.s32` q0`,` q0

- int16x8_t vqnegq_s16 (int16x8_t)
  Form of expected instruction(s): `vqneg.s16` q0`,` q0

- int8x16_t vqnegq_s8 (int8x16_t)
  Form of expected instruction(s): `vqneg.s8` q0`,` q0

##### 6.57.6.40 Bitwise not

- uint32x2_t vmvn_u32 (uint32x2_t)
  Form of expected instruction(s): `vmvn` d0`,` d0

- uint16x4_t vmvn_u16 (uint16x4_t)
  Form of expected instruction(s): `vmvn` d0`,` d0

- uint8x8_t vmvn_u8 (uint8x8_t)
  Form of expected instruction(s): `vmvn` d0`,` d0

- int32x2_t vmvn_s32 (int32x2_t)
  Form of expected instruction(s): `vmvn` d0`,` d0

- int16x4_t vmvn_s16 (int16x4_t)
  Form of expected instruction(s): `vmvn` d0`,` d0

- int8x8_t vmvn_s8 (int8x8_t)
  Form of expected instruction(s): `vmvn` d0`,` d0

- poly8x8_t vmvn_p8 (poly8x8_t)
  Form of expected instruction(s): `vmvn` d0`,` d0

- uint32x4_t vmvnq_u32 (uint32x4_t)
  Form of expected instruction(s): `vmvn` q0`,` q0

- uint16x8_t vmvnq_u16 (uint16x8_t)
  Form of expected instruction(s): `vmvn` q0`,` q0

- uint8x16_t vmvnq_u8 (uint8x16_t)
  Form of expected instruction(s): `vmvn` q0`,` q0

- int32x4_t vmvnq_s32 (int32x4_t)
  Form of expected instruction(s): `vmvn` q0`,` q0

- int16x8_t vmvnq_s16 (int16x8_t)
  Form of expected instruction(s): `vmvn` q0`,` q0

- int8x16_t vmvnq_s8 (int8x16_t)
  Form of expected instruction(s): `vmvn` q0`,` q0

- poly8x16_t vmvnq_p8 (poly8x16_t)
  Form of expected instruction(s): `vmvn` q0`,` q0

##### 6.57.6.41 Count leading sign bits

- int32x2_t vcls_s32 (int32x2_t)
  Form of expected instruction(s): `vcls.s32` d0`,` d0

- int16x4_t vcls_s16 (int16x4_t)
  Form of expected instruction(s): `vcls.s16` d0`,` d0

- int8x8_t vcls_s8 (int8x8_t)
  Form of expected instruction(s): `vcls.s8` d0`,` d0

- int32x4_t vclsq_s32 (int32x4_t)
  Form of expected instruction(s): `vcls.s32` q0`,` q0

- int16x8_t vclsq_s16 (int16x8_t)
  Form of expected instruction(s): `vcls.s16` q0`,` q0

- int8x16_t vclsq_s8 (int8x16_t)
  Form of expected instruction(s): `vcls.s8` q0`,` q0

##### 6.57.6.42 Count leading zeros

- uint32x2_t vclz_u32 (uint32x2_t)
  Form of expected instruction(s): `vclz.i32` d0`,` d0

- uint16x4_t vclz_u16 (uint16x4_t)
  Form of expected instruction(s): `vclz.i16` d0`,` d0

- uint8x8_t vclz_u8 (uint8x8_t)
  Form of expected instruction(s): `vclz.i8` d0`,` d0

- int32x2_t vclz_s32 (int32x2_t)
  Form of expected instruction(s): `vclz.i32` d0`,` d0

- int16x4_t vclz_s16 (int16x4_t)
  Form of expected instruction(s): `vclz.i16` d0`,` d0

- int8x8_t vclz_s8 (int8x8_t)
  Form of expected instruction(s): `vclz.i8` d0`,` d0

- uint32x4_t vclzq_u32 (uint32x4_t)
  Form of expected instruction(s): `vclz.i32` q0`,` q0

- uint16x8_t vclzq_u16 (uint16x8_t)
  Form of expected instruction(s): `vclz.i16` q0`,` q0

- uint8x16_t vclzq_u8 (uint8x16_t)
  Form of expected instruction(s): `vclz.i8` q0`,` q0

- int32x4_t vclzq_s32 (int32x4_t)
  Form of expected instruction(s): `vclz.i32` q0`,` q0

- int16x8_t vclzq_s16 (int16x8_t)
  Form of expected instruction(s): `vclz.i16` q0`,` q0

- int8x16_t vclzq_s8 (int8x16_t)
  Form of expected instruction(s): `vclz.i8` q0`,` q0

##### 6.57.6.43 Count number of set bits

- uint8x8_t vcnt_u8 (uint8x8_t)
  Form of expected instruction(s): `vcnt.8` d0`,` d0

- int8x8_t vcnt_s8 (int8x8_t)
  Form of expected instruction(s): `vcnt.8` d0`,` d0

- poly8x8_t vcnt_p8 (poly8x8_t)
  Form of expected instruction(s): `vcnt.8` d0`,` d0

- uint8x16_t vcntq_u8 (uint8x16_t)
  Form of expected instruction(s): `vcnt.8` q0`,` q0

- int8x16_t vcntq_s8 (int8x16_t)
  Form of expected instruction(s): `vcnt.8` q0`,` q0

- poly8x16_t vcntq_p8 (poly8x16_t)
  Form of expected instruction(s): `vcnt.8` q0`,` q0

##### 6.57.6.44 Reciprocal estimate

- float32x2_t vrecpe_f32 (float32x2_t)
  Form of expected instruction(s): `vrecpe.f32` d0`,` d0

- uint32x2_t vrecpe_u32 (uint32x2_t)
  Form of expected instruction(s): `vrecpe.u32` d0`,` d0

- float32x4_t vrecpeq_f32 (float32x4_t)
  Form of expected instruction(s): `vrecpe.f32` q0`,` q0

- uint32x4_t vrecpeq_u32 (uint32x4_t)
  Form of expected instruction(s): `vrecpe.u32` q0`,` q0

##### 6.57.6.45 Reciprocal square-root estimate

- float32x2_t vrsqrte_f32 (float32x2_t)
  Form of expected instruction(s): `vrsqrte.f32` d0`,` d0

- uint32x2_t vrsqrte_u32 (uint32x2_t)
  Form of expected instruction(s): `vrsqrte.u32` d0`,` d0

- float32x4_t vrsqrteq_f32 (float32x4_t)
  Form of expected instruction(s): `vrsqrte.f32` q0`,` q0

- uint32x4_t vrsqrteq_u32 (uint32x4_t)
  Form of expected instruction(s): `vrsqrte.u32` q0`,` q0

##### 6.57.6.46 Get lanes from a vector

- uint32_t vget_lane_u32 (uint32x2_t, const int)
  Form of expected instruction(s): `vmov.32` r0`,` d0`[`0`]`

- uint16_t vget_lane_u16 (uint16x4_t, const int)
  Form of expected instruction(s): `vmov.u16` r0`,` d0`[`0`]`

- uint8_t vget_lane_u8 (uint8x8_t, const int)
  Form of expected instruction(s): `vmov.u8` r0`,` d0`[`0`]`

- int32_t vget_lane_s32 (int32x2_t, const int)
  Form of expected instruction(s): `vmov.32` r0`,` d0`[`0`]`

- int16_t vget_lane_s16 (int16x4_t, const int)
  Form of expected instruction(s): `vmov.s16` r0`,` d0`[`0`]`

- int8_t vget_lane_s8 (int8x8_t, const int)
  Form of expected instruction(s): `vmov.s8` r0`,` d0`[`0`]`

- float32_t vget_lane_f32 (float32x2_t, const int)
  Form of expected instruction(s): `vmov.32` r0`,` d0`[`0`]`

- poly16_t vget_lane_p16 (poly16x4_t, const int)
  Form of expected instruction(s): `vmov.u16` r0`,` d0`[`0`]`

- poly8_t vget_lane_p8 (poly8x8_t, const int)
  Form of expected instruction(s): `vmov.u8` r0`,` d0`[`0`]`

- uint64_t vget_lane_u64 (uint64x1_t, const int)

- int64_t vget_lane_s64 (int64x1_t, const int)

- uint32_t vgetq_lane_u32 (uint32x4_t, const int)
  Form of expected instruction(s): `vmov.32` r0`,` d0`[`0`]`

- uint16_t vgetq_lane_u16 (uint16x8_t, const int)
  Form of expected instruction(s): `vmov.u16` r0`,` d0`[`0`]`

- uint8_t vgetq_lane_u8 (uint8x16_t, const int)
  Form of expected instruction(s): `vmov.u8` r0`,` d0`[`0`]`

- int32_t vgetq_lane_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vmov.32` r0`,` d0`[`0`]`

- int16_t vgetq_lane_s16 (int16x8_t, const int)
  Form of expected instruction(s): `vmov.s16` r0`,` d0`[`0`]`

- int8_t vgetq_lane_s8 (int8x16_t, const int)
  Form of expected instruction(s): `vmov.s8` r0`,` d0`[`0`]`

- float32_t vgetq_lane_f32 (float32x4_t, const int)
  Form of expected instruction(s): `vmov.32` r0`,` d0`[`0`]`

- poly16_t vgetq_lane_p16 (poly16x8_t, const int)
  Form of expected instruction(s): `vmov.u16` r0`,` d0`[`0`]`

- poly8_t vgetq_lane_p8 (poly8x16_t, const int)
  Form of expected instruction(s): `vmov.u8` r0`,` d0`[`0`]`

- uint64_t vgetq_lane_u64 (uint64x2_t, const int)
  Form of expected instruction(s): `vmov` r0`,` r0`,` d0 or `fmrrd` r0`,` r0`,` d0

- int64_t vgetq_lane_s64 (int64x2_t, const int)
  Form of expected instruction(s): `vmov` r0`,` r0`,` d0 or `fmrrd` r0`,` r0`,` d0

##### 6.57.6.47 Set lanes in a vector

- uint32x2_t vset_lane_u32 (uint32_t, uint32x2_t, const int)
  Form of expected instruction(s): `vmov.32` d0`[`0`],` r0

- uint16x4_t vset_lane_u16 (uint16_t, uint16x4_t, const int)
  Form of expected instruction(s): `vmov.16` d0`[`0`],` r0

- uint8x8_t vset_lane_u8 (uint8_t, uint8x8_t, const int)
  Form of expected instruction(s): `vmov.8` d0`[`0`],` r0

- int32x2_t vset_lane_s32 (int32_t, int32x2_t, const int)
  Form of expected instruction(s): `vmov.32` d0`[`0`],` r0

- int16x4_t vset_lane_s16 (int16_t, int16x4_t, const int)
  Form of expected instruction(s): `vmov.16` d0`[`0`],` r0

- int8x8_t vset_lane_s8 (int8_t, int8x8_t, const int)
  Form of expected instruction(s): `vmov.8` d0`[`0`],` r0

- float32x2_t vset_lane_f32 (float32_t, float32x2_t, const int)
  Form of expected instruction(s): `vmov.32` d0`[`0`],` r0

- poly16x4_t vset_lane_p16 (poly16_t, poly16x4_t, const int)
  Form of expected instruction(s): `vmov.16` d0`[`0`],` r0

- poly8x8_t vset_lane_p8 (poly8_t, poly8x8_t, const int)
  Form of expected instruction(s): `vmov.8` d0`[`0`],` r0

- uint64x1_t vset_lane_u64 (uint64_t, uint64x1_t, const int)

- int64x1_t vset_lane_s64 (int64_t, int64x1_t, const int)

- uint32x4_t vsetq_lane_u32 (uint32_t, uint32x4_t, const int)
  Form of expected instruction(s): `vmov.32` d0`[`0`],` r0

- uint16x8_t vsetq_lane_u16 (uint16_t, uint16x8_t, const int)
  Form of expected instruction(s): `vmov.16` d0`[`0`],` r0

- uint8x16_t vsetq_lane_u8 (uint8_t, uint8x16_t, const int)
  Form of expected instruction(s): `vmov.8` d0`[`0`],` r0

- int32x4_t vsetq_lane_s32 (int32_t, int32x4_t, const int)
  Form of expected instruction(s): `vmov.32` d0`[`0`],` r0

- int16x8_t vsetq_lane_s16 (int16_t, int16x8_t, const int)
  Form of expected instruction(s): `vmov.16` d0`[`0`],` r0

- int8x16_t vsetq_lane_s8 (int8_t, int8x16_t, const int)
  Form of expected instruction(s): `vmov.8` d0`[`0`],` r0

- float32x4_t vsetq_lane_f32 (float32_t, float32x4_t, const int)
  Form of expected instruction(s): `vmov.32` d0`[`0`],` r0

- poly16x8_t vsetq_lane_p16 (poly16_t, poly16x8_t, const int)
  Form of expected instruction(s): `vmov.16` d0`[`0`],` r0

- poly8x16_t vsetq_lane_p8 (poly8_t, poly8x16_t, const int)
  Form of expected instruction(s): `vmov.8` d0`[`0`],` r0

- uint64x2_t vsetq_lane_u64 (uint64_t, uint64x2_t, const int)
  Form of expected instruction(s): `vmov` d0`,` r0`,` r0

- int64x2_t vsetq_lane_s64 (int64_t, int64x2_t, const int)
  Form of expected instruction(s): `vmov` d0`,` r0`,` r0

##### 6.57.6.48 Create vector from literal bit pattern

- poly64x1_t vcreate_p64 (uint64_t)

- uint32x2_t vcreate_u32 (uint64_t)

- uint16x4_t vcreate_u16 (uint64_t)

- uint8x8_t vcreate_u8 (uint64_t)

- int32x2_t vcreate_s32 (uint64_t)

- int16x4_t vcreate_s16 (uint64_t)

- int8x8_t vcreate_s8 (uint64_t)

- uint64x1_t vcreate_u64 (uint64_t)

- int64x1_t vcreate_s64 (uint64_t)

- float32x2_t vcreate_f32 (uint64_t)

- poly16x4_t vcreate_p16 (uint64_t)

- poly8x8_t vcreate_p8 (uint64_t)

##### 6.57.6.49 Set all lanes to the same value

- uint32x2_t vdup_n_u32 (uint32_t)
  Form of expected instruction(s): `vdup.32` d0`,` r0

- uint16x4_t vdup_n_u16 (uint16_t)
  Form of expected instruction(s): `vdup.16` d0`,` r0

- uint8x8_t vdup_n_u8 (uint8_t)
  Form of expected instruction(s): `vdup.8` d0`,` r0

- int32x2_t vdup_n_s32 (int32_t)
  Form of expected instruction(s): `vdup.32` d0`,` r0

- int16x4_t vdup_n_s16 (int16_t)
  Form of expected instruction(s): `vdup.16` d0`,` r0

- int8x8_t vdup_n_s8 (int8_t)
  Form of expected instruction(s): `vdup.8` d0`,` r0

- float32x2_t vdup_n_f32 (float32_t)
  Form of expected instruction(s): `vdup.32` d0`,` r0

- poly16x4_t vdup_n_p16 (poly16_t)
  Form of expected instruction(s): `vdup.16` d0`,` r0

- poly8x8_t vdup_n_p8 (poly8_t)
  Form of expected instruction(s): `vdup.8` d0`,` r0

- poly64x1_t vdup_n_p64 (poly64_t)

- uint64x1_t vdup_n_u64 (uint64_t)

- int64x1_t vdup_n_s64 (int64_t)

- poly64x2_t vdupq_n_p64 (poly64_t)

- uint32x4_t vdupq_n_u32 (uint32_t)
  Form of expected instruction(s): `vdup.32` q0`,` r0

- uint16x8_t vdupq_n_u16 (uint16_t)
  Form of expected instruction(s): `vdup.16` q0`,` r0

- uint8x16_t vdupq_n_u8 (uint8_t)
  Form of expected instruction(s): `vdup.8` q0`,` r0

- int32x4_t vdupq_n_s32 (int32_t)
  Form of expected instruction(s): `vdup.32` q0`,` r0

- int16x8_t vdupq_n_s16 (int16_t)
  Form of expected instruction(s): `vdup.16` q0`,` r0

- int8x16_t vdupq_n_s8 (int8_t)
  Form of expected instruction(s): `vdup.8` q0`,` r0

- float32x4_t vdupq_n_f32 (float32_t)
  Form of expected instruction(s): `vdup.32` q0`,` r0

- poly16x8_t vdupq_n_p16 (poly16_t)
  Form of expected instruction(s): `vdup.16` q0`,` r0

- poly8x16_t vdupq_n_p8 (poly8_t)
  Form of expected instruction(s): `vdup.8` q0`,` r0

- uint64x2_t vdupq_n_u64 (uint64_t)

- int64x2_t vdupq_n_s64 (int64_t)

- uint32x2_t vmov_n_u32 (uint32_t)
  Form of expected instruction(s): `vdup.32` d0`,` r0

- uint16x4_t vmov_n_u16 (uint16_t)
  Form of expected instruction(s): `vdup.16` d0`,` r0

- uint8x8_t vmov_n_u8 (uint8_t)
  Form of expected instruction(s): `vdup.8` d0`,` r0

- int32x2_t vmov_n_s32 (int32_t)
  Form of expected instruction(s): `vdup.32` d0`,` r0

- int16x4_t vmov_n_s16 (int16_t)
  Form of expected instruction(s): `vdup.16` d0`,` r0

- int8x8_t vmov_n_s8 (int8_t)
  Form of expected instruction(s): `vdup.8` d0`,` r0

- float32x2_t vmov_n_f32 (float32_t)
  Form of expected instruction(s): `vdup.32` d0`,` r0

- poly16x4_t vmov_n_p16 (poly16_t)
  Form of expected instruction(s): `vdup.16` d0`,` r0

- poly8x8_t vmov_n_p8 (poly8_t)
  Form of expected instruction(s): `vdup.8` d0`,` r0

- uint64x1_t vmov_n_u64 (uint64_t)

- int64x1_t vmov_n_s64 (int64_t)

- uint32x4_t vmovq_n_u32 (uint32_t)
  Form of expected instruction(s): `vdup.32` q0`,` r0

- uint16x8_t vmovq_n_u16 (uint16_t)
  Form of expected instruction(s): `vdup.16` q0`,` r0

- uint8x16_t vmovq_n_u8 (uint8_t)
  Form of expected instruction(s): `vdup.8` q0`,` r0

- int32x4_t vmovq_n_s32 (int32_t)
  Form of expected instruction(s): `vdup.32` q0`,` r0

- int16x8_t vmovq_n_s16 (int16_t)
  Form of expected instruction(s): `vdup.16` q0`,` r0

- int8x16_t vmovq_n_s8 (int8_t)
  Form of expected instruction(s): `vdup.8` q0`,` r0

- float32x4_t vmovq_n_f32 (float32_t)
  Form of expected instruction(s): `vdup.32` q0`,` r0

- poly16x8_t vmovq_n_p16 (poly16_t)
  Form of expected instruction(s): `vdup.16` q0`,` r0

- poly8x16_t vmovq_n_p8 (poly8_t)
  Form of expected instruction(s): `vdup.8` q0`,` r0

- uint64x2_t vmovq_n_u64 (uint64_t)

- int64x2_t vmovq_n_s64 (int64_t)

- uint32x2_t vdup_lane_u32 (uint32x2_t, const int)
  Form of expected instruction(s): `vdup.32` d0`,` d0`[`0`]`

- uint16x4_t vdup_lane_u16 (uint16x4_t, const int)
  Form of expected instruction(s): `vdup.16` d0`,` d0`[`0`]`

- uint8x8_t vdup_lane_u8 (uint8x8_t, const int)
  Form of expected instruction(s): `vdup.8` d0`,` d0`[`0`]`

- int32x2_t vdup_lane_s32 (int32x2_t, const int)
  Form of expected instruction(s): `vdup.32` d0`,` d0`[`0`]`

- int16x4_t vdup_lane_s16 (int16x4_t, const int)
  Form of expected instruction(s): `vdup.16` d0`,` d0`[`0`]`

- int8x8_t vdup_lane_s8 (int8x8_t, const int)
  Form of expected instruction(s): `vdup.8` d0`,` d0`[`0`]`

- float32x2_t vdup_lane_f32 (float32x2_t, const int)
  Form of expected instruction(s): `vdup.32` d0`,` d0`[`0`]`

- poly16x4_t vdup_lane_p16 (poly16x4_t, const int)
  Form of expected instruction(s): `vdup.16` d0`,` d0`[`0`]`

- poly8x8_t vdup_lane_p8 (poly8x8_t, const int)
  Form of expected instruction(s): `vdup.8` d0`,` d0`[`0`]`

- poly64x1_t vdup_lane_p64 (poly64x1_t, const int)

- uint64x1_t vdup_lane_u64 (uint64x1_t, const int)

- int64x1_t vdup_lane_s64 (int64x1_t, const int)

- uint32x4_t vdupq_lane_u32 (uint32x2_t, const int)
  Form of expected instruction(s): `vdup.32` q0`,` d0`[`0`]`

- uint16x8_t vdupq_lane_u16 (uint16x4_t, const int)
  Form of expected instruction(s): `vdup.16` q0`,` d0`[`0`]`

- uint8x16_t vdupq_lane_u8 (uint8x8_t, const int)
  Form of expected instruction(s): `vdup.8` q0`,` d0`[`0`]`

- int32x4_t vdupq_lane_s32 (int32x2_t, const int)
  Form of expected instruction(s): `vdup.32` q0`,` d0`[`0`]`

- int16x8_t vdupq_lane_s16 (int16x4_t, const int)
  Form of expected instruction(s): `vdup.16` q0`,` d0`[`0`]`

- int8x16_t vdupq_lane_s8 (int8x8_t, const int)
  Form of expected instruction(s): `vdup.8` q0`,` d0`[`0`]`

- float32x4_t vdupq_lane_f32 (float32x2_t, const int)
  Form of expected instruction(s): `vdup.32` q0`,` d0`[`0`]`

- poly16x8_t vdupq_lane_p16 (poly16x4_t, const int)
  Form of expected instruction(s): `vdup.16` q0`,` d0`[`0`]`

- poly8x16_t vdupq_lane_p8 (poly8x8_t, const int)
  Form of expected instruction(s): `vdup.8` q0`,` d0`[`0`]`

- poly64x2_t vdupq_lane_p64 (poly64x1_t, const int)

- uint64x2_t vdupq_lane_u64 (uint64x1_t, const int)

- int64x2_t vdupq_lane_s64 (int64x1_t, const int)

##### 6.57.6.50 Combining vectors

- poly64x2_t vcombine_p64 (poly64x1_t, poly64x1_t)

- uint32x4_t vcombine_u32 (uint32x2_t, uint32x2_t)

- uint16x8_t vcombine_u16 (uint16x4_t, uint16x4_t)

- uint8x16_t vcombine_u8 (uint8x8_t, uint8x8_t)

- int32x4_t vcombine_s32 (int32x2_t, int32x2_t)

- int16x8_t vcombine_s16 (int16x4_t, int16x4_t)

- int8x16_t vcombine_s8 (int8x8_t, int8x8_t)

- uint64x2_t vcombine_u64 (uint64x1_t, uint64x1_t)

- int64x2_t vcombine_s64 (int64x1_t, int64x1_t)

- float32x4_t vcombine_f32 (float32x2_t, float32x2_t)

- poly16x8_t vcombine_p16 (poly16x4_t, poly16x4_t)

- poly8x16_t vcombine_p8 (poly8x8_t, poly8x8_t)

##### 6.57.6.51 Splitting vectors

- poly64x1_t vget_high_p64 (poly64x2_t)

- uint32x2_t vget_high_u32 (uint32x4_t)

- uint16x4_t vget_high_u16 (uint16x8_t)

- uint8x8_t vget_high_u8 (uint8x16_t)

- int32x2_t vget_high_s32 (int32x4_t)

- int16x4_t vget_high_s16 (int16x8_t)

- int8x8_t vget_high_s8 (int8x16_t)

- uint64x1_t vget_high_u64 (uint64x2_t)

- int64x1_t vget_high_s64 (int64x2_t)

- float32x2_t vget_high_f32 (float32x4_t)

- poly16x4_t vget_high_p16 (poly16x8_t)

- poly8x8_t vget_high_p8 (poly8x16_t)

- uint32x2_t vget_low_u32 (uint32x4_t)
  Form of expected instruction(s): `vmov` d0`,` d0

- uint16x4_t vget_low_u16 (uint16x8_t)
  Form of expected instruction(s): `vmov` d0`,` d0

- uint8x8_t vget_low_u8 (uint8x16_t)
  Form of expected instruction(s): `vmov` d0`,` d0

- int32x2_t vget_low_s32 (int32x4_t)
  Form of expected instruction(s): `vmov` d0`,` d0

- int16x4_t vget_low_s16 (int16x8_t)
  Form of expected instruction(s): `vmov` d0`,` d0

- int8x8_t vget_low_s8 (int8x16_t)
  Form of expected instruction(s): `vmov` d0`,` d0

- float32x2_t vget_low_f32 (float32x4_t)
  Form of expected instruction(s): `vmov` d0`,` d0

- poly16x4_t vget_low_p16 (poly16x8_t)
  Form of expected instruction(s): `vmov` d0`,` d0

- poly8x8_t vget_low_p8 (poly8x16_t)
  Form of expected instruction(s): `vmov` d0`,` d0

- poly64x1_t vget_low_p64 (poly64x2_t)

- uint64x1_t vget_low_u64 (uint64x2_t)

- int64x1_t vget_low_s64 (int64x2_t)

##### 6.57.6.52 Conversions

- float32x2_t vcvt_f32_u32 (uint32x2_t)
  Form of expected instruction(s): `vcvt.f32.u32` d0`,` d0

- float32x2_t vcvt_f32_s32 (int32x2_t)
  Form of expected instruction(s): `vcvt.f32.s32` d0`,` d0

- uint32x2_t vcvt_u32_f32 (float32x2_t)
  Form of expected instruction(s): `vcvt.u32.f32` d0`,` d0

- int32x2_t vcvt_s32_f32 (float32x2_t)
  Form of expected instruction(s): `vcvt.s32.f32` d0`,` d0

- float32x4_t vcvtq_f32_u32 (uint32x4_t)
  Form of expected instruction(s): `vcvt.f32.u32` q0`,` q0

- float32x4_t vcvtq_f32_s32 (int32x4_t)
  Form of expected instruction(s): `vcvt.f32.s32` q0`,` q0

- uint32x4_t vcvtq_u32_f32 (float32x4_t)
  Form of expected instruction(s): `vcvt.u32.f32` q0`,` q0

- int32x4_t vcvtq_s32_f32 (float32x4_t)
  Form of expected instruction(s): `vcvt.s32.f32` q0`,` q0

- float16x4_t vcvt_f16_f32 (float32x4_t)
  Form of expected instruction(s): `vcvt.f16.f32` d0`,` q0

- float32x4_t vcvt_f32_f16 (float16x4_t)
  Form of expected instruction(s): `vcvt.f32.f16` q0`,` d0

- float32x2_t vcvt_n_f32_u32 (uint32x2_t, const int)
  Form of expected instruction(s): `vcvt.f32.u32` d0`,` d0`, #`0

- float32x2_t vcvt_n_f32_s32 (int32x2_t, const int)
  Form of expected instruction(s): `vcvt.f32.s32` d0`,` d0`, #`0

- uint32x2_t vcvt_n_u32_f32 (float32x2_t, const int)
  Form of expected instruction(s): `vcvt.u32.f32` d0`,` d0`, #`0

- int32x2_t vcvt_n_s32_f32 (float32x2_t, const int)
  Form of expected instruction(s): `vcvt.s32.f32` d0`,` d0`, #`0

- float32x4_t vcvtq_n_f32_u32 (uint32x4_t, const int)
  Form of expected instruction(s): `vcvt.f32.u32` q0`,` q0`, #`0

- float32x4_t vcvtq_n_f32_s32 (int32x4_t, const int)
  Form of expected instruction(s): `vcvt.f32.s32` q0`,` q0`, #`0

- uint32x4_t vcvtq_n_u32_f32 (float32x4_t, const int)
  Form of expected instruction(s): `vcvt.u32.f32` q0`,` q0`, #`0

- int32x4_t vcvtq_n_s32_f32 (float32x4_t, const int)
  Form of expected instruction(s): `vcvt.s32.f32` q0`,` q0`, #`0

##### 6.57.6.53 Move, single_opcode narrowing

- uint32x2_t vmovn_u64 (uint64x2_t)
  Form of expected instruction(s): `vmovn.i64` d0`,` q0

- uint16x4_t vmovn_u32 (uint32x4_t)
  Form of expected instruction(s): `vmovn.i32` d0`,` q0

- uint8x8_t vmovn_u16 (uint16x8_t)
  Form of expected instruction(s): `vmovn.i16` d0`,` q0

- int32x2_t vmovn_s64 (int64x2_t)
  Form of expected instruction(s): `vmovn.i64` d0`,` q0

- int16x4_t vmovn_s32 (int32x4_t)
  Form of expected instruction(s): `vmovn.i32` d0`,` q0

- int8x8_t vmovn_s16 (int16x8_t)
  Form of expected instruction(s): `vmovn.i16` d0`,` q0

- uint32x2_t vqmovn_u64 (uint64x2_t)
  Form of expected instruction(s): `vqmovn.u64` d0`,` q0

- uint16x4_t vqmovn_u32 (uint32x4_t)
  Form of expected instruction(s): `vqmovn.u32` d0`,` q0

- uint8x8_t vqmovn_u16 (uint16x8_t)
  Form of expected instruction(s): `vqmovn.u16` d0`,` q0

- int32x2_t vqmovn_s64 (int64x2_t)
  Form of expected instruction(s): `vqmovn.s64` d0`,` q0

- int16x4_t vqmovn_s32 (int32x4_t)
  Form of expected instruction(s): `vqmovn.s32` d0`,` q0

- int8x8_t vqmovn_s16 (int16x8_t)
  Form of expected instruction(s): `vqmovn.s16` d0`,` q0

- uint32x2_t vqmovun_s64 (int64x2_t)
  Form of expected instruction(s): `vqmovun.s64` d0`,` q0

- uint16x4_t vqmovun_s32 (int32x4_t)
  Form of expected instruction(s): `vqmovun.s32` d0`,` q0

- uint8x8_t vqmovun_s16 (int16x8_t)
  Form of expected instruction(s): `vqmovun.s16` d0`,` q0

##### 6.57.6.54 Move, single_opcode long

- uint64x2_t vmovl_u32 (uint32x2_t)
  Form of expected instruction(s): `vmovl.u32` q0`,` d0

- uint32x4_t vmovl_u16 (uint16x4_t)
  Form of expected instruction(s): `vmovl.u16` q0`,` d0

- uint16x8_t vmovl_u8 (uint8x8_t)
  Form of expected instruction(s): `vmovl.u8` q0`,` d0

- int64x2_t vmovl_s32 (int32x2_t)
  Form of expected instruction(s): `vmovl.s32` q0`,` d0

- int32x4_t vmovl_s16 (int16x4_t)
  Form of expected instruction(s): `vmovl.s16` q0`,` d0

- int16x8_t vmovl_s8 (int8x8_t)
  Form of expected instruction(s): `vmovl.s8` q0`,` d0

##### 6.57.6.55 Table lookup

- poly8x8_t vtbl1_p8 (poly8x8_t, uint8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`},` d0

- int8x8_t vtbl1_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`},` d0

- uint8x8_t vtbl1_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`},` d0

- poly8x8_t vtbl2_p8 (poly8x8x2_t, uint8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`,` d1`},` d0

- int8x8_t vtbl2_s8 (int8x8x2_t, int8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`,` d1`},` d0

- uint8x8_t vtbl2_u8 (uint8x8x2_t, uint8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`,` d1`},` d0

- poly8x8_t vtbl3_p8 (poly8x8x3_t, uint8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`,` d1`,` d2`},` d0

- int8x8_t vtbl3_s8 (int8x8x3_t, int8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`,` d1`,` d2`},` d0

- uint8x8_t vtbl3_u8 (uint8x8x3_t, uint8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`,` d1`,` d2`},` d0

- poly8x8_t vtbl4_p8 (poly8x8x4_t, uint8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`,` d1`,` d2`,` d3`},` d0

- int8x8_t vtbl4_s8 (int8x8x4_t, int8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`,` d1`,` d2`,` d3`},` d0

- uint8x8_t vtbl4_u8 (uint8x8x4_t, uint8x8_t)
  Form of expected instruction(s): `vtbl.8` d0`, {`d0`,` d1`,` d2`,` d3`},` d0

##### 6.57.6.56 Extended table lookup

- poly8x8_t vtbx1_p8 (poly8x8_t, poly8x8_t, uint8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`},` d0

- int8x8_t vtbx1_s8 (int8x8_t, int8x8_t, int8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`},` d0

- uint8x8_t vtbx1_u8 (uint8x8_t, uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`},` d0

- poly8x8_t vtbx2_p8 (poly8x8_t, poly8x8x2_t, uint8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`,` d1`},` d0

- int8x8_t vtbx2_s8 (int8x8_t, int8x8x2_t, int8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`,` d1`},` d0

- uint8x8_t vtbx2_u8 (uint8x8_t, uint8x8x2_t, uint8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`,` d1`},` d0

- poly8x8_t vtbx3_p8 (poly8x8_t, poly8x8x3_t, uint8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`,` d1`,` d2`},` d0

- int8x8_t vtbx3_s8 (int8x8_t, int8x8x3_t, int8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`,` d1`,` d2`},` d0

- uint8x8_t vtbx3_u8 (uint8x8_t, uint8x8x3_t, uint8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`,` d1`,` d2`},` d0

- poly8x8_t vtbx4_p8 (poly8x8_t, poly8x8x4_t, uint8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`,` d1`,` d2`,` d3`},` d0

- int8x8_t vtbx4_s8 (int8x8_t, int8x8x4_t, int8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`,` d1`,` d2`,` d3`},` d0

- uint8x8_t vtbx4_u8 (uint8x8_t, uint8x8x4_t, uint8x8_t)
  Form of expected instruction(s): `vtbx.8` d0`, {`d0`,` d1`,` d2`,` d3`},` d0

##### 6.57.6.57 Multiply, lane

- float32x2_t vmul_lane_f32 (float32x2_t, float32x2_t, const int)
  Form of expected instruction(s): `vmul.f32` d0`,` d0`,` d0`[`0`]`

- uint32x2_t vmul_lane_u32 (uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vmul.i32` d0`,` d0`,` d0`[`0`]`

- uint16x4_t vmul_lane_u16 (uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vmul.i16` d0`,` d0`,` d0`[`0`]`

- int32x2_t vmul_lane_s32 (int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vmul.i32` d0`,` d0`,` d0`[`0`]`

- int16x4_t vmul_lane_s16 (int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vmul.i16` d0`,` d0`,` d0`[`0`]`

- float32x4_t vmulq_lane_f32 (float32x4_t, float32x2_t, const int)
  Form of expected instruction(s): `vmul.f32` q0`,` q0`,` d0`[`0`]`

- uint32x4_t vmulq_lane_u32 (uint32x4_t, uint32x2_t, const int)
  Form of expected instruction(s): `vmul.i32` q0`,` q0`,` d0`[`0`]`

- uint16x8_t vmulq_lane_u16 (uint16x8_t, uint16x4_t, const int)
  Form of expected instruction(s): `vmul.i16` q0`,` q0`,` d0`[`0`]`

- int32x4_t vmulq_lane_s32 (int32x4_t, int32x2_t, const int)
  Form of expected instruction(s): `vmul.i32` q0`,` q0`,` d0`[`0`]`

- int16x8_t vmulq_lane_s16 (int16x8_t, int16x4_t, const int)
  Form of expected instruction(s): `vmul.i16` q0`,` q0`,` d0`[`0`]`

##### 6.57.6.58 Long multiply, lane

- uint64x2_t vmull_lane_u32 (uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vmull.u32` q0`,` d0`,` d0`[`0`]`

- uint32x4_t vmull_lane_u16 (uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vmull.u16` q0`,` d0`,` d0`[`0`]`

- int64x2_t vmull_lane_s32 (int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vmull.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vmull_lane_s16 (int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vmull.s16` q0`,` d0`,` d0`[`0`]`

##### 6.57.6.59 Saturating doubling long multiply, lane

- int64x2_t vqdmull_lane_s32 (int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vqdmull.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vqdmull_lane_s16 (int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vqdmull.s16` q0`,` d0`,` d0`[`0`]`

##### 6.57.6.60 Saturating doubling multiply high, lane

- int32x4_t vqdmulhq_lane_s32 (int32x4_t, int32x2_t, const int)
  Form of expected instruction(s): `vqdmulh.s32` q0`,` q0`,` d0`[`0`]`

- int16x8_t vqdmulhq_lane_s16 (int16x8_t, int16x4_t, const int)
  Form of expected instruction(s): `vqdmulh.s16` q0`,` q0`,` d0`[`0`]`

- int32x2_t vqdmulh_lane_s32 (int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vqdmulh.s32` d0`,` d0`,` d0`[`0`]`

- int16x4_t vqdmulh_lane_s16 (int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vqdmulh.s16` d0`,` d0`,` d0`[`0`]`

- int32x4_t vqrdmulhq_lane_s32 (int32x4_t, int32x2_t, const int)
  Form of expected instruction(s): `vqrdmulh.s32` q0`,` q0`,` d0`[`0`]`

- int16x8_t vqrdmulhq_lane_s16 (int16x8_t, int16x4_t, const int)
  Form of expected instruction(s): `vqrdmulh.s16` q0`,` q0`,` d0`[`0`]`

- int32x2_t vqrdmulh_lane_s32 (int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vqrdmulh.s32` d0`,` d0`,` d0`[`0`]`

- int16x4_t vqrdmulh_lane_s16 (int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vqrdmulh.s16` d0`,` d0`,` d0`[`0`]`

##### 6.57.6.61 Multiply-accumulate, lane

- float32x2_t vmla_lane_f32 (float32x2_t, float32x2_t, float32x2_t, const int)
  Form of expected instruction(s): `vmla.f32` d0`,` d0`,` d0`[`0`]`

- uint32x2_t vmla_lane_u32 (uint32x2_t, uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vmla.i32` d0`,` d0`,` d0`[`0`]`

- uint16x4_t vmla_lane_u16 (uint16x4_t, uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vmla.i16` d0`,` d0`,` d0`[`0`]`

- int32x2_t vmla_lane_s32 (int32x2_t, int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vmla.i32` d0`,` d0`,` d0`[`0`]`

- int16x4_t vmla_lane_s16 (int16x4_t, int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vmla.i16` d0`,` d0`,` d0`[`0`]`

- float32x4_t vmlaq_lane_f32 (float32x4_t, float32x4_t, float32x2_t, const int)
  Form of expected instruction(s): `vmla.f32` q0`,` q0`,` d0`[`0`]`

- uint32x4_t vmlaq_lane_u32 (uint32x4_t, uint32x4_t, uint32x2_t, const int)
  Form of expected instruction(s): `vmla.i32` q0`,` q0`,` d0`[`0`]`

- uint16x8_t vmlaq_lane_u16 (uint16x8_t, uint16x8_t, uint16x4_t, const int)
  Form of expected instruction(s): `vmla.i16` q0`,` q0`,` d0`[`0`]`

- int32x4_t vmlaq_lane_s32 (int32x4_t, int32x4_t, int32x2_t, const int)
  Form of expected instruction(s): `vmla.i32` q0`,` q0`,` d0`[`0`]`

- int16x8_t vmlaq_lane_s16 (int16x8_t, int16x8_t, int16x4_t, const int)
  Form of expected instruction(s): `vmla.i16` q0`,` q0`,` d0`[`0`]`

- uint64x2_t vmlal_lane_u32 (uint64x2_t, uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vmlal.u32` q0`,` d0`,` d0`[`0`]`

- uint32x4_t vmlal_lane_u16 (uint32x4_t, uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vmlal.u16` q0`,` d0`,` d0`[`0`]`

- int64x2_t vmlal_lane_s32 (int64x2_t, int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vmlal.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vmlal_lane_s16 (int32x4_t, int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vmlal.s16` q0`,` d0`,` d0`[`0`]`

- int64x2_t vqdmlal_lane_s32 (int64x2_t, int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vqdmlal.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vqdmlal_lane_s16 (int32x4_t, int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vqdmlal.s16` q0`,` d0`,` d0`[`0`]`

##### 6.57.6.62 Multiply-subtract, lane

- float32x2_t vmls_lane_f32 (float32x2_t, float32x2_t, float32x2_t, const int)
  Form of expected instruction(s): `vmls.f32` d0`,` d0`,` d0`[`0`]`

- uint32x2_t vmls_lane_u32 (uint32x2_t, uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vmls.i32` d0`,` d0`,` d0`[`0`]`

- uint16x4_t vmls_lane_u16 (uint16x4_t, uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vmls.i16` d0`,` d0`,` d0`[`0`]`

- int32x2_t vmls_lane_s32 (int32x2_t, int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vmls.i32` d0`,` d0`,` d0`[`0`]`

- int16x4_t vmls_lane_s16 (int16x4_t, int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vmls.i16` d0`,` d0`,` d0`[`0`]`

- float32x4_t vmlsq_lane_f32 (float32x4_t, float32x4_t, float32x2_t, const int)
  Form of expected instruction(s): `vmls.f32` q0`,` q0`,` d0`[`0`]`

- uint32x4_t vmlsq_lane_u32 (uint32x4_t, uint32x4_t, uint32x2_t, const int)
  Form of expected instruction(s): `vmls.i32` q0`,` q0`,` d0`[`0`]`

- uint16x8_t vmlsq_lane_u16 (uint16x8_t, uint16x8_t, uint16x4_t, const int)
  Form of expected instruction(s): `vmls.i16` q0`,` q0`,` d0`[`0`]`

- int32x4_t vmlsq_lane_s32 (int32x4_t, int32x4_t, int32x2_t, const int)
  Form of expected instruction(s): `vmls.i32` q0`,` q0`,` d0`[`0`]`

- int16x8_t vmlsq_lane_s16 (int16x8_t, int16x8_t, int16x4_t, const int)
  Form of expected instruction(s): `vmls.i16` q0`,` q0`,` d0`[`0`]`

- uint64x2_t vmlsl_lane_u32 (uint64x2_t, uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vmlsl.u32` q0`,` d0`,` d0`[`0`]`

- uint32x4_t vmlsl_lane_u16 (uint32x4_t, uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vmlsl.u16` q0`,` d0`,` d0`[`0`]`

- int64x2_t vmlsl_lane_s32 (int64x2_t, int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vmlsl.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vmlsl_lane_s16 (int32x4_t, int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vmlsl.s16` q0`,` d0`,` d0`[`0`]`

- int64x2_t vqdmlsl_lane_s32 (int64x2_t, int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vqdmlsl.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vqdmlsl_lane_s16 (int32x4_t, int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vqdmlsl.s16` q0`,` d0`,` d0`[`0`]`

##### 6.57.6.63 Vector multiply by scalar

- float32x2_t vmul_n_f32 (float32x2_t, float32_t)
  Form of expected instruction(s): `vmul.f32` d0`,` d0`,` d0`[`0`]`

- uint32x2_t vmul_n_u32 (uint32x2_t, uint32_t)
  Form of expected instruction(s): `vmul.i32` d0`,` d0`,` d0`[`0`]`

- uint16x4_t vmul_n_u16 (uint16x4_t, uint16_t)
  Form of expected instruction(s): `vmul.i16` d0`,` d0`,` d0`[`0`]`

- int32x2_t vmul_n_s32 (int32x2_t, int32_t)
  Form of expected instruction(s): `vmul.i32` d0`,` d0`,` d0`[`0`]`

- int16x4_t vmul_n_s16 (int16x4_t, int16_t)
  Form of expected instruction(s): `vmul.i16` d0`,` d0`,` d0`[`0`]`

- float32x4_t vmulq_n_f32 (float32x4_t, float32_t)
  Form of expected instruction(s): `vmul.f32` q0`,` q0`,` d0`[`0`]`

- uint32x4_t vmulq_n_u32 (uint32x4_t, uint32_t)
  Form of expected instruction(s): `vmul.i32` q0`,` q0`,` d0`[`0`]`

- uint16x8_t vmulq_n_u16 (uint16x8_t, uint16_t)
  Form of expected instruction(s): `vmul.i16` q0`,` q0`,` d0`[`0`]`

- int32x4_t vmulq_n_s32 (int32x4_t, int32_t)
  Form of expected instruction(s): `vmul.i32` q0`,` q0`,` d0`[`0`]`

- int16x8_t vmulq_n_s16 (int16x8_t, int16_t)
  Form of expected instruction(s): `vmul.i16` q0`,` q0`,` d0`[`0`]`

##### 6.57.6.64 Vector long multiply by scalar

- uint64x2_t vmull_n_u32 (uint32x2_t, uint32_t)
  Form of expected instruction(s): `vmull.u32` q0`,` d0`,` d0`[`0`]`

- uint32x4_t vmull_n_u16 (uint16x4_t, uint16_t)
  Form of expected instruction(s): `vmull.u16` q0`,` d0`,` d0`[`0`]`

- int64x2_t vmull_n_s32 (int32x2_t, int32_t)
  Form of expected instruction(s): `vmull.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vmull_n_s16 (int16x4_t, int16_t)
  Form of expected instruction(s): `vmull.s16` q0`,` d0`,` d0`[`0`]`

##### 6.57.6.65 Vector saturating doubling long multiply by scalar

- int64x2_t vqdmull_n_s32 (int32x2_t, int32_t)
  Form of expected instruction(s): `vqdmull.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vqdmull_n_s16 (int16x4_t, int16_t)
  Form of expected instruction(s): `vqdmull.s16` q0`,` d0`,` d0`[`0`]`

##### 6.57.6.66 Vector saturating doubling multiply high by scalar

- int32x4_t vqdmulhq_n_s32 (int32x4_t, int32_t)
  Form of expected instruction(s): `vqdmulh.s32` q0`,` q0`,` d0`[`0`]`

- int16x8_t vqdmulhq_n_s16 (int16x8_t, int16_t)
  Form of expected instruction(s): `vqdmulh.s16` q0`,` q0`,` d0`[`0`]`

- int32x2_t vqdmulh_n_s32 (int32x2_t, int32_t)
  Form of expected instruction(s): `vqdmulh.s32` d0`,` d0`,` d0`[`0`]`

- int16x4_t vqdmulh_n_s16 (int16x4_t, int16_t)
  Form of expected instruction(s): `vqdmulh.s16` d0`,` d0`,` d0`[`0`]`

- int32x4_t vqrdmulhq_n_s32 (int32x4_t, int32_t)
  Form of expected instruction(s): `vqrdmulh.s32` q0`,` q0`,` d0`[`0`]`

- int16x8_t vqrdmulhq_n_s16 (int16x8_t, int16_t)
  Form of expected instruction(s): `vqrdmulh.s16` q0`,` q0`,` d0`[`0`]`

- int32x2_t vqrdmulh_n_s32 (int32x2_t, int32_t)
  Form of expected instruction(s): `vqrdmulh.s32` d0`,` d0`,` d0`[`0`]`

- int16x4_t vqrdmulh_n_s16 (int16x4_t, int16_t)
  Form of expected instruction(s): `vqrdmulh.s16` d0`,` d0`,` d0`[`0`]`

##### 6.57.6.67 Vector multiply-accumulate by scalar

- float32x2_t vmla_n_f32 (float32x2_t, float32x2_t, float32_t)
  Form of expected instruction(s): `vmla.f32` d0`,` d0`,` d0`[`0`]`

- uint32x2_t vmla_n_u32 (uint32x2_t, uint32x2_t, uint32_t)
  Form of expected instruction(s): `vmla.i32` d0`,` d0`,` d0`[`0`]`

- uint16x4_t vmla_n_u16 (uint16x4_t, uint16x4_t, uint16_t)
  Form of expected instruction(s): `vmla.i16` d0`,` d0`,` d0`[`0`]`

- int32x2_t vmla_n_s32 (int32x2_t, int32x2_t, int32_t)
  Form of expected instruction(s): `vmla.i32` d0`,` d0`,` d0`[`0`]`

- int16x4_t vmla_n_s16 (int16x4_t, int16x4_t, int16_t)
  Form of expected instruction(s): `vmla.i16` d0`,` d0`,` d0`[`0`]`

- float32x4_t vmlaq_n_f32 (float32x4_t, float32x4_t, float32_t)
  Form of expected instruction(s): `vmla.f32` q0`,` q0`,` d0`[`0`]`

- uint32x4_t vmlaq_n_u32 (uint32x4_t, uint32x4_t, uint32_t)
  Form of expected instruction(s): `vmla.i32` q0`,` q0`,` d0`[`0`]`

- uint16x8_t vmlaq_n_u16 (uint16x8_t, uint16x8_t, uint16_t)
  Form of expected instruction(s): `vmla.i16` q0`,` q0`,` d0`[`0`]`

- int32x4_t vmlaq_n_s32 (int32x4_t, int32x4_t, int32_t)
  Form of expected instruction(s): `vmla.i32` q0`,` q0`,` d0`[`0`]`

- int16x8_t vmlaq_n_s16 (int16x8_t, int16x8_t, int16_t)
  Form of expected instruction(s): `vmla.i16` q0`,` q0`,` d0`[`0`]`

- uint64x2_t vmlal_n_u32 (uint64x2_t, uint32x2_t, uint32_t)
  Form of expected instruction(s): `vmlal.u32` q0`,` d0`,` d0`[`0`]`

- uint32x4_t vmlal_n_u16 (uint32x4_t, uint16x4_t, uint16_t)
  Form of expected instruction(s): `vmlal.u16` q0`,` d0`,` d0`[`0`]`

- int64x2_t vmlal_n_s32 (int64x2_t, int32x2_t, int32_t)
  Form of expected instruction(s): `vmlal.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vmlal_n_s16 (int32x4_t, int16x4_t, int16_t)
  Form of expected instruction(s): `vmlal.s16` q0`,` d0`,` d0`[`0`]`

- int64x2_t vqdmlal_n_s32 (int64x2_t, int32x2_t, int32_t)
  Form of expected instruction(s): `vqdmlal.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vqdmlal_n_s16 (int32x4_t, int16x4_t, int16_t)
  Form of expected instruction(s): `vqdmlal.s16` q0`,` d0`,` d0`[`0`]`

##### 6.57.6.68 Vector multiply-subtract by scalar

- float32x2_t vmls_n_f32 (float32x2_t, float32x2_t, float32_t)
  Form of expected instruction(s): `vmls.f32` d0`,` d0`,` d0`[`0`]`

- uint32x2_t vmls_n_u32 (uint32x2_t, uint32x2_t, uint32_t)
  Form of expected instruction(s): `vmls.i32` d0`,` d0`,` d0`[`0`]`

- uint16x4_t vmls_n_u16 (uint16x4_t, uint16x4_t, uint16_t)
  Form of expected instruction(s): `vmls.i16` d0`,` d0`,` d0`[`0`]`

- int32x2_t vmls_n_s32 (int32x2_t, int32x2_t, int32_t)
  Form of expected instruction(s): `vmls.i32` d0`,` d0`,` d0`[`0`]`

- int16x4_t vmls_n_s16 (int16x4_t, int16x4_t, int16_t)
  Form of expected instruction(s): `vmls.i16` d0`,` d0`,` d0`[`0`]`

- float32x4_t vmlsq_n_f32 (float32x4_t, float32x4_t, float32_t)
  Form of expected instruction(s): `vmls.f32` q0`,` q0`,` d0`[`0`]`

- uint32x4_t vmlsq_n_u32 (uint32x4_t, uint32x4_t, uint32_t)
  Form of expected instruction(s): `vmls.i32` q0`,` q0`,` d0`[`0`]`

- uint16x8_t vmlsq_n_u16 (uint16x8_t, uint16x8_t, uint16_t)
  Form of expected instruction(s): `vmls.i16` q0`,` q0`,` d0`[`0`]`

- int32x4_t vmlsq_n_s32 (int32x4_t, int32x4_t, int32_t)
  Form of expected instruction(s): `vmls.i32` q0`,` q0`,` d0`[`0`]`

- int16x8_t vmlsq_n_s16 (int16x8_t, int16x8_t, int16_t)
  Form of expected instruction(s): `vmls.i16` q0`,` q0`,` d0`[`0`]`

- uint64x2_t vmlsl_n_u32 (uint64x2_t, uint32x2_t, uint32_t)
  Form of expected instruction(s): `vmlsl.u32` q0`,` d0`,` d0`[`0`]`

- uint32x4_t vmlsl_n_u16 (uint32x4_t, uint16x4_t, uint16_t)
  Form of expected instruction(s): `vmlsl.u16` q0`,` d0`,` d0`[`0`]`

- int64x2_t vmlsl_n_s32 (int64x2_t, int32x2_t, int32_t)
  Form of expected instruction(s): `vmlsl.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vmlsl_n_s16 (int32x4_t, int16x4_t, int16_t)
  Form of expected instruction(s): `vmlsl.s16` q0`,` d0`,` d0`[`0`]`

- int64x2_t vqdmlsl_n_s32 (int64x2_t, int32x2_t, int32_t)
  Form of expected instruction(s): `vqdmlsl.s32` q0`,` d0`,` d0`[`0`]`

- int32x4_t vqdmlsl_n_s16 (int32x4_t, int16x4_t, int16_t)
  Form of expected instruction(s): `vqdmlsl.s16` q0`,` d0`,` d0`[`0`]`

##### 6.57.6.69 Vector extract

- poly64x1_t vext_p64 (poly64x1_t, poly64x1_t, const int)
  Form of expected instruction(s): `vext.64` d0`,` d0`,` d0`, #`0

- uint32x2_t vext_u32 (uint32x2_t, uint32x2_t, const int)
  Form of expected instruction(s): `vext.32` d0`,` d0`,` d0`, #`0

- uint16x4_t vext_u16 (uint16x4_t, uint16x4_t, const int)
  Form of expected instruction(s): `vext.16` d0`,` d0`,` d0`, #`0

- uint8x8_t vext_u8 (uint8x8_t, uint8x8_t, const int)
  Form of expected instruction(s): `vext.8` d0`,` d0`,` d0`, #`0

- int32x2_t vext_s32 (int32x2_t, int32x2_t, const int)
  Form of expected instruction(s): `vext.32` d0`,` d0`,` d0`, #`0

- int16x4_t vext_s16 (int16x4_t, int16x4_t, const int)
  Form of expected instruction(s): `vext.16` d0`,` d0`,` d0`, #`0

- int8x8_t vext_s8 (int8x8_t, int8x8_t, const int)
  Form of expected instruction(s): `vext.8` d0`,` d0`,` d0`, #`0

- uint64x1_t vext_u64 (uint64x1_t, uint64x1_t, const int)
  Form of expected instruction(s): `vext.64` d0`,` d0`,` d0`, #`0

- int64x1_t vext_s64 (int64x1_t, int64x1_t, const int)
  Form of expected instruction(s): `vext.64` d0`,` d0`,` d0`, #`0

- float32x2_t vext_f32 (float32x2_t, float32x2_t, const int)
  Form of expected instruction(s): `vext.32` d0`,` d0`,` d0`, #`0

- poly16x4_t vext_p16 (poly16x4_t, poly16x4_t, const int)
  Form of expected instruction(s): `vext.16` d0`,` d0`,` d0`, #`0

- poly8x8_t vext_p8 (poly8x8_t, poly8x8_t, const int)
  Form of expected instruction(s): `vext.8` d0`,` d0`,` d0`, #`0

- poly64x2_t vextq_p64 (poly64x2_t, poly64x2_t, const int)
  Form of expected instruction(s): `vext.64` q0`,` q0`,` q0`, #`0

- uint32x4_t vextq_u32 (uint32x4_t, uint32x4_t, const int)
  Form of expected instruction(s): `vext.32` q0`,` q0`,` q0`, #`0

- uint16x8_t vextq_u16 (uint16x8_t, uint16x8_t, const int)
  Form of expected instruction(s): `vext.16` q0`,` q0`,` q0`, #`0

- uint8x16_t vextq_u8 (uint8x16_t, uint8x16_t, const int)
  Form of expected instruction(s): `vext.8` q0`,` q0`,` q0`, #`0

- int32x4_t vextq_s32 (int32x4_t, int32x4_t, const int)
  Form of expected instruction(s): `vext.32` q0`,` q0`,` q0`, #`0

- int16x8_t vextq_s16 (int16x8_t, int16x8_t, const int)
  Form of expected instruction(s): `vext.16` q0`,` q0`,` q0`, #`0

- int8x16_t vextq_s8 (int8x16_t, int8x16_t, const int)
  Form of expected instruction(s): `vext.8` q0`,` q0`,` q0`, #`0

- uint64x2_t vextq_u64 (uint64x2_t, uint64x2_t, const int)
  Form of expected instruction(s): `vext.64` q0`,` q0`,` q0`, #`0

- int64x2_t vextq_s64 (int64x2_t, int64x2_t, const int)
  Form of expected instruction(s): `vext.64` q0`,` q0`,` q0`, #`0

- float32x4_t vextq_f32 (float32x4_t, float32x4_t, const int)
  Form of expected instruction(s): `vext.32` q0`,` q0`,` q0`, #`0

- poly16x8_t vextq_p16 (poly16x8_t, poly16x8_t, const int)
  Form of expected instruction(s): `vext.16` q0`,` q0`,` q0`, #`0

- poly8x16_t vextq_p8 (poly8x16_t, poly8x16_t, const int)
  Form of expected instruction(s): `vext.8` q0`,` q0`,` q0`, #`0

##### 6.57.6.70 Reverse elements

- uint32x2_t vrev64_u32 (uint32x2_t)
  Form of expected instruction(s): `vrev64.32` d0`,` d0

- uint16x4_t vrev64_u16 (uint16x4_t)
  Form of expected instruction(s): `vrev64.16` d0`,` d0

- uint8x8_t vrev64_u8 (uint8x8_t)
  Form of expected instruction(s): `vrev64.8` d0`,` d0

- int32x2_t vrev64_s32 (int32x2_t)
  Form of expected instruction(s): `vrev64.32` d0`,` d0

- int16x4_t vrev64_s16 (int16x4_t)
  Form of expected instruction(s): `vrev64.16` d0`,` d0

- int8x8_t vrev64_s8 (int8x8_t)
  Form of expected instruction(s): `vrev64.8` d0`,` d0

- float32x2_t vrev64_f32 (float32x2_t)
  Form of expected instruction(s): `vrev64.32` d0`,` d0

- poly16x4_t vrev64_p16 (poly16x4_t)
  Form of expected instruction(s): `vrev64.16` d0`,` d0

- poly8x8_t vrev64_p8 (poly8x8_t)
  Form of expected instruction(s): `vrev64.8` d0`,` d0

- uint32x4_t vrev64q_u32 (uint32x4_t)
  Form of expected instruction(s): `vrev64.32` q0`,` q0

- uint16x8_t vrev64q_u16 (uint16x8_t)
  Form of expected instruction(s): `vrev64.16` q0`,` q0

- uint8x16_t vrev64q_u8 (uint8x16_t)
  Form of expected instruction(s): `vrev64.8` q0`,` q0

- int32x4_t vrev64q_s32 (int32x4_t)
  Form of expected instruction(s): `vrev64.32` q0`,` q0

- int16x8_t vrev64q_s16 (int16x8_t)
  Form of expected instruction(s): `vrev64.16` q0`,` q0

- int8x16_t vrev64q_s8 (int8x16_t)
  Form of expected instruction(s): `vrev64.8` q0`,` q0

- float32x4_t vrev64q_f32 (float32x4_t)
  Form of expected instruction(s): `vrev64.32` q0`,` q0

- poly16x8_t vrev64q_p16 (poly16x8_t)
  Form of expected instruction(s): `vrev64.16` q0`,` q0

- poly8x16_t vrev64q_p8 (poly8x16_t)
  Form of expected instruction(s): `vrev64.8` q0`,` q0

- uint16x4_t vrev32_u16 (uint16x4_t)
  Form of expected instruction(s): `vrev32.16` d0`,` d0

- int16x4_t vrev32_s16 (int16x4_t)
  Form of expected instruction(s): `vrev32.16` d0`,` d0

- uint8x8_t vrev32_u8 (uint8x8_t)
  Form of expected instruction(s): `vrev32.8` d0`,` d0

- int8x8_t vrev32_s8 (int8x8_t)
  Form of expected instruction(s): `vrev32.8` d0`,` d0

- poly16x4_t vrev32_p16 (poly16x4_t)
  Form of expected instruction(s): `vrev32.16` d0`,` d0

- poly8x8_t vrev32_p8 (poly8x8_t)
  Form of expected instruction(s): `vrev32.8` d0`,` d0

- uint16x8_t vrev32q_u16 (uint16x8_t)
  Form of expected instruction(s): `vrev32.16` q0`,` q0

- int16x8_t vrev32q_s16 (int16x8_t)
  Form of expected instruction(s): `vrev32.16` q0`,` q0

- uint8x16_t vrev32q_u8 (uint8x16_t)
  Form of expected instruction(s): `vrev32.8` q0`,` q0

- int8x16_t vrev32q_s8 (int8x16_t)
  Form of expected instruction(s): `vrev32.8` q0`,` q0

- poly16x8_t vrev32q_p16 (poly16x8_t)
  Form of expected instruction(s): `vrev32.16` q0`,` q0

- poly8x16_t vrev32q_p8 (poly8x16_t)
  Form of expected instruction(s): `vrev32.8` q0`,` q0

- uint8x8_t vrev16_u8 (uint8x8_t)
  Form of expected instruction(s): `vrev16.8` d0`,` d0

- int8x8_t vrev16_s8 (int8x8_t)
  Form of expected instruction(s): `vrev16.8` d0`,` d0

- poly8x8_t vrev16_p8 (poly8x8_t)
  Form of expected instruction(s): `vrev16.8` d0`,` d0

- uint8x16_t vrev16q_u8 (uint8x16_t)
  Form of expected instruction(s): `vrev16.8` q0`,` q0

- int8x16_t vrev16q_s8 (int8x16_t)
  Form of expected instruction(s): `vrev16.8` q0`,` q0

- poly8x16_t vrev16q_p8 (poly8x16_t)
  Form of expected instruction(s): `vrev16.8` q0`,` q0

##### 6.57.6.71 Bit selection

- poly64x1_t vbsl_p64 (uint64x1_t, poly64x1_t, poly64x1_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- uint32x2_t vbsl_u32 (uint32x2_t, uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- uint16x4_t vbsl_u16 (uint16x4_t, uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- uint8x8_t vbsl_u8 (uint8x8_t, uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- int32x2_t vbsl_s32 (uint32x2_t, int32x2_t, int32x2_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- int16x4_t vbsl_s16 (uint16x4_t, int16x4_t, int16x4_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- int8x8_t vbsl_s8 (uint8x8_t, int8x8_t, int8x8_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- uint64x1_t vbsl_u64 (uint64x1_t, uint64x1_t, uint64x1_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- int64x1_t vbsl_s64 (uint64x1_t, int64x1_t, int64x1_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- float32x2_t vbsl_f32 (uint32x2_t, float32x2_t, float32x2_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- poly16x4_t vbsl_p16 (uint16x4_t, poly16x4_t, poly16x4_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- poly8x8_t vbsl_p8 (uint8x8_t, poly8x8_t, poly8x8_t)
  Form of expected instruction(s): `vbsl` d0`,` d0`,` d0 or `vbit` d0`,` d0`,` d0 or `vbif` d0`,` d0`,` d0

- poly64x2_t vbslq_p64 (uint64x2_t, poly64x2_t, poly64x2_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- uint32x4_t vbslq_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- uint16x8_t vbslq_u16 (uint16x8_t, uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- uint8x16_t vbslq_u8 (uint8x16_t, uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- int32x4_t vbslq_s32 (uint32x4_t, int32x4_t, int32x4_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- int16x8_t vbslq_s16 (uint16x8_t, int16x8_t, int16x8_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- int8x16_t vbslq_s8 (uint8x16_t, int8x16_t, int8x16_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- uint64x2_t vbslq_u64 (uint64x2_t, uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- int64x2_t vbslq_s64 (uint64x2_t, int64x2_t, int64x2_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- float32x4_t vbslq_f32 (uint32x4_t, float32x4_t, float32x4_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- poly16x8_t vbslq_p16 (uint16x8_t, poly16x8_t, poly16x8_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

- poly8x16_t vbslq_p8 (uint8x16_t, poly8x16_t, poly8x16_t)
  Form of expected instruction(s): `vbsl` q0`,` q0`,` q0 or `vbit` q0`,` q0`,` q0 or `vbif` q0`,` q0`,` q0

##### 6.57.6.72 Transpose elements

- uint16x4x2_t vtrn_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vtrn.16` d0`,` d1

- uint8x8x2_t vtrn_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vtrn.8` d0`,` d1

- int16x4x2_t vtrn_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vtrn.16` d0`,` d1

- int8x8x2_t vtrn_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vtrn.8` d0`,` d1

- poly16x4x2_t vtrn_p16 (poly16x4_t, poly16x4_t)
  Form of expected instruction(s): `vtrn.16` d0`,` d1

- poly8x8x2_t vtrn_p8 (poly8x8_t, poly8x8_t)
  Form of expected instruction(s): `vtrn.8` d0`,` d1

- float32x2x2_t vtrn_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vuzp.32` d0`,` d1

- uint32x2x2_t vtrn_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vuzp.32` d0`,` d1

- int32x2x2_t vtrn_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vuzp.32` d0`,` d1

- uint32x4x2_t vtrnq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vtrn.32` q0`,` q1

- uint16x8x2_t vtrnq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vtrn.16` q0`,` q1

- uint8x16x2_t vtrnq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vtrn.8` q0`,` q1

- int32x4x2_t vtrnq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vtrn.32` q0`,` q1

- int16x8x2_t vtrnq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vtrn.16` q0`,` q1

- int8x16x2_t vtrnq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vtrn.8` q0`,` q1

- float32x4x2_t vtrnq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vtrn.32` q0`,` q1

- poly16x8x2_t vtrnq_p16 (poly16x8_t, poly16x8_t)
  Form of expected instruction(s): `vtrn.16` q0`,` q1

- poly8x16x2_t vtrnq_p8 (poly8x16_t, poly8x16_t)
  Form of expected instruction(s): `vtrn.8` q0`,` q1

##### 6.57.6.73 Zip elements

- uint16x4x2_t vzip_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vzip.16` d0`,` d1

- uint8x8x2_t vzip_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vzip.8` d0`,` d1

- int16x4x2_t vzip_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vzip.16` d0`,` d1

- int8x8x2_t vzip_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vzip.8` d0`,` d1

- poly16x4x2_t vzip_p16 (poly16x4_t, poly16x4_t)
  Form of expected instruction(s): `vzip.16` d0`,` d1

- poly8x8x2_t vzip_p8 (poly8x8_t, poly8x8_t)
  Form of expected instruction(s): `vzip.8` d0`,` d1

- float32x2x2_t vzip_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vuzp.32` d0`,` d1

- uint32x2x2_t vzip_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vuzp.32` d0`,` d1

- int32x2x2_t vzip_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vuzp.32` d0`,` d1

- uint32x4x2_t vzipq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vzip.32` q0`,` q1

- uint16x8x2_t vzipq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vzip.16` q0`,` q1

- uint8x16x2_t vzipq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vzip.8` q0`,` q1

- int32x4x2_t vzipq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vzip.32` q0`,` q1

- int16x8x2_t vzipq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vzip.16` q0`,` q1

- int8x16x2_t vzipq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vzip.8` q0`,` q1

- float32x4x2_t vzipq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vzip.32` q0`,` q1

- poly16x8x2_t vzipq_p16 (poly16x8_t, poly16x8_t)
  Form of expected instruction(s): `vzip.16` q0`,` q1

- poly8x16x2_t vzipq_p8 (poly8x16_t, poly8x16_t)
  Form of expected instruction(s): `vzip.8` q0`,` q1

##### 6.57.6.74 Unzip elements

- uint32x2x2_t vuzp_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vuzp.32` d0`,` d1

- uint16x4x2_t vuzp_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vuzp.16` d0`,` d1

- uint8x8x2_t vuzp_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vuzp.8` d0`,` d1

- int32x2x2_t vuzp_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vuzp.32` d0`,` d1

- int16x4x2_t vuzp_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vuzp.16` d0`,` d1

- int8x8x2_t vuzp_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vuzp.8` d0`,` d1

- float32x2x2_t vuzp_f32 (float32x2_t, float32x2_t)
  Form of expected instruction(s): `vuzp.32` d0`,` d1

- poly16x4x2_t vuzp_p16 (poly16x4_t, poly16x4_t)
  Form of expected instruction(s): `vuzp.16` d0`,` d1

- poly8x8x2_t vuzp_p8 (poly8x8_t, poly8x8_t)
  Form of expected instruction(s): `vuzp.8` d0`,` d1

- uint32x4x2_t vuzpq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vuzp.32` q0`,` q1

- uint16x8x2_t vuzpq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vuzp.16` q0`,` q1

- uint8x16x2_t vuzpq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vuzp.8` q0`,` q1

- int32x4x2_t vuzpq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vuzp.32` q0`,` q1

- int16x8x2_t vuzpq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vuzp.16` q0`,` q1

- int8x16x2_t vuzpq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vuzp.8` q0`,` q1

- float32x4x2_t vuzpq_f32 (float32x4_t, float32x4_t)
  Form of expected instruction(s): `vuzp.32` q0`,` q1

- poly16x8x2_t vuzpq_p16 (poly16x8_t, poly16x8_t)
  Form of expected instruction(s): `vuzp.16` q0`,` q1

- poly8x16x2_t vuzpq_p8 (poly8x16_t, poly8x16_t)
  Form of expected instruction(s): `vuzp.8` q0`,` q1

##### 6.57.6.75 Element/structure loads, VLD1 variants

- poly64x1_t vld1_p64 (const poly64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- uint32x2_t vld1_u32 (const uint32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`}, [`r0`]`

- uint16x4_t vld1_u16 (const uint16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`}, [`r0`]`

- uint8x8_t vld1_u8 (const uint8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`}, [`r0`]`

- int32x2_t vld1_s32 (const int32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`}, [`r0`]`

- int16x4_t vld1_s16 (const int16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`}, [`r0`]`

- int8x8_t vld1_s8 (const int8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`}, [`r0`]`

- uint64x1_t vld1_u64 (const uint64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- int64x1_t vld1_s64 (const int64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- float32x2_t vld1_f32 (const float32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`}, [`r0`]`

- poly16x4_t vld1_p16 (const poly16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`}, [`r0`]`

- poly8x8_t vld1_p8 (const poly8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`}, [`r0`]`

- poly64x2_t vld1q_p64 (const poly64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`}, [`r0`]`

- uint32x4_t vld1q_u32 (const uint32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`,` d1`}, [`r0`]`

- uint16x8_t vld1q_u16 (const uint16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`,` d1`}, [`r0`]`

- uint8x16_t vld1q_u8 (const uint8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`,` d1`}, [`r0`]`

- int32x4_t vld1q_s32 (const int32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`,` d1`}, [`r0`]`

- int16x8_t vld1q_s16 (const int16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`,` d1`}, [`r0`]`

- int8x16_t vld1q_s8 (const int8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`,` d1`}, [`r0`]`

- uint64x2_t vld1q_u64 (const uint64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`}, [`r0`]`

- int64x2_t vld1q_s64 (const int64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`}, [`r0`]`

- float32x4_t vld1q_f32 (const float32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`,` d1`}, [`r0`]`

- poly16x8_t vld1q_p16 (const poly16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`,` d1`}, [`r0`]`

- poly8x16_t vld1q_p8 (const poly8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`,` d1`}, [`r0`]`

- uint32x2_t vld1_lane_u32 (const uint32_t *, uint32x2_t, const int)
  Form of expected instruction(s): `vld1.32 {`d0`[`0`]}, [`r0`]`

- uint16x4_t vld1_lane_u16 (const uint16_t *, uint16x4_t, const int)
  Form of expected instruction(s): `vld1.16 {`d0`[`0`]}, [`r0`]`

- uint8x8_t vld1_lane_u8 (const uint8_t *, uint8x8_t, const int)
  Form of expected instruction(s): `vld1.8 {`d0`[`0`]}, [`r0`]`

- int32x2_t vld1_lane_s32 (const int32_t *, int32x2_t, const int)
  Form of expected instruction(s): `vld1.32 {`d0`[`0`]}, [`r0`]`

- int16x4_t vld1_lane_s16 (const int16_t *, int16x4_t, const int)
  Form of expected instruction(s): `vld1.16 {`d0`[`0`]}, [`r0`]`

- int8x8_t vld1_lane_s8 (const int8_t *, int8x8_t, const int)
  Form of expected instruction(s): `vld1.8 {`d0`[`0`]}, [`r0`]`

- float32x2_t vld1_lane_f32 (const float32_t *, float32x2_t, const int)
  Form of expected instruction(s): `vld1.32 {`d0`[`0`]}, [`r0`]`

- poly16x4_t vld1_lane_p16 (const poly16_t *, poly16x4_t, const int)
  Form of expected instruction(s): `vld1.16 {`d0`[`0`]}, [`r0`]`

- poly8x8_t vld1_lane_p8 (const poly8_t *, poly8x8_t, const int)
  Form of expected instruction(s): `vld1.8 {`d0`[`0`]}, [`r0`]`

- poly64x1_t vld1_lane_p64 (const poly64_t *, poly64x1_t, const int)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- uint64x1_t vld1_lane_u64 (const uint64_t *, uint64x1_t, const int)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- int64x1_t vld1_lane_s64 (const int64_t *, int64x1_t, const int)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- uint32x4_t vld1q_lane_u32 (const uint32_t *, uint32x4_t, const int)
  Form of expected instruction(s): `vld1.32 {`d0`[`0`]}, [`r0`]`

- uint16x8_t vld1q_lane_u16 (const uint16_t *, uint16x8_t, const int)
  Form of expected instruction(s): `vld1.16 {`d0`[`0`]}, [`r0`]`

- uint8x16_t vld1q_lane_u8 (const uint8_t *, uint8x16_t, const int)
  Form of expected instruction(s): `vld1.8 {`d0`[`0`]}, [`r0`]`

- int32x4_t vld1q_lane_s32 (const int32_t *, int32x4_t, const int)
  Form of expected instruction(s): `vld1.32 {`d0`[`0`]}, [`r0`]`

- int16x8_t vld1q_lane_s16 (const int16_t *, int16x8_t, const int)
  Form of expected instruction(s): `vld1.16 {`d0`[`0`]}, [`r0`]`

- int8x16_t vld1q_lane_s8 (const int8_t *, int8x16_t, const int)
  Form of expected instruction(s): `vld1.8 {`d0`[`0`]}, [`r0`]`

- float32x4_t vld1q_lane_f32 (const float32_t *, float32x4_t, const int)
  Form of expected instruction(s): `vld1.32 {`d0`[`0`]}, [`r0`]`

- poly16x8_t vld1q_lane_p16 (const poly16_t *, poly16x8_t, const int)
  Form of expected instruction(s): `vld1.16 {`d0`[`0`]}, [`r0`]`

- poly8x16_t vld1q_lane_p8 (const poly8_t *, poly8x16_t, const int)
  Form of expected instruction(s): `vld1.8 {`d0`[`0`]}, [`r0`]`

- poly64x2_t vld1q_lane_p64 (const poly64_t *, poly64x2_t, const int)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- uint64x2_t vld1q_lane_u64 (const uint64_t *, uint64x2_t, const int)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- int64x2_t vld1q_lane_s64 (const int64_t *, int64x2_t, const int)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- uint32x2_t vld1_dup_u32 (const uint32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`[]}, [`r0`]`

- uint16x4_t vld1_dup_u16 (const uint16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`[]}, [`r0`]`

- uint8x8_t vld1_dup_u8 (const uint8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`[]}, [`r0`]`

- int32x2_t vld1_dup_s32 (const int32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`[]}, [`r0`]`

- int16x4_t vld1_dup_s16 (const int16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`[]}, [`r0`]`

- int8x8_t vld1_dup_s8 (const int8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`[]}, [`r0`]`

- float32x2_t vld1_dup_f32 (const float32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`[]}, [`r0`]`

- poly16x4_t vld1_dup_p16 (const poly16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`[]}, [`r0`]`

- poly8x8_t vld1_dup_p8 (const poly8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`[]}, [`r0`]`

- poly64x1_t vld1_dup_p64 (const poly64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- uint64x1_t vld1_dup_u64 (const uint64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- int64x1_t vld1_dup_s64 (const int64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- uint32x4_t vld1q_dup_u32 (const uint32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`[],` d1`[]}, [`r0`]`

- uint16x8_t vld1q_dup_u16 (const uint16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`[],` d1`[]}, [`r0`]`

- uint8x16_t vld1q_dup_u8 (const uint8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`[],` d1`[]}, [`r0`]`

- int32x4_t vld1q_dup_s32 (const int32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`[],` d1`[]}, [`r0`]`

- int16x8_t vld1q_dup_s16 (const int16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`[],` d1`[]}, [`r0`]`

- int8x16_t vld1q_dup_s8 (const int8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`[],` d1`[]}, [`r0`]`

- float32x4_t vld1q_dup_f32 (const float32_t *)
  Form of expected instruction(s): `vld1.32 {`d0`[],` d1`[]}, [`r0`]`

- poly16x8_t vld1q_dup_p16 (const poly16_t *)
  Form of expected instruction(s): `vld1.16 {`d0`[],` d1`[]}, [`r0`]`

- poly8x16_t vld1q_dup_p8 (const poly8_t *)
  Form of expected instruction(s): `vld1.8 {`d0`[],` d1`[]}, [`r0`]`

- poly64x2_t vld1q_dup_p64 (const poly64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- uint64x2_t vld1q_dup_u64 (const uint64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

- int64x2_t vld1q_dup_s64 (const int64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`}, [`r0`]`

##### 6.57.6.76 Element/structure stores, VST1 variants

- void vst1_p64 (poly64_t *, poly64x1_t)
  Form of expected instruction(s): `vst1.64 {`d0`}, [`r0`]`

- void vst1_u32 (uint32_t *, uint32x2_t)
  Form of expected instruction(s): `vst1.32 {`d0`}, [`r0`]`

- void vst1_u16 (uint16_t *, uint16x4_t)
  Form of expected instruction(s): `vst1.16 {`d0`}, [`r0`]`

- void vst1_u8 (uint8_t *, uint8x8_t)
  Form of expected instruction(s): `vst1.8 {`d0`}, [`r0`]`

- void vst1_s32 (int32_t *, int32x2_t)
  Form of expected instruction(s): `vst1.32 {`d0`}, [`r0`]`

- void vst1_s16 (int16_t *, int16x4_t)
  Form of expected instruction(s): `vst1.16 {`d0`}, [`r0`]`

- void vst1_s8 (int8_t *, int8x8_t)
  Form of expected instruction(s): `vst1.8 {`d0`}, [`r0`]`

- void vst1_u64 (uint64_t *, uint64x1_t)
  Form of expected instruction(s): `vst1.64 {`d0`}, [`r0`]`

- void vst1_s64 (int64_t *, int64x1_t)
  Form of expected instruction(s): `vst1.64 {`d0`}, [`r0`]`

- void vst1_f32 (float32_t *, float32x2_t)
  Form of expected instruction(s): `vst1.32 {`d0`}, [`r0`]`

- void vst1_p16 (poly16_t *, poly16x4_t)
  Form of expected instruction(s): `vst1.16 {`d0`}, [`r0`]`

- void vst1_p8 (poly8_t *, poly8x8_t)
  Form of expected instruction(s): `vst1.8 {`d0`}, [`r0`]`

- void vst1q_p64 (poly64_t *, poly64x2_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`}, [`r0`]`

- void vst1q_u32 (uint32_t *, uint32x4_t)
  Form of expected instruction(s): `vst1.32 {`d0`,` d1`}, [`r0`]`

- void vst1q_u16 (uint16_t *, uint16x8_t)
  Form of expected instruction(s): `vst1.16 {`d0`,` d1`}, [`r0`]`

- void vst1q_u8 (uint8_t *, uint8x16_t)
  Form of expected instruction(s): `vst1.8 {`d0`,` d1`}, [`r0`]`

- void vst1q_s32 (int32_t *, int32x4_t)
  Form of expected instruction(s): `vst1.32 {`d0`,` d1`}, [`r0`]`

- void vst1q_s16 (int16_t *, int16x8_t)
  Form of expected instruction(s): `vst1.16 {`d0`,` d1`}, [`r0`]`

- void vst1q_s8 (int8_t *, int8x16_t)
  Form of expected instruction(s): `vst1.8 {`d0`,` d1`}, [`r0`]`

- void vst1q_u64 (uint64_t *, uint64x2_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`}, [`r0`]`

- void vst1q_s64 (int64_t *, int64x2_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`}, [`r0`]`

- void vst1q_f32 (float32_t *, float32x4_t)
  Form of expected instruction(s): `vst1.32 {`d0`,` d1`}, [`r0`]`

- void vst1q_p16 (poly16_t *, poly16x8_t)
  Form of expected instruction(s): `vst1.16 {`d0`,` d1`}, [`r0`]`

- void vst1q_p8 (poly8_t *, poly8x16_t)
  Form of expected instruction(s): `vst1.8 {`d0`,` d1`}, [`r0`]`

- void vst1_lane_u32 (uint32_t *, uint32x2_t, const int)
  Form of expected instruction(s): `vst1.32 {`d0`[`0`]}, [`r0`]`

- void vst1_lane_u16 (uint16_t *, uint16x4_t, const int)
  Form of expected instruction(s): `vst1.16 {`d0`[`0`]}, [`r0`]`

- void vst1_lane_u8 (uint8_t *, uint8x8_t, const int)
  Form of expected instruction(s): `vst1.8 {`d0`[`0`]}, [`r0`]`

- void vst1_lane_s32 (int32_t *, int32x2_t, const int)
  Form of expected instruction(s): `vst1.32 {`d0`[`0`]}, [`r0`]`

- void vst1_lane_s16 (int16_t *, int16x4_t, const int)
  Form of expected instruction(s): `vst1.16 {`d0`[`0`]}, [`r0`]`

- void vst1_lane_s8 (int8_t *, int8x8_t, const int)
  Form of expected instruction(s): `vst1.8 {`d0`[`0`]}, [`r0`]`

- void vst1_lane_f32 (float32_t *, float32x2_t, const int)
  Form of expected instruction(s): `vst1.32 {`d0`[`0`]}, [`r0`]`

- void vst1_lane_p16 (poly16_t *, poly16x4_t, const int)
  Form of expected instruction(s): `vst1.16 {`d0`[`0`]}, [`r0`]`

- void vst1_lane_p8 (poly8_t *, poly8x8_t, const int)
  Form of expected instruction(s): `vst1.8 {`d0`[`0`]}, [`r0`]`

- void vst1_lane_p64 (poly64_t *, poly64x1_t, const int)
  Form of expected instruction(s): `vst1.64 {`d0`}, [`r0`]`

- void vst1_lane_s64 (int64_t *, int64x1_t, const int)
  Form of expected instruction(s): `vst1.64 {`d0`}, [`r0`]`

- void vst1_lane_u64 (uint64_t *, uint64x1_t, const int)
  Form of expected instruction(s): `vst1.64 {`d0`}, [`r0`]`

- void vst1q_lane_u32 (uint32_t *, uint32x4_t, const int)
  Form of expected instruction(s): `vst1.32 {`d0`[`0`]}, [`r0`]`

- void vst1q_lane_u16 (uint16_t *, uint16x8_t, const int)
  Form of expected instruction(s): `vst1.16 {`d0`[`0`]}, [`r0`]`

- void vst1q_lane_u8 (uint8_t *, uint8x16_t, const int)
  Form of expected instruction(s): `vst1.8 {`d0`[`0`]}, [`r0`]`

- void vst1q_lane_s32 (int32_t *, int32x4_t, const int)
  Form of expected instruction(s): `vst1.32 {`d0`[`0`]}, [`r0`]`

- void vst1q_lane_s16 (int16_t *, int16x8_t, const int)
  Form of expected instruction(s): `vst1.16 {`d0`[`0`]}, [`r0`]`

- void vst1q_lane_s8 (int8_t *, int8x16_t, const int)
  Form of expected instruction(s): `vst1.8 {`d0`[`0`]}, [`r0`]`

- void vst1q_lane_f32 (float32_t *, float32x4_t, const int)
  Form of expected instruction(s): `vst1.32 {`d0`[`0`]}, [`r0`]`

- void vst1q_lane_p16 (poly16_t *, poly16x8_t, const int)
  Form of expected instruction(s): `vst1.16 {`d0`[`0`]}, [`r0`]`

- void vst1q_lane_p8 (poly8_t *, poly8x16_t, const int)
  Form of expected instruction(s): `vst1.8 {`d0`[`0`]}, [`r0`]`

- void vst1q_lane_p64 (poly64_t *, poly64x2_t, const int)
  Form of expected instruction(s): `vst1.64 {`d0`}, [`r0`]`

- void vst1q_lane_s64 (int64_t *, int64x2_t, const int)
  Form of expected instruction(s): `vst1.64 {`d0`}, [`r0`]`

- void vst1q_lane_u64 (uint64_t *, uint64x2_t, const int)
  Form of expected instruction(s): `vst1.64 {`d0`}, [`r0`]`

##### 6.57.6.77 Element/structure loads, VLD2 variants

- uint32x2x2_t vld2_u32 (const uint32_t *)
  Form of expected instruction(s): `vld2.32 {`d0`,` d1`}, [`r0`]`

- uint16x4x2_t vld2_u16 (const uint16_t *)
  Form of expected instruction(s): `vld2.16 {`d0`,` d1`}, [`r0`]`

- uint8x8x2_t vld2_u8 (const uint8_t *)
  Form of expected instruction(s): `vld2.8 {`d0`,` d1`}, [`r0`]`

- int32x2x2_t vld2_s32 (const int32_t *)
  Form of expected instruction(s): `vld2.32 {`d0`,` d1`}, [`r0`]`

- int16x4x2_t vld2_s16 (const int16_t *)
  Form of expected instruction(s): `vld2.16 {`d0`,` d1`}, [`r0`]`

- int8x8x2_t vld2_s8 (const int8_t *)
  Form of expected instruction(s): `vld2.8 {`d0`,` d1`}, [`r0`]`

- float32x2x2_t vld2_f32 (const float32_t *)
  Form of expected instruction(s): `vld2.32 {`d0`,` d1`}, [`r0`]`

- poly16x4x2_t vld2_p16 (const poly16_t *)
  Form of expected instruction(s): `vld2.16 {`d0`,` d1`}, [`r0`]`

- poly8x8x2_t vld2_p8 (const poly8_t *)
  Form of expected instruction(s): `vld2.8 {`d0`,` d1`}, [`r0`]`

- poly64x1x2_t vld2_p64 (const poly64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`}, [`r0`]`

- uint64x1x2_t vld2_u64 (const uint64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`}, [`r0`]`

- int64x1x2_t vld2_s64 (const int64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`}, [`r0`]`

- uint32x4x2_t vld2q_u32 (const uint32_t *)
  Form of expected instruction(s): `vld2.32 {`d0`,` d1`}, [`r0`]`

- uint16x8x2_t vld2q_u16 (const uint16_t *)
  Form of expected instruction(s): `vld2.16 {`d0`,` d1`}, [`r0`]`

- uint8x16x2_t vld2q_u8 (const uint8_t *)
  Form of expected instruction(s): `vld2.8 {`d0`,` d1`}, [`r0`]`

- int32x4x2_t vld2q_s32 (const int32_t *)
  Form of expected instruction(s): `vld2.32 {`d0`,` d1`}, [`r0`]`

- int16x8x2_t vld2q_s16 (const int16_t *)
  Form of expected instruction(s): `vld2.16 {`d0`,` d1`}, [`r0`]`

- int8x16x2_t vld2q_s8 (const int8_t *)
  Form of expected instruction(s): `vld2.8 {`d0`,` d1`}, [`r0`]`

- float32x4x2_t vld2q_f32 (const float32_t *)
  Form of expected instruction(s): `vld2.32 {`d0`,` d1`}, [`r0`]`

- poly16x8x2_t vld2q_p16 (const poly16_t *)
  Form of expected instruction(s): `vld2.16 {`d0`,` d1`}, [`r0`]`

- poly8x16x2_t vld2q_p8 (const poly8_t *)
  Form of expected instruction(s): `vld2.8 {`d0`,` d1`}, [`r0`]`

- uint32x2x2_t vld2_lane_u32 (const uint32_t *, uint32x2x2_t, const int)
  Form of expected instruction(s): `vld2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- uint16x4x2_t vld2_lane_u16 (const uint16_t *, uint16x4x2_t, const int)
  Form of expected instruction(s): `vld2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- uint8x8x2_t vld2_lane_u8 (const uint8_t *, uint8x8x2_t, const int)
  Form of expected instruction(s): `vld2.8 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- int32x2x2_t vld2_lane_s32 (const int32_t *, int32x2x2_t, const int)
  Form of expected instruction(s): `vld2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- int16x4x2_t vld2_lane_s16 (const int16_t *, int16x4x2_t, const int)
  Form of expected instruction(s): `vld2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- int8x8x2_t vld2_lane_s8 (const int8_t *, int8x8x2_t, const int)
  Form of expected instruction(s): `vld2.8 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- float32x2x2_t vld2_lane_f32 (const float32_t *, float32x2x2_t, const int)
  Form of expected instruction(s): `vld2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- poly16x4x2_t vld2_lane_p16 (const poly16_t *, poly16x4x2_t, const int)
  Form of expected instruction(s): `vld2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- poly8x8x2_t vld2_lane_p8 (const poly8_t *, poly8x8x2_t, const int)
  Form of expected instruction(s): `vld2.8 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- int32x4x2_t vld2q_lane_s32 (const int32_t *, int32x4x2_t, const int)
  Form of expected instruction(s): `vld2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- int16x8x2_t vld2q_lane_s16 (const int16_t *, int16x8x2_t, const int)
  Form of expected instruction(s): `vld2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- uint32x4x2_t vld2q_lane_u32 (const uint32_t *, uint32x4x2_t, const int)
  Form of expected instruction(s): `vld2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- uint16x8x2_t vld2q_lane_u16 (const uint16_t *, uint16x8x2_t, const int)
  Form of expected instruction(s): `vld2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- float32x4x2_t vld2q_lane_f32 (const float32_t *, float32x4x2_t, const int)
  Form of expected instruction(s): `vld2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- poly16x8x2_t vld2q_lane_p16 (const poly16_t *, poly16x8x2_t, const int)
  Form of expected instruction(s): `vld2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- uint32x2x2_t vld2_dup_u32 (const uint32_t *)
  Form of expected instruction(s): `vld2.32 {`d0`[],` d1`[]}, [`r0`]`

- uint16x4x2_t vld2_dup_u16 (const uint16_t *)
  Form of expected instruction(s): `vld2.16 {`d0`[],` d1`[]}, [`r0`]`

- uint8x8x2_t vld2_dup_u8 (const uint8_t *)
  Form of expected instruction(s): `vld2.8 {`d0`[],` d1`[]}, [`r0`]`

- int32x2x2_t vld2_dup_s32 (const int32_t *)
  Form of expected instruction(s): `vld2.32 {`d0`[],` d1`[]}, [`r0`]`

- int16x4x2_t vld2_dup_s16 (const int16_t *)
  Form of expected instruction(s): `vld2.16 {`d0`[],` d1`[]}, [`r0`]`

- int8x8x2_t vld2_dup_s8 (const int8_t *)
  Form of expected instruction(s): `vld2.8 {`d0`[],` d1`[]}, [`r0`]`

- float32x2x2_t vld2_dup_f32 (const float32_t *)
  Form of expected instruction(s): `vld2.32 {`d0`[],` d1`[]}, [`r0`]`

- poly16x4x2_t vld2_dup_p16 (const poly16_t *)
  Form of expected instruction(s): `vld2.16 {`d0`[],` d1`[]}, [`r0`]`

- poly8x8x2_t vld2_dup_p8 (const poly8_t *)
  Form of expected instruction(s): `vld2.8 {`d0`[],` d1`[]}, [`r0`]`

- poly64x1x2_t vld2_dup_p64 (const poly64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`}, [`r0`]`

- uint64x1x2_t vld2_dup_u64 (const uint64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`}, [`r0`]`

- int64x1x2_t vld2_dup_s64 (const int64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`}, [`r0`]`

##### 6.57.6.78 Element/structure stores, VST2 variants

- void vst2_u32 (uint32_t *, uint32x2x2_t)
  Form of expected instruction(s): `vst2.32 {`d0`,` d1`}, [`r0`]`

- void vst2_u16 (uint16_t *, uint16x4x2_t)
  Form of expected instruction(s): `vst2.16 {`d0`,` d1`}, [`r0`]`

- void vst2_u8 (uint8_t *, uint8x8x2_t)
  Form of expected instruction(s): `vst2.8 {`d0`,` d1`}, [`r0`]`

- void vst2_s32 (int32_t *, int32x2x2_t)
  Form of expected instruction(s): `vst2.32 {`d0`,` d1`}, [`r0`]`

- void vst2_s16 (int16_t *, int16x4x2_t)
  Form of expected instruction(s): `vst2.16 {`d0`,` d1`}, [`r0`]`

- void vst2_s8 (int8_t *, int8x8x2_t)
  Form of expected instruction(s): `vst2.8 {`d0`,` d1`}, [`r0`]`

- void vst2_f32 (float32_t *, float32x2x2_t)
  Form of expected instruction(s): `vst2.32 {`d0`,` d1`}, [`r0`]`

- void vst2_p16 (poly16_t *, poly16x4x2_t)
  Form of expected instruction(s): `vst2.16 {`d0`,` d1`}, [`r0`]`

- void vst2_p8 (poly8_t *, poly8x8x2_t)
  Form of expected instruction(s): `vst2.8 {`d0`,` d1`}, [`r0`]`

- void vst2_p64 (poly64_t *, poly64x1x2_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`}, [`r0`]`

- void vst2_u64 (uint64_t *, uint64x1x2_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`}, [`r0`]`

- void vst2_s64 (int64_t *, int64x1x2_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`}, [`r0`]`

- void vst2q_u32 (uint32_t *, uint32x4x2_t)
  Form of expected instruction(s): `vst2.32 {`d0`,` d1`}, [`r0`]`

- void vst2q_u16 (uint16_t *, uint16x8x2_t)
  Form of expected instruction(s): `vst2.16 {`d0`,` d1`}, [`r0`]`

- void vst2q_u8 (uint8_t *, uint8x16x2_t)
  Form of expected instruction(s): `vst2.8 {`d0`,` d1`}, [`r0`]`

- void vst2q_s32 (int32_t *, int32x4x2_t)
  Form of expected instruction(s): `vst2.32 {`d0`,` d1`}, [`r0`]`

- void vst2q_s16 (int16_t *, int16x8x2_t)
  Form of expected instruction(s): `vst2.16 {`d0`,` d1`}, [`r0`]`

- void vst2q_s8 (int8_t *, int8x16x2_t)
  Form of expected instruction(s): `vst2.8 {`d0`,` d1`}, [`r0`]`

- void vst2q_f32 (float32_t *, float32x4x2_t)
  Form of expected instruction(s): `vst2.32 {`d0`,` d1`}, [`r0`]`

- void vst2q_p16 (poly16_t *, poly16x8x2_t)
  Form of expected instruction(s): `vst2.16 {`d0`,` d1`}, [`r0`]`

- void vst2q_p8 (poly8_t *, poly8x16x2_t)
  Form of expected instruction(s): `vst2.8 {`d0`,` d1`}, [`r0`]`

- void vst2_lane_u32 (uint32_t *, uint32x2x2_t, const int)
  Form of expected instruction(s): `vst2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2_lane_u16 (uint16_t *, uint16x4x2_t, const int)
  Form of expected instruction(s): `vst2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2_lane_u8 (uint8_t *, uint8x8x2_t, const int)
  Form of expected instruction(s): `vst2.8 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2_lane_s32 (int32_t *, int32x2x2_t, const int)
  Form of expected instruction(s): `vst2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2_lane_s16 (int16_t *, int16x4x2_t, const int)
  Form of expected instruction(s): `vst2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2_lane_s8 (int8_t *, int8x8x2_t, const int)
  Form of expected instruction(s): `vst2.8 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2_lane_f32 (float32_t *, float32x2x2_t, const int)
  Form of expected instruction(s): `vst2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2_lane_p16 (poly16_t *, poly16x4x2_t, const int)
  Form of expected instruction(s): `vst2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2_lane_p8 (poly8_t *, poly8x8x2_t, const int)
  Form of expected instruction(s): `vst2.8 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2q_lane_s32 (int32_t *, int32x4x2_t, const int)
  Form of expected instruction(s): `vst2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2q_lane_s16 (int16_t *, int16x8x2_t, const int)
  Form of expected instruction(s): `vst2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2q_lane_u32 (uint32_t *, uint32x4x2_t, const int)
  Form of expected instruction(s): `vst2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2q_lane_u16 (uint16_t *, uint16x8x2_t, const int)
  Form of expected instruction(s): `vst2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2q_lane_f32 (float32_t *, float32x4x2_t, const int)
  Form of expected instruction(s): `vst2.32 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

- void vst2q_lane_p16 (poly16_t *, poly16x8x2_t, const int)
  Form of expected instruction(s): `vst2.16 {`d0`[`0`],` d1`[`0`]}, [`r0`]`

##### 6.57.6.79 Element/structure loads, VLD3 variants

- uint32x2x3_t vld3_u32 (const uint32_t *)
  Form of expected instruction(s): `vld3.32 {`d0`,` d1`,` d2`}, [`r0`]`

- uint16x4x3_t vld3_u16 (const uint16_t *)
  Form of expected instruction(s): `vld3.16 {`d0`,` d1`,` d2`}, [`r0`]`

- uint8x8x3_t vld3_u8 (const uint8_t *)
  Form of expected instruction(s): `vld3.8 {`d0`,` d1`,` d2`}, [`r0`]`

- int32x2x3_t vld3_s32 (const int32_t *)
  Form of expected instruction(s): `vld3.32 {`d0`,` d1`,` d2`}, [`r0`]`

- int16x4x3_t vld3_s16 (const int16_t *)
  Form of expected instruction(s): `vld3.16 {`d0`,` d1`,` d2`}, [`r0`]`

- int8x8x3_t vld3_s8 (const int8_t *)
  Form of expected instruction(s): `vld3.8 {`d0`,` d1`,` d2`}, [`r0`]`

- float32x2x3_t vld3_f32 (const float32_t *)
  Form of expected instruction(s): `vld3.32 {`d0`,` d1`,` d2`}, [`r0`]`

- poly16x4x3_t vld3_p16 (const poly16_t *)
  Form of expected instruction(s): `vld3.16 {`d0`,` d1`,` d2`}, [`r0`]`

- poly8x8x3_t vld3_p8 (const poly8_t *)
  Form of expected instruction(s): `vld3.8 {`d0`,` d1`,` d2`}, [`r0`]`

- poly64x1x3_t vld3_p64 (const poly64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`}, [`r0`]`

- uint64x1x3_t vld3_u64 (const uint64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`}, [`r0`]`

- int64x1x3_t vld3_s64 (const int64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`}, [`r0`]`

- uint32x4x3_t vld3q_u32 (const uint32_t *)
  Form of expected instruction(s): `vld3.32 {`d0`,` d1`,` d2`}, [`r0`]`

- uint16x8x3_t vld3q_u16 (const uint16_t *)
  Form of expected instruction(s): `vld3.16 {`d0`,` d1`,` d2`}, [`r0`]`

- uint8x16x3_t vld3q_u8 (const uint8_t *)
  Form of expected instruction(s): `vld3.8 {`d0`,` d1`,` d2`}, [`r0`]`

- int32x4x3_t vld3q_s32 (const int32_t *)
  Form of expected instruction(s): `vld3.32 {`d0`,` d1`,` d2`}, [`r0`]`

- int16x8x3_t vld3q_s16 (const int16_t *)
  Form of expected instruction(s): `vld3.16 {`d0`,` d1`,` d2`}, [`r0`]`

- int8x16x3_t vld3q_s8 (const int8_t *)
  Form of expected instruction(s): `vld3.8 {`d0`,` d1`,` d2`}, [`r0`]`

- float32x4x3_t vld3q_f32 (const float32_t *)
  Form of expected instruction(s): `vld3.32 {`d0`,` d1`,` d2`}, [`r0`]`

- poly16x8x3_t vld3q_p16 (const poly16_t *)
  Form of expected instruction(s): `vld3.16 {`d0`,` d1`,` d2`}, [`r0`]`

- poly8x16x3_t vld3q_p8 (const poly8_t *)
  Form of expected instruction(s): `vld3.8 {`d0`,` d1`,` d2`}, [`r0`]`

- uint32x2x3_t vld3_lane_u32 (const uint32_t *, uint32x2x3_t, const int)
  Form of expected instruction(s): `vld3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- uint16x4x3_t vld3_lane_u16 (const uint16_t *, uint16x4x3_t, const int)
  Form of expected instruction(s): `vld3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- uint8x8x3_t vld3_lane_u8 (const uint8_t *, uint8x8x3_t, const int)
  Form of expected instruction(s): `vld3.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- int32x2x3_t vld3_lane_s32 (const int32_t *, int32x2x3_t, const int)
  Form of expected instruction(s): `vld3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- int16x4x3_t vld3_lane_s16 (const int16_t *, int16x4x3_t, const int)
  Form of expected instruction(s): `vld3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- int8x8x3_t vld3_lane_s8 (const int8_t *, int8x8x3_t, const int)
  Form of expected instruction(s): `vld3.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- float32x2x3_t vld3_lane_f32 (const float32_t *, float32x2x3_t, const int)
  Form of expected instruction(s): `vld3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- poly16x4x3_t vld3_lane_p16 (const poly16_t *, poly16x4x3_t, const int)
  Form of expected instruction(s): `vld3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- poly8x8x3_t vld3_lane_p8 (const poly8_t *, poly8x8x3_t, const int)
  Form of expected instruction(s): `vld3.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- int32x4x3_t vld3q_lane_s32 (const int32_t *, int32x4x3_t, const int)
  Form of expected instruction(s): `vld3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- int16x8x3_t vld3q_lane_s16 (const int16_t *, int16x8x3_t, const int)
  Form of expected instruction(s): `vld3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- uint32x4x3_t vld3q_lane_u32 (const uint32_t *, uint32x4x3_t, const int)
  Form of expected instruction(s): `vld3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- uint16x8x3_t vld3q_lane_u16 (const uint16_t *, uint16x8x3_t, const int)
  Form of expected instruction(s): `vld3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- float32x4x3_t vld3q_lane_f32 (const float32_t *, float32x4x3_t, const int)
  Form of expected instruction(s): `vld3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- poly16x8x3_t vld3q_lane_p16 (const poly16_t *, poly16x8x3_t, const int)
  Form of expected instruction(s): `vld3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- uint32x2x3_t vld3_dup_u32 (const uint32_t *)
  Form of expected instruction(s): `vld3.32 {`d0`[],` d1`[],` d2`[]}, [`r0`]`

- uint16x4x3_t vld3_dup_u16 (const uint16_t *)
  Form of expected instruction(s): `vld3.16 {`d0`[],` d1`[],` d2`[]}, [`r0`]`

- uint8x8x3_t vld3_dup_u8 (const uint8_t *)
  Form of expected instruction(s): `vld3.8 {`d0`[],` d1`[],` d2`[]}, [`r0`]`

- int32x2x3_t vld3_dup_s32 (const int32_t *)
  Form of expected instruction(s): `vld3.32 {`d0`[],` d1`[],` d2`[]}, [`r0`]`

- int16x4x3_t vld3_dup_s16 (const int16_t *)
  Form of expected instruction(s): `vld3.16 {`d0`[],` d1`[],` d2`[]}, [`r0`]`

- int8x8x3_t vld3_dup_s8 (const int8_t *)
  Form of expected instruction(s): `vld3.8 {`d0`[],` d1`[],` d2`[]}, [`r0`]`

- float32x2x3_t vld3_dup_f32 (const float32_t *)
  Form of expected instruction(s): `vld3.32 {`d0`[],` d1`[],` d2`[]}, [`r0`]`

- poly16x4x3_t vld3_dup_p16 (const poly16_t *)
  Form of expected instruction(s): `vld3.16 {`d0`[],` d1`[],` d2`[]}, [`r0`]`

- poly8x8x3_t vld3_dup_p8 (const poly8_t *)
  Form of expected instruction(s): `vld3.8 {`d0`[],` d1`[],` d2`[]}, [`r0`]`

- poly64x1x3_t vld3_dup_p64 (const poly64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`}, [`r0`]`

- uint64x1x3_t vld3_dup_u64 (const uint64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`}, [`r0`]`

- int64x1x3_t vld3_dup_s64 (const int64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`}, [`r0`]`

##### 6.57.6.80 Element/structure stores, VST3 variants

- void vst3_u32 (uint32_t *, uint32x2x3_t)
  Form of expected instruction(s): `vst3.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_u16 (uint16_t *, uint16x4x3_t)
  Form of expected instruction(s): `vst3.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_u8 (uint8_t *, uint8x8x3_t)
  Form of expected instruction(s): `vst3.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_s32 (int32_t *, int32x2x3_t)
  Form of expected instruction(s): `vst3.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_s16 (int16_t *, int16x4x3_t)
  Form of expected instruction(s): `vst3.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_s8 (int8_t *, int8x8x3_t)
  Form of expected instruction(s): `vst3.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_f32 (float32_t *, float32x2x3_t)
  Form of expected instruction(s): `vst3.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_p16 (poly16_t *, poly16x4x3_t)
  Form of expected instruction(s): `vst3.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_p8 (poly8_t *, poly8x8x3_t)
  Form of expected instruction(s): `vst3.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_p64 (poly64_t *, poly64x1x3_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_u64 (uint64_t *, uint64x1x3_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3_s64 (int64_t *, int64x1x3_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst3q_u32 (uint32_t *, uint32x4x3_t)
  Form of expected instruction(s): `vst3.32 {`d0`,` d1`,` d2`}, [`r0`]`

- void vst3q_u16 (uint16_t *, uint16x8x3_t)
  Form of expected instruction(s): `vst3.16 {`d0`,` d1`,` d2`}, [`r0`]`

- void vst3q_u8 (uint8_t *, uint8x16x3_t)
  Form of expected instruction(s): `vst3.8 {`d0`,` d1`,` d2`}, [`r0`]`

- void vst3q_s32 (int32_t *, int32x4x3_t)
  Form of expected instruction(s): `vst3.32 {`d0`,` d1`,` d2`}, [`r0`]`

- void vst3q_s16 (int16_t *, int16x8x3_t)
  Form of expected instruction(s): `vst3.16 {`d0`,` d1`,` d2`}, [`r0`]`

- void vst3q_s8 (int8_t *, int8x16x3_t)
  Form of expected instruction(s): `vst3.8 {`d0`,` d1`,` d2`}, [`r0`]`

- void vst3q_f32 (float32_t *, float32x4x3_t)
  Form of expected instruction(s): `vst3.32 {`d0`,` d1`,` d2`}, [`r0`]`

- void vst3q_p16 (poly16_t *, poly16x8x3_t)
  Form of expected instruction(s): `vst3.16 {`d0`,` d1`,` d2`}, [`r0`]`

- void vst3q_p8 (poly8_t *, poly8x16x3_t)
  Form of expected instruction(s): `vst3.8 {`d0`,` d1`,` d2`}, [`r0`]`

- void vst3_lane_u32 (uint32_t *, uint32x2x3_t, const int)
  Form of expected instruction(s): `vst3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3_lane_u16 (uint16_t *, uint16x4x3_t, const int)
  Form of expected instruction(s): `vst3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3_lane_u8 (uint8_t *, uint8x8x3_t, const int)
  Form of expected instruction(s): `vst3.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3_lane_s32 (int32_t *, int32x2x3_t, const int)
  Form of expected instruction(s): `vst3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3_lane_s16 (int16_t *, int16x4x3_t, const int)
  Form of expected instruction(s): `vst3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3_lane_s8 (int8_t *, int8x8x3_t, const int)
  Form of expected instruction(s): `vst3.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3_lane_f32 (float32_t *, float32x2x3_t, const int)
  Form of expected instruction(s): `vst3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3_lane_p16 (poly16_t *, poly16x4x3_t, const int)
  Form of expected instruction(s): `vst3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3_lane_p8 (poly8_t *, poly8x8x3_t, const int)
  Form of expected instruction(s): `vst3.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3q_lane_s32 (int32_t *, int32x4x3_t, const int)
  Form of expected instruction(s): `vst3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3q_lane_s16 (int16_t *, int16x8x3_t, const int)
  Form of expected instruction(s): `vst3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3q_lane_u32 (uint32_t *, uint32x4x3_t, const int)
  Form of expected instruction(s): `vst3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3q_lane_u16 (uint16_t *, uint16x8x3_t, const int)
  Form of expected instruction(s): `vst3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3q_lane_f32 (float32_t *, float32x4x3_t, const int)
  Form of expected instruction(s): `vst3.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

- void vst3q_lane_p16 (poly16_t *, poly16x8x3_t, const int)
  Form of expected instruction(s): `vst3.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`]}, [`r0`]`

##### 6.57.6.81 Element/structure loads, VLD4 variants

- uint32x2x4_t vld4_u32 (const uint32_t *)
  Form of expected instruction(s): `vld4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- uint16x4x4_t vld4_u16 (const uint16_t *)
  Form of expected instruction(s): `vld4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- uint8x8x4_t vld4_u8 (const uint8_t *)
  Form of expected instruction(s): `vld4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- int32x2x4_t vld4_s32 (const int32_t *)
  Form of expected instruction(s): `vld4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- int16x4x4_t vld4_s16 (const int16_t *)
  Form of expected instruction(s): `vld4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- int8x8x4_t vld4_s8 (const int8_t *)
  Form of expected instruction(s): `vld4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- float32x2x4_t vld4_f32 (const float32_t *)
  Form of expected instruction(s): `vld4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- poly16x4x4_t vld4_p16 (const poly16_t *)
  Form of expected instruction(s): `vld4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- poly8x8x4_t vld4_p8 (const poly8_t *)
  Form of expected instruction(s): `vld4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- poly64x1x4_t vld4_p64 (const poly64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- uint64x1x4_t vld4_u64 (const uint64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- int64x1x4_t vld4_s64 (const int64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- uint32x4x4_t vld4q_u32 (const uint32_t *)
  Form of expected instruction(s): `vld4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- uint16x8x4_t vld4q_u16 (const uint16_t *)
  Form of expected instruction(s): `vld4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- uint8x16x4_t vld4q_u8 (const uint8_t *)
  Form of expected instruction(s): `vld4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- int32x4x4_t vld4q_s32 (const int32_t *)
  Form of expected instruction(s): `vld4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- int16x8x4_t vld4q_s16 (const int16_t *)
  Form of expected instruction(s): `vld4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- int8x16x4_t vld4q_s8 (const int8_t *)
  Form of expected instruction(s): `vld4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- float32x4x4_t vld4q_f32 (const float32_t *)
  Form of expected instruction(s): `vld4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- poly16x8x4_t vld4q_p16 (const poly16_t *)
  Form of expected instruction(s): `vld4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- poly8x16x4_t vld4q_p8 (const poly8_t *)
  Form of expected instruction(s): `vld4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- uint32x2x4_t vld4_lane_u32 (const uint32_t *, uint32x2x4_t, const int)
  Form of expected instruction(s): `vld4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- uint16x4x4_t vld4_lane_u16 (const uint16_t *, uint16x4x4_t, const int)
  Form of expected instruction(s): `vld4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- uint8x8x4_t vld4_lane_u8 (const uint8_t *, uint8x8x4_t, const int)
  Form of expected instruction(s): `vld4.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- int32x2x4_t vld4_lane_s32 (const int32_t *, int32x2x4_t, const int)
  Form of expected instruction(s): `vld4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- int16x4x4_t vld4_lane_s16 (const int16_t *, int16x4x4_t, const int)
  Form of expected instruction(s): `vld4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- int8x8x4_t vld4_lane_s8 (const int8_t *, int8x8x4_t, const int)
  Form of expected instruction(s): `vld4.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- float32x2x4_t vld4_lane_f32 (const float32_t *, float32x2x4_t, const int)
  Form of expected instruction(s): `vld4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- poly16x4x4_t vld4_lane_p16 (const poly16_t *, poly16x4x4_t, const int)
  Form of expected instruction(s): `vld4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- poly8x8x4_t vld4_lane_p8 (const poly8_t *, poly8x8x4_t, const int)
  Form of expected instruction(s): `vld4.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- int32x4x4_t vld4q_lane_s32 (const int32_t *, int32x4x4_t, const int)
  Form of expected instruction(s): `vld4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- int16x8x4_t vld4q_lane_s16 (const int16_t *, int16x8x4_t, const int)
  Form of expected instruction(s): `vld4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- uint32x4x4_t vld4q_lane_u32 (const uint32_t *, uint32x4x4_t, const int)
  Form of expected instruction(s): `vld4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- uint16x8x4_t vld4q_lane_u16 (const uint16_t *, uint16x8x4_t, const int)
  Form of expected instruction(s): `vld4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- float32x4x4_t vld4q_lane_f32 (const float32_t *, float32x4x4_t, const int)
  Form of expected instruction(s): `vld4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- poly16x8x4_t vld4q_lane_p16 (const poly16_t *, poly16x8x4_t, const int)
  Form of expected instruction(s): `vld4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- uint32x2x4_t vld4_dup_u32 (const uint32_t *)
  Form of expected instruction(s): `vld4.32 {`d0`[],` d1`[],` d2`[],` d3`[]}, [`r0`]`

- uint16x4x4_t vld4_dup_u16 (const uint16_t *)
  Form of expected instruction(s): `vld4.16 {`d0`[],` d1`[],` d2`[],` d3`[]}, [`r0`]`

- uint8x8x4_t vld4_dup_u8 (const uint8_t *)
  Form of expected instruction(s): `vld4.8 {`d0`[],` d1`[],` d2`[],` d3`[]}, [`r0`]`

- int32x2x4_t vld4_dup_s32 (const int32_t *)
  Form of expected instruction(s): `vld4.32 {`d0`[],` d1`[],` d2`[],` d3`[]}, [`r0`]`

- int16x4x4_t vld4_dup_s16 (const int16_t *)
  Form of expected instruction(s): `vld4.16 {`d0`[],` d1`[],` d2`[],` d3`[]}, [`r0`]`

- int8x8x4_t vld4_dup_s8 (const int8_t *)
  Form of expected instruction(s): `vld4.8 {`d0`[],` d1`[],` d2`[],` d3`[]}, [`r0`]`

- float32x2x4_t vld4_dup_f32 (const float32_t *)
  Form of expected instruction(s): `vld4.32 {`d0`[],` d1`[],` d2`[],` d3`[]}, [`r0`]`

- poly16x4x4_t vld4_dup_p16 (const poly16_t *)
  Form of expected instruction(s): `vld4.16 {`d0`[],` d1`[],` d2`[],` d3`[]}, [`r0`]`

- poly8x8x4_t vld4_dup_p8 (const poly8_t *)
  Form of expected instruction(s): `vld4.8 {`d0`[],` d1`[],` d2`[],` d3`[]}, [`r0`]`

- poly64x1x4_t vld4_dup_p64 (const poly64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- uint64x1x4_t vld4_dup_u64 (const uint64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- int64x1x4_t vld4_dup_s64 (const int64_t *)
  Form of expected instruction(s): `vld1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

##### 6.57.6.82 Element/structure stores, VST4 variants

- void vst4_u32 (uint32_t *, uint32x2x4_t)
  Form of expected instruction(s): `vst4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_u16 (uint16_t *, uint16x4x4_t)
  Form of expected instruction(s): `vst4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_u8 (uint8_t *, uint8x8x4_t)
  Form of expected instruction(s): `vst4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_s32 (int32_t *, int32x2x4_t)
  Form of expected instruction(s): `vst4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_s16 (int16_t *, int16x4x4_t)
  Form of expected instruction(s): `vst4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_s8 (int8_t *, int8x8x4_t)
  Form of expected instruction(s): `vst4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_f32 (float32_t *, float32x2x4_t)
  Form of expected instruction(s): `vst4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_p16 (poly16_t *, poly16x4x4_t)
  Form of expected instruction(s): `vst4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_p8 (poly8_t *, poly8x8x4_t)
  Form of expected instruction(s): `vst4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_p64 (poly64_t *, poly64x1x4_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_u64 (uint64_t *, uint64x1x4_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_s64 (int64_t *, int64x1x4_t)
  Form of expected instruction(s): `vst1.64 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4q_u32 (uint32_t *, uint32x4x4_t)
  Form of expected instruction(s): `vst4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4q_u16 (uint16_t *, uint16x8x4_t)
  Form of expected instruction(s): `vst4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4q_u8 (uint8_t *, uint8x16x4_t)
  Form of expected instruction(s): `vst4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4q_s32 (int32_t *, int32x4x4_t)
  Form of expected instruction(s): `vst4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4q_s16 (int16_t *, int16x8x4_t)
  Form of expected instruction(s): `vst4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4q_s8 (int8_t *, int8x16x4_t)
  Form of expected instruction(s): `vst4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4q_f32 (float32_t *, float32x4x4_t)
  Form of expected instruction(s): `vst4.32 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4q_p16 (poly16_t *, poly16x8x4_t)
  Form of expected instruction(s): `vst4.16 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4q_p8 (poly8_t *, poly8x16x4_t)
  Form of expected instruction(s): `vst4.8 {`d0`,` d1`,` d2`,` d3`}, [`r0`]`

- void vst4_lane_u32 (uint32_t *, uint32x2x4_t, const int)
  Form of expected instruction(s): `vst4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4_lane_u16 (uint16_t *, uint16x4x4_t, const int)
  Form of expected instruction(s): `vst4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4_lane_u8 (uint8_t *, uint8x8x4_t, const int)
  Form of expected instruction(s): `vst4.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4_lane_s32 (int32_t *, int32x2x4_t, const int)
  Form of expected instruction(s): `vst4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4_lane_s16 (int16_t *, int16x4x4_t, const int)
  Form of expected instruction(s): `vst4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4_lane_s8 (int8_t *, int8x8x4_t, const int)
  Form of expected instruction(s): `vst4.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4_lane_f32 (float32_t *, float32x2x4_t, const int)
  Form of expected instruction(s): `vst4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4_lane_p16 (poly16_t *, poly16x4x4_t, const int)
  Form of expected instruction(s): `vst4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4_lane_p8 (poly8_t *, poly8x8x4_t, const int)
  Form of expected instruction(s): `vst4.8 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4q_lane_s32 (int32_t *, int32x4x4_t, const int)
  Form of expected instruction(s): `vst4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4q_lane_s16 (int16_t *, int16x8x4_t, const int)
  Form of expected instruction(s): `vst4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4q_lane_u32 (uint32_t *, uint32x4x4_t, const int)
  Form of expected instruction(s): `vst4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4q_lane_u16 (uint16_t *, uint16x8x4_t, const int)
  Form of expected instruction(s): `vst4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4q_lane_f32 (float32_t *, float32x4x4_t, const int)
  Form of expected instruction(s): `vst4.32 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

- void vst4q_lane_p16 (poly16_t *, poly16x8x4_t, const int)
  Form of expected instruction(s): `vst4.16 {`d0`[`0`],` d1`[`0`],` d2`[`0`],` d3`[`0`]}, [`r0`]`

##### 6.57.6.83 Logical operations (AND)

- uint32x2_t vand_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vand` d0`,` d0`,` d0

- uint16x4_t vand_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vand` d0`,` d0`,` d0

- uint8x8_t vand_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vand` d0`,` d0`,` d0

- int32x2_t vand_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vand` d0`,` d0`,` d0

- int16x4_t vand_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vand` d0`,` d0`,` d0

- int8x8_t vand_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vand` d0`,` d0`,` d0

- uint64x1_t vand_u64 (uint64x1_t, uint64x1_t)

- int64x1_t vand_s64 (int64x1_t, int64x1_t)

- uint32x4_t vandq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vand` q0`,` q0`,` q0

- uint16x8_t vandq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vand` q0`,` q0`,` q0

- uint8x16_t vandq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vand` q0`,` q0`,` q0

- int32x4_t vandq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vand` q0`,` q0`,` q0

- int16x8_t vandq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vand` q0`,` q0`,` q0

- int8x16_t vandq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vand` q0`,` q0`,` q0

- uint64x2_t vandq_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vand` q0`,` q0`,` q0

- int64x2_t vandq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vand` q0`,` q0`,` q0

##### 6.57.6.84 Logical operations (OR)

- uint32x2_t vorr_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vorr` d0`,` d0`,` d0

- uint16x4_t vorr_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vorr` d0`,` d0`,` d0

- uint8x8_t vorr_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vorr` d0`,` d0`,` d0

- int32x2_t vorr_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vorr` d0`,` d0`,` d0

- int16x4_t vorr_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vorr` d0`,` d0`,` d0

- int8x8_t vorr_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vorr` d0`,` d0`,` d0

- uint64x1_t vorr_u64 (uint64x1_t, uint64x1_t)

- int64x1_t vorr_s64 (int64x1_t, int64x1_t)

- uint32x4_t vorrq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vorr` q0`,` q0`,` q0

- uint16x8_t vorrq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vorr` q0`,` q0`,` q0

- uint8x16_t vorrq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vorr` q0`,` q0`,` q0

- int32x4_t vorrq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vorr` q0`,` q0`,` q0

- int16x8_t vorrq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vorr` q0`,` q0`,` q0

- int8x16_t vorrq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vorr` q0`,` q0`,` q0

- uint64x2_t vorrq_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vorr` q0`,` q0`,` q0

- int64x2_t vorrq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vorr` q0`,` q0`,` q0

##### 6.57.6.85 Logical operations (exclusive OR)

- uint32x2_t veor_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `veor` d0`,` d0`,` d0

- uint16x4_t veor_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `veor` d0`,` d0`,` d0

- uint8x8_t veor_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `veor` d0`,` d0`,` d0

- int32x2_t veor_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `veor` d0`,` d0`,` d0

- int16x4_t veor_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `veor` d0`,` d0`,` d0

- int8x8_t veor_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `veor` d0`,` d0`,` d0

- uint64x1_t veor_u64 (uint64x1_t, uint64x1_t)

- int64x1_t veor_s64 (int64x1_t, int64x1_t)

- uint32x4_t veorq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `veor` q0`,` q0`,` q0

- uint16x8_t veorq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `veor` q0`,` q0`,` q0

- uint8x16_t veorq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `veor` q0`,` q0`,` q0

- int32x4_t veorq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `veor` q0`,` q0`,` q0

- int16x8_t veorq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `veor` q0`,` q0`,` q0

- int8x16_t veorq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `veor` q0`,` q0`,` q0

- uint64x2_t veorq_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `veor` q0`,` q0`,` q0

- int64x2_t veorq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `veor` q0`,` q0`,` q0

##### 6.57.6.86 Logical operations (AND-NOT)

- uint32x2_t vbic_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vbic` d0`,` d0`,` d0

- uint16x4_t vbic_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vbic` d0`,` d0`,` d0

- uint8x8_t vbic_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vbic` d0`,` d0`,` d0

- int32x2_t vbic_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vbic` d0`,` d0`,` d0

- int16x4_t vbic_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vbic` d0`,` d0`,` d0

- int8x8_t vbic_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vbic` d0`,` d0`,` d0

- uint64x1_t vbic_u64 (uint64x1_t, uint64x1_t)

- int64x1_t vbic_s64 (int64x1_t, int64x1_t)

- uint32x4_t vbicq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vbic` q0`,` q0`,` q0

- uint16x8_t vbicq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vbic` q0`,` q0`,` q0

- uint8x16_t vbicq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vbic` q0`,` q0`,` q0

- int32x4_t vbicq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vbic` q0`,` q0`,` q0

- int16x8_t vbicq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vbic` q0`,` q0`,` q0

- int8x16_t vbicq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vbic` q0`,` q0`,` q0

- uint64x2_t vbicq_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vbic` q0`,` q0`,` q0

- int64x2_t vbicq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vbic` q0`,` q0`,` q0

##### 6.57.6.87 Logical operations (OR-NOT)

- uint32x2_t vorn_u32 (uint32x2_t, uint32x2_t)
  Form of expected instruction(s): `vorn` d0`,` d0`,` d0

- uint16x4_t vorn_u16 (uint16x4_t, uint16x4_t)
  Form of expected instruction(s): `vorn` d0`,` d0`,` d0

- uint8x8_t vorn_u8 (uint8x8_t, uint8x8_t)
  Form of expected instruction(s): `vorn` d0`,` d0`,` d0

- int32x2_t vorn_s32 (int32x2_t, int32x2_t)
  Form of expected instruction(s): `vorn` d0`,` d0`,` d0

- int16x4_t vorn_s16 (int16x4_t, int16x4_t)
  Form of expected instruction(s): `vorn` d0`,` d0`,` d0

- int8x8_t vorn_s8 (int8x8_t, int8x8_t)
  Form of expected instruction(s): `vorn` d0`,` d0`,` d0

- uint64x1_t vorn_u64 (uint64x1_t, uint64x1_t)

- int64x1_t vorn_s64 (int64x1_t, int64x1_t)

- uint32x4_t vornq_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `vorn` q0`,` q0`,` q0

- uint16x8_t vornq_u16 (uint16x8_t, uint16x8_t)
  Form of expected instruction(s): `vorn` q0`,` q0`,` q0

- uint8x16_t vornq_u8 (uint8x16_t, uint8x16_t)
  Form of expected instruction(s): `vorn` q0`,` q0`,` q0

- int32x4_t vornq_s32 (int32x4_t, int32x4_t)
  Form of expected instruction(s): `vorn` q0`,` q0`,` q0

- int16x8_t vornq_s16 (int16x8_t, int16x8_t)
  Form of expected instruction(s): `vorn` q0`,` q0`,` q0

- int8x16_t vornq_s8 (int8x16_t, int8x16_t)
  Form of expected instruction(s): `vorn` q0`,` q0`,` q0

- uint64x2_t vornq_u64 (uint64x2_t, uint64x2_t)
  Form of expected instruction(s): `vorn` q0`,` q0`,` q0

- int64x2_t vornq_s64 (int64x2_t, int64x2_t)
  Form of expected instruction(s): `vorn` q0`,` q0`,` q0

##### 6.57.6.88 Reinterpret casts

- poly8x8_t vreinterpret_p8_p16 (poly16x4_t)

- poly8x8_t vreinterpret_p8_f32 (float32x2_t)

- poly8x8_t vreinterpret_p8_p64 (poly64x1_t)

- poly8x8_t vreinterpret_p8_s64 (int64x1_t)

- poly8x8_t vreinterpret_p8_u64 (uint64x1_t)

- poly8x8_t vreinterpret_p8_s8 (int8x8_t)

- poly8x8_t vreinterpret_p8_s16 (int16x4_t)

- poly8x8_t vreinterpret_p8_s32 (int32x2_t)

- poly8x8_t vreinterpret_p8_u8 (uint8x8_t)

- poly8x8_t vreinterpret_p8_u16 (uint16x4_t)

- poly8x8_t vreinterpret_p8_u32 (uint32x2_t)

- poly16x4_t vreinterpret_p16_p8 (poly8x8_t)

- poly16x4_t vreinterpret_p16_f32 (float32x2_t)

- poly16x4_t vreinterpret_p16_p64 (poly64x1_t)

- poly16x4_t vreinterpret_p16_s64 (int64x1_t)

- poly16x4_t vreinterpret_p16_u64 (uint64x1_t)

- poly16x4_t vreinterpret_p16_s8 (int8x8_t)

- poly16x4_t vreinterpret_p16_s16 (int16x4_t)

- poly16x4_t vreinterpret_p16_s32 (int32x2_t)

- poly16x4_t vreinterpret_p16_u8 (uint8x8_t)

- poly16x4_t vreinterpret_p16_u16 (uint16x4_t)

- poly16x4_t vreinterpret_p16_u32 (uint32x2_t)

- float32x2_t vreinterpret_f32_p8 (poly8x8_t)

- float32x2_t vreinterpret_f32_p16 (poly16x4_t)

- float32x2_t vreinterpret_f32_p64 (poly64x1_t)

- float32x2_t vreinterpret_f32_s64 (int64x1_t)

- float32x2_t vreinterpret_f32_u64 (uint64x1_t)

- float32x2_t vreinterpret_f32_s8 (int8x8_t)

- float32x2_t vreinterpret_f32_s16 (int16x4_t)

- float32x2_t vreinterpret_f32_s32 (int32x2_t)

- float32x2_t vreinterpret_f32_u8 (uint8x8_t)

- float32x2_t vreinterpret_f32_u16 (uint16x4_t)

- float32x2_t vreinterpret_f32_u32 (uint32x2_t)

- poly64x1_t vreinterpret_p64_p8 (poly8x8_t)

- poly64x1_t vreinterpret_p64_p16 (poly16x4_t)

- poly64x1_t vreinterpret_p64_f32 (float32x2_t)

- poly64x1_t vreinterpret_p64_s64 (int64x1_t)

- poly64x1_t vreinterpret_p64_u64 (uint64x1_t)

- poly64x1_t vreinterpret_p64_s8 (int8x8_t)

- poly64x1_t vreinterpret_p64_s16 (int16x4_t)

- poly64x1_t vreinterpret_p64_s32 (int32x2_t)

- poly64x1_t vreinterpret_p64_u8 (uint8x8_t)

- poly64x1_t vreinterpret_p64_u16 (uint16x4_t)

- poly64x1_t vreinterpret_p64_u32 (uint32x2_t)

- int64x1_t vreinterpret_s64_p8 (poly8x8_t)

- int64x1_t vreinterpret_s64_p16 (poly16x4_t)

- int64x1_t vreinterpret_s64_f32 (float32x2_t)

- int64x1_t vreinterpret_s64_p64 (poly64x1_t)

- int64x1_t vreinterpret_s64_u64 (uint64x1_t)

- int64x1_t vreinterpret_s64_s8 (int8x8_t)

- int64x1_t vreinterpret_s64_s16 (int16x4_t)

- int64x1_t vreinterpret_s64_s32 (int32x2_t)

- int64x1_t vreinterpret_s64_u8 (uint8x8_t)

- int64x1_t vreinterpret_s64_u16 (uint16x4_t)

- int64x1_t vreinterpret_s64_u32 (uint32x2_t)

- uint64x1_t vreinterpret_u64_p8 (poly8x8_t)

- uint64x1_t vreinterpret_u64_p16 (poly16x4_t)

- uint64x1_t vreinterpret_u64_f32 (float32x2_t)

- uint64x1_t vreinterpret_u64_p64 (poly64x1_t)

- uint64x1_t vreinterpret_u64_s64 (int64x1_t)

- uint64x1_t vreinterpret_u64_s8 (int8x8_t)

- uint64x1_t vreinterpret_u64_s16 (int16x4_t)

- uint64x1_t vreinterpret_u64_s32 (int32x2_t)

- uint64x1_t vreinterpret_u64_u8 (uint8x8_t)

- uint64x1_t vreinterpret_u64_u16 (uint16x4_t)

- uint64x1_t vreinterpret_u64_u32 (uint32x2_t)

- int8x8_t vreinterpret_s8_p8 (poly8x8_t)

- int8x8_t vreinterpret_s8_p16 (poly16x4_t)

- int8x8_t vreinterpret_s8_f32 (float32x2_t)

- int8x8_t vreinterpret_s8_p64 (poly64x1_t)

- int8x8_t vreinterpret_s8_s64 (int64x1_t)

- int8x8_t vreinterpret_s8_u64 (uint64x1_t)

- int8x8_t vreinterpret_s8_s16 (int16x4_t)

- int8x8_t vreinterpret_s8_s32 (int32x2_t)

- int8x8_t vreinterpret_s8_u8 (uint8x8_t)

- int8x8_t vreinterpret_s8_u16 (uint16x4_t)

- int8x8_t vreinterpret_s8_u32 (uint32x2_t)

- int16x4_t vreinterpret_s16_p8 (poly8x8_t)

- int16x4_t vreinterpret_s16_p16 (poly16x4_t)

- int16x4_t vreinterpret_s16_f32 (float32x2_t)

- int16x4_t vreinterpret_s16_p64 (poly64x1_t)

- int16x4_t vreinterpret_s16_s64 (int64x1_t)

- int16x4_t vreinterpret_s16_u64 (uint64x1_t)

- int16x4_t vreinterpret_s16_s8 (int8x8_t)

- int16x4_t vreinterpret_s16_s32 (int32x2_t)

- int16x4_t vreinterpret_s16_u8 (uint8x8_t)

- int16x4_t vreinterpret_s16_u16 (uint16x4_t)

- int16x4_t vreinterpret_s16_u32 (uint32x2_t)

- int32x2_t vreinterpret_s32_p8 (poly8x8_t)

- int32x2_t vreinterpret_s32_p16 (poly16x4_t)

- int32x2_t vreinterpret_s32_f32 (float32x2_t)

- int32x2_t vreinterpret_s32_p64 (poly64x1_t)

- int32x2_t vreinterpret_s32_s64 (int64x1_t)

- int32x2_t vreinterpret_s32_u64 (uint64x1_t)

- int32x2_t vreinterpret_s32_s8 (int8x8_t)

- int32x2_t vreinterpret_s32_s16 (int16x4_t)

- int32x2_t vreinterpret_s32_u8 (uint8x8_t)

- int32x2_t vreinterpret_s32_u16 (uint16x4_t)

- int32x2_t vreinterpret_s32_u32 (uint32x2_t)

- uint8x8_t vreinterpret_u8_p8 (poly8x8_t)

- uint8x8_t vreinterpret_u8_p16 (poly16x4_t)

- uint8x8_t vreinterpret_u8_f32 (float32x2_t)

- uint8x8_t vreinterpret_u8_p64 (poly64x1_t)

- uint8x8_t vreinterpret_u8_s64 (int64x1_t)

- uint8x8_t vreinterpret_u8_u64 (uint64x1_t)

- uint8x8_t vreinterpret_u8_s8 (int8x8_t)

- uint8x8_t vreinterpret_u8_s16 (int16x4_t)

- uint8x8_t vreinterpret_u8_s32 (int32x2_t)

- uint8x8_t vreinterpret_u8_u16 (uint16x4_t)

- uint8x8_t vreinterpret_u8_u32 (uint32x2_t)

- uint16x4_t vreinterpret_u16_p8 (poly8x8_t)

- uint16x4_t vreinterpret_u16_p16 (poly16x4_t)

- uint16x4_t vreinterpret_u16_f32 (float32x2_t)

- uint16x4_t vreinterpret_u16_p64 (poly64x1_t)

- uint16x4_t vreinterpret_u16_s64 (int64x1_t)

- uint16x4_t vreinterpret_u16_u64 (uint64x1_t)

- uint16x4_t vreinterpret_u16_s8 (int8x8_t)

- uint16x4_t vreinterpret_u16_s16 (int16x4_t)

- uint16x4_t vreinterpret_u16_s32 (int32x2_t)

- uint16x4_t vreinterpret_u16_u8 (uint8x8_t)

- uint16x4_t vreinterpret_u16_u32 (uint32x2_t)

- uint32x2_t vreinterpret_u32_p8 (poly8x8_t)

- uint32x2_t vreinterpret_u32_p16 (poly16x4_t)

- uint32x2_t vreinterpret_u32_f32 (float32x2_t)

- uint32x2_t vreinterpret_u32_p64 (poly64x1_t)

- uint32x2_t vreinterpret_u32_s64 (int64x1_t)

- uint32x2_t vreinterpret_u32_u64 (uint64x1_t)

- uint32x2_t vreinterpret_u32_s8 (int8x8_t)

- uint32x2_t vreinterpret_u32_s16 (int16x4_t)

- uint32x2_t vreinterpret_u32_s32 (int32x2_t)

- uint32x2_t vreinterpret_u32_u8 (uint8x8_t)

- uint32x2_t vreinterpret_u32_u16 (uint16x4_t)

- poly8x16_t vreinterpretq_p8_p16 (poly16x8_t)

- poly8x16_t vreinterpretq_p8_f32 (float32x4_t)

- poly8x16_t vreinterpretq_p8_p64 (poly64x2_t)

- poly8x16_t vreinterpretq_p8_p128 (poly128_t)

- poly8x16_t vreinterpretq_p8_s64 (int64x2_t)

- poly8x16_t vreinterpretq_p8_u64 (uint64x2_t)

- poly8x16_t vreinterpretq_p8_s8 (int8x16_t)

- poly8x16_t vreinterpretq_p8_s16 (int16x8_t)

- poly8x16_t vreinterpretq_p8_s32 (int32x4_t)

- poly8x16_t vreinterpretq_p8_u8 (uint8x16_t)

- poly8x16_t vreinterpretq_p8_u16 (uint16x8_t)

- poly8x16_t vreinterpretq_p8_u32 (uint32x4_t)

- poly16x8_t vreinterpretq_p16_p8 (poly8x16_t)

- poly16x8_t vreinterpretq_p16_f32 (float32x4_t)

- poly16x8_t vreinterpretq_p16_p64 (poly64x2_t)

- poly16x8_t vreinterpretq_p16_p128 (poly128_t)

- poly16x8_t vreinterpretq_p16_s64 (int64x2_t)

- poly16x8_t vreinterpretq_p16_u64 (uint64x2_t)

- poly16x8_t vreinterpretq_p16_s8 (int8x16_t)

- poly16x8_t vreinterpretq_p16_s16 (int16x8_t)

- poly16x8_t vreinterpretq_p16_s32 (int32x4_t)

- poly16x8_t vreinterpretq_p16_u8 (uint8x16_t)

- poly16x8_t vreinterpretq_p16_u16 (uint16x8_t)

- poly16x8_t vreinterpretq_p16_u32 (uint32x4_t)

- float32x4_t vreinterpretq_f32_p8 (poly8x16_t)

- float32x4_t vreinterpretq_f32_p16 (poly16x8_t)

- float32x4_t vreinterpretq_f32_p64 (poly64x2_t)

- float32x4_t vreinterpretq_f32_p128 (poly128_t)

- float32x4_t vreinterpretq_f32_s64 (int64x2_t)

- float32x4_t vreinterpretq_f32_u64 (uint64x2_t)

- float32x4_t vreinterpretq_f32_s8 (int8x16_t)

- float32x4_t vreinterpretq_f32_s16 (int16x8_t)

- float32x4_t vreinterpretq_f32_s32 (int32x4_t)

- float32x4_t vreinterpretq_f32_u8 (uint8x16_t)

- float32x4_t vreinterpretq_f32_u16 (uint16x8_t)

- float32x4_t vreinterpretq_f32_u32 (uint32x4_t)

- poly64x2_t vreinterpretq_p64_p8 (poly8x16_t)

- poly64x2_t vreinterpretq_p64_p16 (poly16x8_t)

- poly64x2_t vreinterpretq_p64_f32 (float32x4_t)

- poly64x2_t vreinterpretq_p64_p128 (poly128_t)

- poly64x2_t vreinterpretq_p64_s64 (int64x2_t)

- poly64x2_t vreinterpretq_p64_u64 (uint64x2_t)

- poly64x2_t vreinterpretq_p64_s8 (int8x16_t)

- poly64x2_t vreinterpretq_p64_s16 (int16x8_t)

- poly64x2_t vreinterpretq_p64_s32 (int32x4_t)

- poly64x2_t vreinterpretq_p64_u8 (uint8x16_t)

- poly64x2_t vreinterpretq_p64_u16 (uint16x8_t)

- poly64x2_t vreinterpretq_p64_u32 (uint32x4_t)

- poly128_t vreinterpretq_p128_p8 (poly8x16_t)

- poly128_t vreinterpretq_p128_p16 (poly16x8_t)

- poly128_t vreinterpretq_p128_f32 (float32x4_t)

- poly128_t vreinterpretq_p128_p64 (poly64x2_t)

- poly128_t vreinterpretq_p128_s64 (int64x2_t)

- poly128_t vreinterpretq_p128_u64 (uint64x2_t)

- poly128_t vreinterpretq_p128_s8 (int8x16_t)

- poly128_t vreinterpretq_p128_s16 (int16x8_t)

- poly128_t vreinterpretq_p128_s32 (int32x4_t)

- poly128_t vreinterpretq_p128_u8 (uint8x16_t)

- poly128_t vreinterpretq_p128_u16 (uint16x8_t)

- poly128_t vreinterpretq_p128_u32 (uint32x4_t)

- int64x2_t vreinterpretq_s64_p8 (poly8x16_t)

- int64x2_t vreinterpretq_s64_p16 (poly16x8_t)

- int64x2_t vreinterpretq_s64_f32 (float32x4_t)

- int64x2_t vreinterpretq_s64_p64 (poly64x2_t)

- int64x2_t vreinterpretq_s64_p128 (poly128_t)

- int64x2_t vreinterpretq_s64_u64 (uint64x2_t)

- int64x2_t vreinterpretq_s64_s8 (int8x16_t)

- int64x2_t vreinterpretq_s64_s16 (int16x8_t)

- int64x2_t vreinterpretq_s64_s32 (int32x4_t)

- int64x2_t vreinterpretq_s64_u8 (uint8x16_t)

- int64x2_t vreinterpretq_s64_u16 (uint16x8_t)

- int64x2_t vreinterpretq_s64_u32 (uint32x4_t)

- uint64x2_t vreinterpretq_u64_p8 (poly8x16_t)

- uint64x2_t vreinterpretq_u64_p16 (poly16x8_t)

- uint64x2_t vreinterpretq_u64_f32 (float32x4_t)

- uint64x2_t vreinterpretq_u64_p64 (poly64x2_t)

- uint64x2_t vreinterpretq_u64_p128 (poly128_t)

- uint64x2_t vreinterpretq_u64_s64 (int64x2_t)

- uint64x2_t vreinterpretq_u64_s8 (int8x16_t)

- uint64x2_t vreinterpretq_u64_s16 (int16x8_t)

- uint64x2_t vreinterpretq_u64_s32 (int32x4_t)

- uint64x2_t vreinterpretq_u64_u8 (uint8x16_t)

- uint64x2_t vreinterpretq_u64_u16 (uint16x8_t)

- uint64x2_t vreinterpretq_u64_u32 (uint32x4_t)

- int8x16_t vreinterpretq_s8_p8 (poly8x16_t)

- int8x16_t vreinterpretq_s8_p16 (poly16x8_t)

- int8x16_t vreinterpretq_s8_f32 (float32x4_t)

- int8x16_t vreinterpretq_s8_p64 (poly64x2_t)

- int8x16_t vreinterpretq_s8_p128 (poly128_t)

- int8x16_t vreinterpretq_s8_s64 (int64x2_t)

- int8x16_t vreinterpretq_s8_u64 (uint64x2_t)

- int8x16_t vreinterpretq_s8_s16 (int16x8_t)

- int8x16_t vreinterpretq_s8_s32 (int32x4_t)

- int8x16_t vreinterpretq_s8_u8 (uint8x16_t)

- int8x16_t vreinterpretq_s8_u16 (uint16x8_t)

- int8x16_t vreinterpretq_s8_u32 (uint32x4_t)

- int16x8_t vreinterpretq_s16_p8 (poly8x16_t)

- int16x8_t vreinterpretq_s16_p16 (poly16x8_t)

- int16x8_t vreinterpretq_s16_f32 (float32x4_t)

- int16x8_t vreinterpretq_s16_p64 (poly64x2_t)

- int16x8_t vreinterpretq_s16_p128 (poly128_t)

- int16x8_t vreinterpretq_s16_s64 (int64x2_t)

- int16x8_t vreinterpretq_s16_u64 (uint64x2_t)

- int16x8_t vreinterpretq_s16_s8 (int8x16_t)

- int16x8_t vreinterpretq_s16_s32 (int32x4_t)

- int16x8_t vreinterpretq_s16_u8 (uint8x16_t)

- int16x8_t vreinterpretq_s16_u16 (uint16x8_t)

- int16x8_t vreinterpretq_s16_u32 (uint32x4_t)

- int32x4_t vreinterpretq_s32_p8 (poly8x16_t)

- int32x4_t vreinterpretq_s32_p16 (poly16x8_t)

- int32x4_t vreinterpretq_s32_f32 (float32x4_t)

- int32x4_t vreinterpretq_s32_p64 (poly64x2_t)

- int32x4_t vreinterpretq_s32_p128 (poly128_t)

- int32x4_t vreinterpretq_s32_s64 (int64x2_t)

- int32x4_t vreinterpretq_s32_u64 (uint64x2_t)

- int32x4_t vreinterpretq_s32_s8 (int8x16_t)

- int32x4_t vreinterpretq_s32_s16 (int16x8_t)

- int32x4_t vreinterpretq_s32_u8 (uint8x16_t)

- int32x4_t vreinterpretq_s32_u16 (uint16x8_t)

- int32x4_t vreinterpretq_s32_u32 (uint32x4_t)

- uint8x16_t vreinterpretq_u8_p8 (poly8x16_t)

- uint8x16_t vreinterpretq_u8_p16 (poly16x8_t)

- uint8x16_t vreinterpretq_u8_f32 (float32x4_t)

- uint8x16_t vreinterpretq_u8_p64 (poly64x2_t)

- uint8x16_t vreinterpretq_u8_p128 (poly128_t)

- uint8x16_t vreinterpretq_u8_s64 (int64x2_t)

- uint8x16_t vreinterpretq_u8_u64 (uint64x2_t)

- uint8x16_t vreinterpretq_u8_s8 (int8x16_t)

- uint8x16_t vreinterpretq_u8_s16 (int16x8_t)

- uint8x16_t vreinterpretq_u8_s32 (int32x4_t)

- uint8x16_t vreinterpretq_u8_u16 (uint16x8_t)

- uint8x16_t vreinterpretq_u8_u32 (uint32x4_t)

- uint16x8_t vreinterpretq_u16_p8 (poly8x16_t)

- uint16x8_t vreinterpretq_u16_p16 (poly16x8_t)

- uint16x8_t vreinterpretq_u16_f32 (float32x4_t)

- uint16x8_t vreinterpretq_u16_p64 (poly64x2_t)

- uint16x8_t vreinterpretq_u16_p128 (poly128_t)

- uint16x8_t vreinterpretq_u16_s64 (int64x2_t)

- uint16x8_t vreinterpretq_u16_u64 (uint64x2_t)

- uint16x8_t vreinterpretq_u16_s8 (int8x16_t)

- uint16x8_t vreinterpretq_u16_s16 (int16x8_t)

- uint16x8_t vreinterpretq_u16_s32 (int32x4_t)

- uint16x8_t vreinterpretq_u16_u8 (uint8x16_t)

- uint16x8_t vreinterpretq_u16_u32 (uint32x4_t)

- uint32x4_t vreinterpretq_u32_p8 (poly8x16_t)

- uint32x4_t vreinterpretq_u32_p16 (poly16x8_t)

- uint32x4_t vreinterpretq_u32_f32 (float32x4_t)

- uint32x4_t vreinterpretq_u32_p64 (poly64x2_t)

- uint32x4_t vreinterpretq_u32_p128 (poly128_t)

- uint32x4_t vreinterpretq_u32_s64 (int64x2_t)

- uint32x4_t vreinterpretq_u32_u64 (uint64x2_t)

- uint32x4_t vreinterpretq_u32_s8 (int8x16_t)

- uint32x4_t vreinterpretq_u32_s16 (int16x8_t)

- uint32x4_t vreinterpretq_u32_s32 (int32x4_t)

- uint32x4_t vreinterpretq_u32_u8 (uint8x16_t)

- uint32x4_t vreinterpretq_u32_u16 (uint16x8_t)

- poly128_t vldrq_p128(poly128_t const *)

- void vstrq_p128(poly128_t *, poly128_t)

- uint64x1_t vceq_p64 (poly64x1_t, poly64x1_t)

- uint64x1_t vtst_p64 (poly64x1_t, poly64x1_t)

- uint32_t vsha1h_u32 (uint32_t)
  Form of expected instruction(s): `sha1h.32` q0`,` q1

- uint32x4_t vsha1cq_u32 (uint32x4_t, uint32_t, uint32x4_t)
  Form of expected instruction(s): `sha1c.32` q0`,` q1`,` q2

- uint32x4_t vsha1pq_u32 (uint32x4_t, uint32_t, uint32x4_t)
  Form of expected instruction(s): `sha1p.32` q0`,` q1`,` q2

- uint32x4_t vsha1mq_u32 (uint32x4_t, uint32_t, uint32x4_t)
  Form of expected instruction(s): `sha1m.32` q0`,` q1`,` q2

- uint32x4_t vsha1su0q_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `sha1su0.32` q0`,` q1`,` q2

- uint32x4_t vsha1su1q_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `sha1su1.32` q0`,` q1`,` q2

- uint32x4_t vsha256hq_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `sha256h.32` q0`,` q1`,` q2

- uint32x4_t vsha256h2q_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `sha256h2.32` q0`,` q1`,` q2

- uint32x4_t vsha256su0q_u32 (uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `sha256su0.32` q0`,` q1

- uint32x4_t vsha256su1q_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
  Form of expected instruction(s): `sha256su1.32` q0`,` q1`,` q2

- poly128_t vmull_p64 (poly64_t a, poly64_t b)
  Form of expected instruction(s): `vmull.p64` q0`,` d1`,` d2

- poly128_t vmull_high_p64 (poly64x2_t a, poly64x2_t b)
  Form of expected instruction(s): `vmull.p64` q0`,` d1`,` d2