Next: FR-V Built-in Functions, Previous: AVR Built-in Functions, Up: Target Builtins

#### 6.57.9 Blackfin Built-in Functions

Currently, there are two Blackfin-specific built-in functions. These are used for generating `CSYNC` and `SSYNC` machine insns without using inline assembly; by using these built-in functions the compiler can automatically add workarounds for hardware errata involving these instructions. These functions are named as follows:

         void __builtin_bfin_csync (void)
         void __builtin_bfin_ssync (void)